From c45655386e532c85ff1d679fc2aa40b3aaff9916 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <f.fainelli@gmail.com>
Date: Sat, 14 Jun 2025 09:59:51 +0200
Subject: [PATCH] net: dsa: b53: add support for FDB operations on 5325/5365
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

BCM5325 and BCM5365 are part of a much older generation of switches which,
due to their limited number of ports and VLAN entries (up to 256) allowed
a single 64-bit register to hold a full ARL entry.
This requires a little bit of massaging when reading, writing and
converting ARL entries in both directions.

Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
Link: https://patch.msgid.link/20250614080000.1884236-6-noltari@gmail.com
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/dsa/b53/b53_common.c | 101 +++++++++++++++++++++++++------
 drivers/net/dsa/b53/b53_priv.h   |  29 +++++++++
 drivers/net/dsa/b53/b53_regs.h   |   7 ++-
 3 files changed, 115 insertions(+), 22 deletions(-)

--- a/drivers/net/dsa/b53/b53_common.c
+++ b/drivers/net/dsa/b53/b53_common.c
@@ -1764,6 +1764,45 @@ static int b53_arl_read(struct b53_devic
 	return *idx >= dev->num_arl_bins ? -ENOSPC : -ENOENT;
 }
 
+static int b53_arl_read_25(struct b53_device *dev, u64 mac,
+			   u16 vid, struct b53_arl_entry *ent, u8 *idx)
+{
+	DECLARE_BITMAP(free_bins, B53_ARLTBL_MAX_BIN_ENTRIES);
+	unsigned int i;
+	int ret;
+
+	ret = b53_arl_op_wait(dev);
+	if (ret)
+		return ret;
+
+	bitmap_zero(free_bins, dev->num_arl_bins);
+
+	/* Read the bins */
+	for (i = 0; i < dev->num_arl_bins; i++) {
+		u64 mac_vid;
+
+		b53_read64(dev, B53_ARLIO_PAGE,
+			   B53_ARLTBL_MAC_VID_ENTRY(i), &mac_vid);
+
+		b53_arl_to_entry_25(ent, mac_vid);
+
+		if (!(mac_vid & ARLTBL_VALID_25)) {
+			set_bit(i, free_bins);
+			continue;
+		}
+		if ((mac_vid & ARLTBL_MAC_MASK) != mac)
+			continue;
+		if (dev->vlan_enabled &&
+		    ((mac_vid >> ARLTBL_VID_S_65) & ARLTBL_VID_MASK_25) != vid)
+			continue;
+		*idx = i;
+		return 0;
+	}
+
+	*idx = find_first_bit(free_bins, dev->num_arl_bins);
+	return *idx >= dev->num_arl_bins ? -ENOSPC : -ENOENT;
+}
+
 static int b53_arl_op(struct b53_device *dev, int op, int port,
 		      const unsigned char *addr, u16 vid, bool is_valid)
 {
@@ -1786,7 +1825,10 @@ static int b53_arl_op(struct b53_device
 	if (ret)
 		return ret;
 
-	ret = b53_arl_read(dev, mac, vid, &ent, &idx);
+	if (is5325(dev) || is5365(dev))
+		ret = b53_arl_read_25(dev, mac, vid, &ent, &idx);
+	else
+		ret = b53_arl_read(dev, mac, vid, &ent, &idx);
 
 	/* If this is a read, just finish now */
 	if (op)
@@ -1830,12 +1872,17 @@ static int b53_arl_op(struct b53_device
 	ent.is_static = true;
 	ent.is_age = false;
 	memcpy(ent.mac, addr, ETH_ALEN);
-	b53_arl_from_entry(&mac_vid, &fwd_entry, &ent);
+	if (is5325(dev) || is5365(dev))
+		b53_arl_from_entry_25(&mac_vid, &ent);
+	else
+		b53_arl_from_entry(&mac_vid, &fwd_entry, &ent);
 
 	b53_write64(dev, B53_ARLIO_PAGE,
 		    B53_ARLTBL_MAC_VID_ENTRY(idx), mac_vid);
-	b53_write32(dev, B53_ARLIO_PAGE,
-		    B53_ARLTBL_DATA_ENTRY(idx), fwd_entry);
+
+	if (!is5325(dev) && !is5365(dev))
+		b53_write32(dev, B53_ARLIO_PAGE,
+			    B53_ARLTBL_DATA_ENTRY(idx), fwd_entry);
 
 	return b53_arl_rw_op(dev, 0);
 }
@@ -1847,12 +1894,6 @@ int b53_fdb_add(struct dsa_switch *ds, i
 	struct b53_device *priv = ds->priv;
 	int ret;
 
-	/* 5325 and 5365 require some more massaging, but could
-	 * be supported eventually
-	 */
-	if (is5325(priv) || is5365(priv))
-		return -EOPNOTSUPP;
-
 	mutex_lock(&priv->arl_mutex);
 	ret = b53_arl_op(priv, 0, port, addr, vid, true);
 	mutex_unlock(&priv->arl_mutex);
@@ -1879,10 +1920,15 @@ EXPORT_SYMBOL(b53_fdb_del);
 static int b53_arl_search_wait(struct b53_device *dev)
 {
 	unsigned int timeout = 1000;
-	u8 reg;
+	u8 reg, offset;
+
+	if (is5325(dev) || is5365(dev))
+		offset = B53_ARL_SRCH_CTL_25;
+	else
+		offset = B53_ARL_SRCH_CTL;
 
 	do {
-		b53_read8(dev, B53_ARLIO_PAGE, B53_ARL_SRCH_CTL, &reg);
+		b53_read8(dev, B53_ARLIO_PAGE, offset, &reg);
 		if (!(reg & ARL_SRCH_STDN))
 			return 0;
 
@@ -1899,13 +1945,24 @@ static void b53_arl_search_rd(struct b53
 			      struct b53_arl_entry *ent)
 {
 	u64 mac_vid;
-	u32 fwd_entry;
 
-	b53_read64(dev, B53_ARLIO_PAGE,
-		   B53_ARL_SRCH_RSTL_MACVID(idx), &mac_vid);
-	b53_read32(dev, B53_ARLIO_PAGE,
-		   B53_ARL_SRCH_RSTL(idx), &fwd_entry);
-	b53_arl_to_entry(ent, mac_vid, fwd_entry);
+	if (is5325(dev)) {
+		b53_read64(dev, B53_ARLIO_PAGE, B53_ARL_SRCH_RSTL_0_MACVID_25,
+			   &mac_vid);
+		b53_arl_to_entry_25(ent, mac_vid);
+	} else if (is5365(dev)) {
+		b53_read64(dev, B53_ARLIO_PAGE, B53_ARL_SRCH_RSTL_0_MACVID_65,
+			   &mac_vid);
+		b53_arl_to_entry_25(ent, mac_vid);
+	} else {
+		u32 fwd_entry;
+
+		b53_read64(dev, B53_ARLIO_PAGE, B53_ARL_SRCH_RSTL_MACVID(idx),
+			   &mac_vid);
+		b53_read32(dev, B53_ARLIO_PAGE, B53_ARL_SRCH_RSTL(idx),
+			   &fwd_entry);
+		b53_arl_to_entry(ent, mac_vid, fwd_entry);
+	}
 }
 
 static int b53_fdb_copy(int port, const struct b53_arl_entry *ent,
@@ -1926,14 +1983,20 @@ int b53_fdb_dump(struct dsa_switch *ds,
 	struct b53_device *priv = ds->priv;
 	struct b53_arl_entry results[2];
 	unsigned int count = 0;
+	u8 offset;
 	int ret;
 	u8 reg;
 
 	mutex_lock(&priv->arl_mutex);
 
+	if (is5325(priv) || is5365(priv))
+		offset = B53_ARL_SRCH_CTL_25;
+	else
+		offset = B53_ARL_SRCH_CTL;
+
 	/* Start search operation */
 	reg = ARL_SRCH_STDN;
-	b53_write8(priv, B53_ARLIO_PAGE, B53_ARL_SRCH_CTL, reg);
+	b53_write8(priv, offset, B53_ARL_SRCH_CTL, reg);
 
 	do {
 		ret = b53_arl_search_wait(priv);
--- a/drivers/net/dsa/b53/b53_priv.h
+++ b/drivers/net/dsa/b53/b53_priv.h
@@ -317,6 +317,19 @@ static inline void b53_arl_to_entry(stru
 	ent->vid = mac_vid >> ARLTBL_VID_S;
 }
 
+static inline void b53_arl_to_entry_25(struct b53_arl_entry *ent,
+				       u64 mac_vid)
+{
+	memset(ent, 0, sizeof(*ent));
+	ent->port = (mac_vid >> ARLTBL_DATA_PORT_ID_S_25) &
+		     ARLTBL_DATA_PORT_ID_MASK_25;
+	ent->is_valid = !!(mac_vid & ARLTBL_VALID_25);
+	ent->is_age = !!(mac_vid & ARLTBL_AGE_25);
+	ent->is_static = !!(mac_vid & ARLTBL_STATIC_25);
+	u64_to_ether_addr(mac_vid, ent->mac);
+	ent->vid = mac_vid >> ARLTBL_VID_S_65;
+}
+
 static inline void b53_arl_from_entry(u64 *mac_vid, u32 *fwd_entry,
 				      const struct b53_arl_entry *ent)
 {
@@ -331,6 +344,22 @@ static inline void b53_arl_from_entry(u6
 		*fwd_entry |= ARLTBL_AGE;
 }
 
+static inline void b53_arl_from_entry_25(u64 *mac_vid,
+					 const struct b53_arl_entry *ent)
+{
+	*mac_vid = ether_addr_to_u64(ent->mac);
+	*mac_vid |= (u64)(ent->port & ARLTBL_DATA_PORT_ID_MASK_25) <<
+			  ARLTBL_DATA_PORT_ID_S_25;
+	*mac_vid |= (u64)(ent->vid & ARLTBL_VID_MASK_25) <<
+			  ARLTBL_VID_S_65;
+	if (ent->is_valid)
+		*mac_vid |= ARLTBL_VALID_25;
+	if (ent->is_static)
+		*mac_vid |= ARLTBL_STATIC_25;
+	if (ent->is_age)
+		*mac_vid |= ARLTBL_AGE_25;
+}
+
 #ifdef CONFIG_BCM47XX
 
 #include <linux/bcm47xx_nvram.h>
--- a/drivers/net/dsa/b53/b53_regs.h
+++ b/drivers/net/dsa/b53/b53_regs.h
@@ -324,9 +324,10 @@
 #define   ARLTBL_VID_MASK		0xfff
 #define   ARLTBL_DATA_PORT_ID_S_25	48
 #define   ARLTBL_DATA_PORT_ID_MASK_25	0xf
-#define   ARLTBL_AGE_25			BIT(61)
-#define   ARLTBL_STATIC_25		BIT(62)
-#define   ARLTBL_VALID_25		BIT(63)
+#define   ARLTBL_VID_S_65		53
+#define   ARLTBL_AGE_25			BIT_ULL(61)
+#define   ARLTBL_STATIC_25		BIT_ULL(62)
+#define   ARLTBL_VALID_25		BIT_ULL(63)
 
 /* ARL Table Data Entry N Registers (32 bit) */
 #define B53_ARLTBL_DATA_ENTRY(n)	((0x10 * (n)) + 0x18)
