// SPDX-License-Identifier: MIT, GPL-2.0 or later
/* Copyright (c) 2025, Yang Xiwen <forbidden405@outlook.com> */

/dts-v1/;

#include "ipq6018.dtsi"
#include "ipq6018-cp-cpu.dtsi"
#include "ipq6018-ess.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "TP-Link EAP623-Outdoor HD V1.0";
	compatible = "tplink,eap623od-hd-v1", "qcom,ipq6018";

	aliases {
		serial0 = &blsp1_uart3;
		led-boot = &led_sys_green;
		led-failsafe = &led_sys_yellow;
		led-running = &led_sys_green;
		led-upgrade = &led_sys_yellow;
	};

	chosen {
		stdout-path = "serial0:115200n8";
		bootargs-append = " root=/dev/ubiblock0_1";
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&tlmm 9 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_sys_green: led-0 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_STATUS;
			gpios = <&tlmm 37 GPIO_ACTIVE_HIGH>;
		};

		led_sys_yellow: led-1 {
			color = <LED_COLOR_ID_YELLOW>;
			function = LED_FUNCTION_STATUS;
			gpios = <&tlmm 32 GPIO_ACTIVE_HIGH>;
		};
	};
};

&blsp1_uart3 {
	pinctrl-0 = <&serial_3_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&tlmm {
	mdio_pins: mdio-pins {
		mdc {
			pins = "gpio64";
			function = "mdc";
			drive-strength = <8>;
			bias-pull-up;
		};

		mdio {
			pins = "gpio65";
			function = "mdio";
			drive-strength = <8>;
			bias-pull-up;
		};
	};

	phy_pins: phy-reset-pin {
		pins = "gpio77";
		function = "gpio";
		bias-pull-up;
	};
};

&mdio {
	status = "okay";
	reset-gpios = <&tlmm 77 GPIO_ACTIVE_LOW>;
	reset-delay-us = <10000>;
	reset-post-delay-us = <50000>;
	pinctrl-0 = <&mdio_pins>, <&phy_pins>;
	pinctrl-names = "default";

	rtl8211f: ethernet-phy@4 {
		reg = <4>;

		realtek,clkout-disable;
		realtek,aldps-enable;
	};
};

&switch {
	status = "okay";
	switch_lan_bmp = <ESS_PORT5>; /* lan port bitmap */
	switch_mac_mode1 = <MAC_MODE_SGMII_PLUS>; /* mac mode for uniphy instance0*/

	qcom,port_phyinfo {
		port@5 {
			port_id = <5>;
			phy_address = <4>;
			port_mac_sel = "QGMAC_PORT";
		};
	};
};

&edma {
	status = "okay";
};

&dp5 {
	status = "okay";
	phy-handle = <&rtl8211f>;
	phy-mode = "sgmii";
	label = "lan";
};

&qpic_bam {
	status = "okay";
};

&qpic_nand {
	status = "okay";

	nand@0 {
		reg = <0>;
		nand-ecc-strength = <4>;
		nand-ecc-step-size = <512>;
		nand-bus-width = <8>;

		partitions {
			compatible = "qcom,smem-part";
		};
	};
};

&wifi {
	qcom,ath11k-calibration-variant = "TPLink-EAP623-Outdoor-HD-v1";
	status = "okay";
};
