From 6f8c1ed25809181c187a59b1caaa1521756924bf Mon Sep 17 00:00:00 2001
From: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Date: Tue, 22 Oct 2024 17:47:26 +0200
Subject: [PATCH] arm64: dts: qcom: ipq: change labels to lower-case

DTS coding style expects labels to be lowercase.  No functional impact.
Verified with comparing decompiled DTB (dtx_diff and fdtdump+diff).

Signed-off-by: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Link: https://lore.kernel.org/r/20241022-dts-qcom-label-v3-1-0505bc7d2c56@linaro.org
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
---
 arch/arm64/boot/dts/qcom/ipq5018.dtsi | 10 +++---
 arch/arm64/boot/dts/qcom/ipq5332.dtsi | 18 +++++-----
 arch/arm64/boot/dts/qcom/ipq6018.dtsi | 26 +++++++-------
 arch/arm64/boot/dts/qcom/ipq8074.dtsi | 18 +++++-----
 arch/arm64/boot/dts/qcom/ipq9574.dtsi | 50 +++++++++++++--------------
 5 files changed, 61 insertions(+), 61 deletions(-)

--- a/arch/arm64/boot/dts/qcom/ipq5018.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq5018.dtsi
@@ -31,27 +31,27 @@
 		#address-cells = <1>;
 		#size-cells = <0>;
 
-		CPU0: cpu@0 {
+		cpu0: cpu@0 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a53";
 			reg = <0x0>;
 			enable-method = "psci";
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			clocks = <&apcs_glb APCS_ALIAS0_CORE_CLK>;
 			operating-points-v2 = <&cpu_opp_table>;
 		};
 
-		CPU1: cpu@1 {
+		cpu1: cpu@1 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a53";
 			reg = <0x1>;
 			enable-method = "psci";
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			clocks = <&apcs_glb APCS_ALIAS0_CORE_CLK>;
 			operating-points-v2 = <&cpu_opp_table>;
 		};
 
-		L2_0: l2-cache {
+		l2_0: l2-cache {
 			compatible = "cache";
 			cache-level = <2>;
 			cache-size = <0x80000>;
--- a/arch/arm64/boot/dts/qcom/ipq5332.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq5332.dtsi
@@ -31,47 +31,47 @@
 		#address-cells = <1>;
 		#size-cells = <0>;
 
-		CPU0: cpu@0 {
+		cpu0: cpu@0 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a53";
 			reg = <0x0>;
 			enable-method = "psci";
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			clocks = <&apcs_glb APCS_ALIAS0_CORE_CLK>;
 			operating-points-v2 = <&cpu_opp_table>;
 		};
 
-		CPU1: cpu@1 {
+		cpu1: cpu@1 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a53";
 			reg = <0x1>;
 			enable-method = "psci";
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			clocks = <&apcs_glb APCS_ALIAS0_CORE_CLK>;
 			operating-points-v2 = <&cpu_opp_table>;
 		};
 
-		CPU2: cpu@2 {
+		cpu2: cpu@2 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a53";
 			reg = <0x2>;
 			enable-method = "psci";
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			clocks = <&apcs_glb APCS_ALIAS0_CORE_CLK>;
 			operating-points-v2 = <&cpu_opp_table>;
 		};
 
-		CPU3: cpu@3 {
+		cpu3: cpu@3 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a53";
 			reg = <0x3>;
 			enable-method = "psci";
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			clocks = <&apcs_glb APCS_ALIAS0_CORE_CLK>;
 			operating-points-v2 = <&cpu_opp_table>;
 		};
 
-		L2_0: l2-cache {
+		l2_0: l2-cache {
 			compatible = "cache";
 			cache-level = <2>;
 			cache-unified;
--- a/arch/arm64/boot/dts/qcom/ipq6018.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq6018.dtsi
@@ -34,12 +34,12 @@
 		#address-cells = <1>;
 		#size-cells = <0>;
 
-		CPU0: cpu@0 {
+		cpu0: cpu@0 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a53";
 			reg = <0x0>;
 			enable-method = "psci";
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			clocks = <&apcs_glb APCS_ALIAS0_CORE_CLK>;
 			clock-names = "cpu";
 			operating-points-v2 = <&cpu_opp_table>;
@@ -47,12 +47,12 @@
 			#cooling-cells = <2>;
 		};
 
-		CPU1: cpu@1 {
+		cpu1: cpu@1 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a53";
 			enable-method = "psci";
 			reg = <0x1>;
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			clocks = <&apcs_glb APCS_ALIAS0_CORE_CLK>;
 			clock-names = "cpu";
 			operating-points-v2 = <&cpu_opp_table>;
@@ -60,12 +60,12 @@
 			#cooling-cells = <2>;
 		};
 
-		CPU2: cpu@2 {
+		cpu2: cpu@2 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a53";
 			enable-method = "psci";
 			reg = <0x2>;
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			clocks = <&apcs_glb APCS_ALIAS0_CORE_CLK>;
 			clock-names = "cpu";
 			operating-points-v2 = <&cpu_opp_table>;
@@ -73,12 +73,12 @@
 			#cooling-cells = <2>;
 		};
 
-		CPU3: cpu@3 {
+		cpu3: cpu@3 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a53";
 			enable-method = "psci";
 			reg = <0x3>;
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			clocks = <&apcs_glb APCS_ALIAS0_CORE_CLK>;
 			clock-names = "cpu";
 			operating-points-v2 = <&cpu_opp_table>;
@@ -86,7 +86,7 @@
 			#cooling-cells = <2>;
 		};
 
-		L2_0: l2-cache {
+		l2_0: l2-cache {
 			compatible = "cache";
 			cache-level = <2>;
 			cache-unified;
@@ -1015,10 +1015,10 @@
 			cooling-maps {
 				map0 {
 					trip = <&cpu_alert>;
-					cooling-device = <&CPU0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
+					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
 				};
 			};
 		};
--- a/arch/arm64/boot/dts/qcom/ipq8074.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq8074.dtsi
@@ -32,39 +32,39 @@
 		#address-cells = <1>;
 		#size-cells = <0>;
 
-		CPU0: cpu@0 {
+		cpu0: cpu@0 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a53";
 			reg = <0x0>;
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			enable-method = "psci";
 		};
 
-		CPU1: cpu@1 {
+		cpu1: cpu@1 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a53";
 			enable-method = "psci";
 			reg = <0x1>;
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 		};
 
-		CPU2: cpu@2 {
+		cpu2: cpu@2 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a53";
 			enable-method = "psci";
 			reg = <0x2>;
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 		};
 
-		CPU3: cpu@3 {
+		cpu3: cpu@3 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a53";
 			enable-method = "psci";
 			reg = <0x3>;
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 		};
 
-		L2_0: l2-cache {
+		l2_0: l2-cache {
 			compatible = "cache";
 			cache-level = <2>;
 			cache-unified;
--- a/arch/arm64/boot/dts/qcom/ipq9574.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq9574.dtsi
@@ -34,12 +34,12 @@
 		#address-cells = <1>;
 		#size-cells = <0>;
 
-		CPU0: cpu@0 {
+		cpu0: cpu@0 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a73";
 			reg = <0x0>;
 			enable-method = "psci";
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			clocks = <&apcs_glb APCS_ALIAS0_CORE_CLK>;
 			clock-names = "cpu";
 			operating-points-v2 = <&cpu_opp_table>;
@@ -47,12 +47,12 @@
 			#cooling-cells = <2>;
 		};
 
-		CPU1: cpu@1 {
+		cpu1: cpu@1 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a73";
 			reg = <0x1>;
 			enable-method = "psci";
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			clocks = <&apcs_glb APCS_ALIAS0_CORE_CLK>;
 			clock-names = "cpu";
 			operating-points-v2 = <&cpu_opp_table>;
@@ -60,12 +60,12 @@
 			#cooling-cells = <2>;
 		};
 
-		CPU2: cpu@2 {
+		cpu2: cpu@2 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a73";
 			reg = <0x2>;
 			enable-method = "psci";
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			clocks = <&apcs_glb APCS_ALIAS0_CORE_CLK>;
 			clock-names = "cpu";
 			operating-points-v2 = <&cpu_opp_table>;
@@ -73,12 +73,12 @@
 			#cooling-cells = <2>;
 		};
 
-		CPU3: cpu@3 {
+		cpu3: cpu@3 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a73";
 			reg = <0x3>;
 			enable-method = "psci";
-			next-level-cache = <&L2_0>;
+			next-level-cache = <&l2_0>;
 			clocks = <&apcs_glb APCS_ALIAS0_CORE_CLK>;
 			clock-names = "cpu";
 			operating-points-v2 = <&cpu_opp_table>;
@@ -86,7 +86,7 @@
 			#cooling-cells = <2>;
 		};
 
-		L2_0: l2-cache {
+		l2_0: l2-cache {
 			compatible = "cache";
 			cache-level = <2>;
 			cache-unified;
@@ -865,10 +865,10 @@
 			cooling-maps {
 				map0 {
 					trip = <&cpu0_alert>;
-					cooling-device = <&CPU0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
+					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
 				};
 			};
 		};
@@ -893,10 +893,10 @@
 			cooling-maps {
 				map0 {
 					trip = <&cpu1_alert>;
-					cooling-device = <&CPU0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
+					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
 				};
 			};
 		};
@@ -921,10 +921,10 @@
 			cooling-maps {
 				map0 {
 					trip = <&cpu2_alert>;
-					cooling-device = <&CPU0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
+					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
 				};
 			};
 		};
@@ -949,10 +949,10 @@
 			cooling-maps {
 				map0 {
 					trip = <&cpu3_alert>;
-					cooling-device = <&CPU0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-							 <&CPU3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
+					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
 				};
 			};
 		};
