From c2019f64539dd24e6e0da3cea2219d6f9e6b03e4 Mon Sep 17 00:00:00 2001
From: Ziyang Huang <hzyitc@outlook.com>
Date: Sun, 8 Sep 2024 16:40:11 +0800
Subject: [PATCH] arm64: dts: qcom: ipq5018: Add SPI nand node

Add SPI NAND support for IPQ5018 SoC.

Signed-off-by: Ziyang Huang <hzyitc@outlook.com>
Signed-off-by: George Moussalem <george.moussalem@outlook.com>
---
 arch/arm64/boot/dts/qcom/ipq5018.dtsi | 40 +++++++++++++++++++++++++++
 1 file changed, 40 insertions(+)

--- a/arch/arm64/boot/dts/qcom/ipq5018.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq5018.dtsi
@@ -456,6 +456,36 @@
 			status = "disabled";
 		};
 
+		qpic_bam: dma@7984000 {
+			compatible = "qcom,bam-v1.7.0";
+			reg = <0x07984000 0x1c000>;
+			interrupts = <GIC_SPI 146 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&gcc GCC_QPIC_AHB_CLK>;
+			clock-names = "bam_clk";
+			#dma-cells = <1>;
+			qcom,ee = <0>;
+			status = "disabled";
+		};
+
+		qpic_nand: qpic-nand@79b0000 {
+			compatible = "qcom,ipq5018-snand", "qcom,ipq9574-snand";
+			reg = <0x079b0000 0x10000>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			clocks = <&gcc GCC_QPIC_CLK>,
+				 <&gcc GCC_QPIC_AHB_CLK>,
+				 <&gcc GCC_QPIC_IO_MACRO_CLK>;
+			clock-names = "core", "aon", "iom";
+
+			dmas = <&qpic_bam 0>,
+			       <&qpic_bam 1>,
+			       <&qpic_bam 2>,
+			       <&qpic_bam 3>;
+			dma-names = "tx", "rx", "cmd", "status";
+
+			status = "disabled";
+		};
+
 		usb: usb@8af8800 {
 			compatible = "qcom,ipq5018-dwc3", "qcom,dwc3";
 			reg = <0x08af8800 0x400>;
