From 2469a06f61b88939d92fd8e61a32afd5566c0be0 Mon Sep 17 00:00:00 2001
From: David Plowman <david.plowman@raspberrypi.com>
Date: Thu, 21 Oct 2021 14:47:00 +0100
Subject: [PATCH] media: i2c: ov5647: Sensor should report RAW color space

Tested on Raspberry Pi running libcamera.

Signed-off-by: David Plowman <david.plowman@raspberrypi.com>
---
 drivers/media/i2c/ov5647.c | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

--- a/drivers/media/i2c/ov5647.c
+++ b/drivers/media/i2c/ov5647.c
@@ -508,7 +508,7 @@ static const struct ov5647_mode ov5647_m
 	{
 		.format = {
 			.code		= MEDIA_BUS_FMT_SBGGR10_1X10,
-			.colorspace	= V4L2_COLORSPACE_SRGB,
+			.colorspace	= V4L2_COLORSPACE_RAW,
 			.field		= V4L2_FIELD_NONE,
 			.width		= 2592,
 			.height		= 1944
@@ -529,7 +529,7 @@ static const struct ov5647_mode ov5647_m
 	{
 		.format = {
 			.code		= MEDIA_BUS_FMT_SBGGR10_1X10,
-			.colorspace	= V4L2_COLORSPACE_SRGB,
+			.colorspace	= V4L2_COLORSPACE_RAW,
 			.field		= V4L2_FIELD_NONE,
 			.width		= 1920,
 			.height		= 1080
@@ -550,7 +550,7 @@ static const struct ov5647_mode ov5647_m
 	{
 		.format = {
 			.code		= MEDIA_BUS_FMT_SBGGR10_1X10,
-			.colorspace	= V4L2_COLORSPACE_SRGB,
+			.colorspace	= V4L2_COLORSPACE_RAW,
 			.field		= V4L2_FIELD_NONE,
 			.width		= 1296,
 			.height		= 972
@@ -571,7 +571,7 @@ static const struct ov5647_mode ov5647_m
 	{
 		.format = {
 			.code		= MEDIA_BUS_FMT_SBGGR10_1X10,
-			.colorspace	= V4L2_COLORSPACE_SRGB,
+			.colorspace	= V4L2_COLORSPACE_RAW,
 			.field		= V4L2_FIELD_NONE,
 			.width		= 640,
 			.height		= 480
