From 62f726848da42554e6d270dfda17ed19bfa3456f Mon Sep 17 00:00:00 2001
From: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Date: Tue, 4 Feb 2025 20:38:17 +0200
Subject: [PATCH] wifi: rtw88: Extend struct rtw_pwr_track_tbl for RTL8814AU

Currently this struct has the members required for chips with 2 RF
paths. Add more members to support chips with 4 RF paths, like the
RTL8814AU.

Signed-off-by: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Acked-by: Ping-Ke Shih <pkshih@realtek.com>
Signed-off-by: Ping-Ke Shih <pkshih@realtek.com>
Link: https://patch.msgid.link/be5a73f4-a0fe-43d6-9457-930cde199284@gmail.com
---
 drivers/net/wireless/realtek/rtw88/main.h | 12 ++++++++++++
 1 file changed, 12 insertions(+)

--- a/drivers/net/wireless/realtek/rtw88/main.h
+++ b/drivers/net/wireless/realtek/rtw88/main.h
@@ -1131,14 +1131,26 @@ struct rtw_rfe_def {
  * For 2G there are cck rate and ofdm rate with different settings.
  */
 struct rtw_pwr_track_tbl {
+	const u8 *pwrtrk_5gd_n[RTW_PWR_TRK_5G_NUM];
+	const u8 *pwrtrk_5gd_p[RTW_PWR_TRK_5G_NUM];
+	const u8 *pwrtrk_5gc_n[RTW_PWR_TRK_5G_NUM];
+	const u8 *pwrtrk_5gc_p[RTW_PWR_TRK_5G_NUM];
 	const u8 *pwrtrk_5gb_n[RTW_PWR_TRK_5G_NUM];
 	const u8 *pwrtrk_5gb_p[RTW_PWR_TRK_5G_NUM];
 	const u8 *pwrtrk_5ga_n[RTW_PWR_TRK_5G_NUM];
 	const u8 *pwrtrk_5ga_p[RTW_PWR_TRK_5G_NUM];
+	const u8 *pwrtrk_2gd_n;
+	const u8 *pwrtrk_2gd_p;
+	const u8 *pwrtrk_2gc_n;
+	const u8 *pwrtrk_2gc_p;
 	const u8 *pwrtrk_2gb_n;
 	const u8 *pwrtrk_2gb_p;
 	const u8 *pwrtrk_2ga_n;
 	const u8 *pwrtrk_2ga_p;
+	const u8 *pwrtrk_2g_cckd_n;
+	const u8 *pwrtrk_2g_cckd_p;
+	const u8 *pwrtrk_2g_cckc_n;
+	const u8 *pwrtrk_2g_cckc_p;
 	const u8 *pwrtrk_2g_cckb_n;
 	const u8 *pwrtrk_2g_cckb_p;
 	const u8 *pwrtrk_2g_ccka_n;
