From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Subject: [PATCH] brcmfmac: add in-driver tables with country codes
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This adds early support for changing region. Ideally this data should
be stored in DT as all these mappings are devices specific.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
---

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/of.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/of.c
@@ -66,6 +66,36 @@ static int brcmf_of_get_country_codes(st
 	return 0;
 }
 
+/* TODO: FIXME: Use DT */
+static void brcmf_of_probe_cc(struct device *dev,
+			      struct brcmf_mp_device *settings)
+{
+	static struct brcmfmac_pd_cc_entry netgear_r8000_cc_ent[] = {
+		{ "JP", "JP", 78 },
+		{ "US", "Q2", 86 },
+	};
+	struct brcmfmac_pd_cc_entry *cc_ent = NULL;
+	int table_size = 0;
+
+	if (of_machine_is_compatible("netgear,r8000")) {
+		cc_ent = netgear_r8000_cc_ent;
+		table_size = ARRAY_SIZE(netgear_r8000_cc_ent);
+	}
+
+	if (cc_ent && table_size) {
+		struct brcmfmac_pd_cc *cc;
+		size_t memsize;
+
+		memsize = table_size * sizeof(struct brcmfmac_pd_cc_entry);
+		cc = devm_kzalloc(dev, sizeof(*cc) + memsize, GFP_KERNEL);
+		if (!cc)
+			return;
+		cc->table_size = table_size;
+		memcpy(cc->table, cc_ent, memsize);
+		settings->country_codes = cc;
+	}
+}
+
 int brcmf_of_probe(struct device *dev, enum brcmf_bus_type bus_type,
 		   struct brcmf_mp_device *settings)
 {
@@ -121,6 +151,8 @@ int brcmf_of_probe(struct device *dev, e
 
 	brcmf_dbg(INFO, "%s LPO clock\n", clk ? "enable" : "no");
 
+	brcmf_of_probe_cc(dev, settings);
+
 	if (!np || !of_device_is_compatible(np, "brcm,bcm4329-fmac"))
 		return 0;
 
