--- a/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi
@@ -632,7 +632,7 @@
 	disable-wp;
 	no-mmc;
 	no-sdio;
-	sd-uhs-sdr104;
+	sd-uhs-sdr50;
 	vmmc-supply = <&vcc3v3_sd_s0>;
 	vqmmc-supply = <&vccio_sd_s0>;
 	status = "okay";
