From 0ca1a9040cff3ace3d7fce5cdd83f1cbaa8da50c Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Fri, 2 Sep 2016 17:21:42 +0100
Subject: [PATCH] bcm2835-sdhost: Don't exit cmd wait loop on error

The FAIL flag can be set in the CMD register before command processing
is complete, leading to spurious "failed to complete" errors. This has
the effect of promoting harmless CRC7 errors during CMD1 processing
into errors that can delay and even prevent booting.

Also:
1) Convert the last KERN_ERROR message in the register dumping to
   KERN_INFO.
2) Remove an unnecessary reset call from  bcm2835_sdhost_add_host.

See: https://github.com/raspberrypi/linux/pull/1492

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 drivers/mmc/host/bcm2835-sdhost.c | 10 +++-------
 1 file changed, 3 insertions(+), 7 deletions(-)

--- a/drivers/mmc/host/bcm2835-sdhost.c
+++ b/drivers/mmc/host/bcm2835-sdhost.c
@@ -373,7 +373,7 @@ static void bcm2835_sdhost_dumpregs(stru
 	pr_info("%s: SDRSP2 0x%08x\n",
 		mmc_hostname(host->mmc),
 		bcm2835_sdhost_read(host, SDRSP2));
-	pr_err("%s: SDRSP3 0x%08x\n",
+	pr_info("%s: SDRSP3 0x%08x\n",
 		mmc_hostname(host->mmc),
 		bcm2835_sdhost_read(host, SDRSP3));
 	pr_info("%s: SDHSTS 0x%08x\n",
@@ -1183,9 +1183,8 @@ static void bcm2835_sdhost_finish_comman
 		retries = 1; // We've already waited long enough this time
 	}
 
-	retries = host->cmd_quick_poll_retries;
 	for (sdcmd = bcm2835_sdhost_read(host, SDCMD);
-	     (sdcmd & SDCMD_NEW_FLAG) && !(sdcmd & SDCMD_FAIL_FLAG) && retries;
+	     (sdcmd & SDCMD_NEW_FLAG) && retries;
 	     retries--) {
 		cpu_relax();
 		sdcmd = bcm2835_sdhost_read(host, SDCMD);
@@ -1208,8 +1207,7 @@ static void bcm2835_sdhost_finish_comman
 			usleep_range(1, 10);
 			spin_lock_irqsave(&host->lock, *irq_flags);
 			sdcmd = bcm2835_sdhost_read(host, SDCMD);
-			if (!(sdcmd & SDCMD_NEW_FLAG) ||
-			    (sdcmd & SDCMD_FAIL_FLAG))
+			if (!(sdcmd & SDCMD_NEW_FLAG))
 				break;
 		}
 	}
@@ -1892,8 +1890,6 @@ int bcm2835_sdhost_add_host(struct bcm28
 
 	mmc = host->mmc;
 
-	bcm2835_sdhost_reset_internal(host);
-
 	mmc->f_max = host->max_clk;
 	mmc->f_min = host->max_clk / SDCDIV_MAX_CDIV;
 
