From 9654afa1c26516e3461cd8575f08b367fe5ff42a Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Mon, 15 Feb 2016 17:31:41 -0800
Subject: [PATCH] drm/vc4: Fix setting of vertical timings in the CRTC.

It looks like when I went to add the interlaced bits, I just took the
existing PV_VERT* block and indented it, instead of copy and pasting
it first.  Without this, changing resolution never worked.

Signed-off-by: Eric Anholt <eric@anholt.net>
(cherry picked from commit a7c5047d1ce178dd2b1fa577fc8909ad663d56d5)
---
 drivers/gpu/drm/vc4/vc4_crtc.c | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/drivers/gpu/drm/vc4/vc4_crtc.c
+++ b/drivers/gpu/drm/vc4/vc4_crtc.c
@@ -217,6 +217,16 @@ static void vc4_crtc_mode_set_nofb(struc
 				 PV_HORZB_HFP) |
 		   VC4_SET_FIELD(mode->hdisplay, PV_HORZB_HACTIVE));
 
+	CRTC_WRITE(PV_VERTA,
+		   VC4_SET_FIELD(mode->vtotal - mode->vsync_end,
+				 PV_VERTA_VBP) |
+		   VC4_SET_FIELD(mode->vsync_end - mode->vsync_start,
+				 PV_VERTA_VSYNC));
+	CRTC_WRITE(PV_VERTB,
+		   VC4_SET_FIELD(mode->vsync_start - mode->vdisplay,
+				 PV_VERTB_VFP) |
+		   VC4_SET_FIELD(vactive, PV_VERTB_VACTIVE));
+
 	if (interlace) {
 		CRTC_WRITE(PV_VERTA_EVEN,
 			   VC4_SET_FIELD(mode->vtotal - mode->vsync_end - 1,
