From b49d7bb4825654f81bcee8e219028712811515a5 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Mon, 29 Jun 2015 08:11:36 +0200
Subject: [PATCH] ARM: BCM5301X: Enable ChipCommon UART on untested devices
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 arch/arm/boot/dts/bcm4708-asus-rt-ac56u.dts       | 4 ++++
 arch/arm/boot/dts/bcm4708-asus-rt-ac68u.dts       | 4 ++++
 arch/arm/boot/dts/bcm4708-netgear-r6300-v2.dts    | 4 ++++
 arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts       | 4 ++++
 arch/arm/boot/dts/bcm47081-buffalo-wzr-900dhp.dts | 4 ++++
 arch/arm/boot/dts/bcm4709-asus-rt-ac87u.dts       | 5 +++++
 arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts | 5 +++++
 arch/arm/boot/dts/bcm4709-netgear-r8000.dts       | 5 +++++
 8 files changed, 35 insertions(+)

--- a/arch/arm/boot/dts/bcm4708-asus-rt-ac56u.dts
+++ b/arch/arm/boot/dts/bcm4708-asus-rt-ac56u.dts
@@ -96,3 +96,7 @@
 		};
 	};
 };
+
+&uart0 {
+	status = "okay";
+};
--- a/arch/arm/boot/dts/bcm4708-asus-rt-ac68u.dts
+++ b/arch/arm/boot/dts/bcm4708-asus-rt-ac68u.dts
@@ -83,3 +83,7 @@
 		};
 	};
 };
+
+&uart0 {
+	status = "okay";
+};
--- a/arch/arm/boot/dts/bcm4708-netgear-r6300-v2.dts
+++ b/arch/arm/boot/dts/bcm4708-netgear-r6300-v2.dts
@@ -87,3 +87,7 @@
 &spi_nor {
 	status = "okay";
 };
+
+&uart0 {
+	status = "okay";
+};
--- a/arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts
+++ b/arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts
@@ -77,3 +77,7 @@
 		};
 	};
 };
+
+&uart0 {
+	status = "okay";
+};
--- a/arch/arm/boot/dts/bcm47081-buffalo-wzr-900dhp.dts
+++ b/arch/arm/boot/dts/bcm47081-buffalo-wzr-900dhp.dts
@@ -37,3 +37,7 @@
 		};
 	};
 };
+
+&uart0 {
+	status = "okay";
+};
--- a/arch/arm/boot/dts/bcm4709-asus-rt-ac87u.dts
+++ b/arch/arm/boot/dts/bcm4709-asus-rt-ac87u.dts
@@ -65,3 +65,7 @@
 		};
 	};
 };
+
+&uart0 {
+	status = "okay";
+};
--- a/arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts
+++ b/arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts
@@ -128,6 +128,9 @@
 	};
 };
 
+&uart0 {
+	status = "okay";
+};
 
 &usb2 {
 	vcc-gpio = <&chipcommon 13 GPIO_ACTIVE_HIGH>;
