From 87dd923568a28a6784581a3f4c18970b834779a8 Mon Sep 17 00:00:00 2001
From: popcornmix <popcornmix@gmail.com>
Date: Mon, 21 Mar 2016 15:38:38 +0000
Subject: [PATCH] dwc_otg: Enable the hack for Split Interrupt transactions by
 default

dwc_otg.fiq_fsm_mask=0xF has long been a suggestion for users with audio stutters or other USB bandwidth issues.
So far we are aware of many success stories but no failure caused by this setting.
Make it a default to learn more.

See: https://www.raspberrypi.org/forums/viewtopic.php?f=28&t=70437

Signed-off-by: popcornmix <popcornmix@gmail.com>
---
 drivers/usb/host/dwc_otg/dwc_otg_driver.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/usb/host/dwc_otg/dwc_otg_driver.c
+++ b/drivers/usb/host/dwc_otg/dwc_otg_driver.c
@@ -247,7 +247,7 @@ bool fiq_fsm_enable = true;
 //Bulk split-transaction NAK holdoff in microframes
 uint16_t nak_holdoff = 8;
 
-unsigned short fiq_fsm_mask = 0x07;
+unsigned short fiq_fsm_mask = 0x0F;
 
 /**
  * This function shows the Driver Version.
