#!/bin/sh
#
# Copyright (C) 2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh
. /lib/ipq806x.sh

board_config_update

board=$(ipq806x_board_name)

case "$board" in
c2600)
	ucidef_set_led_usbport "usb1" "USB 1" "${board}:white:usb_2" "usb1-port1" "usb2-port1"
	ucidef_set_led_usbport "usb2" "USB 2" "${board}:white:usb_4" "usb3-port1" "usb4-port1"
	ucidef_set_led_switch "wan" "wan" "${board}:white:wan" "switch0" "0x20"
	ucidef_set_led_switch "lan" "lan" "${board}:white:lan" "switch0" "0x1e"
	ucidef_set_led_default "general" "general" "${board}:white:ledgnr" "1"
	;;
d7800 |\
r7500 |\
r7500v2)
	ucidef_set_led_usbdev "usb1" "USB 1" "${board}:white:usb1" "1-1"
	ucidef_set_led_usbdev "usb2" "USB 2" "${board}:white:usb3" "3-1"
	ucidef_set_led_netdev "wan" "WAN" "${board}:white:wan" "eth0"
	ucidef_set_led_ide "esata" "eSATA" "${board}:amber:esata"
	ucidef_set_led_default "wps" "WPS" "${board}:white:wps" "0"
	ucidef_set_led_default "rfkill" "rfkill" "${board}:white:rfkill" "0"
	;;
r7800)
	ucidef_set_led_usbport "usb1" "USB 1" "${board}:white:usb1" "usb1-port1" "usb2-port1"
	ucidef_set_led_usbport "usb2" "USB 2" "${board}:white:usb2" "usb3-port1" "usb4-port1"
	ucidef_set_led_netdev "wan" "WAN" "${board}:white:wan" "eth0"
	ucidef_set_led_ide "esata" "eSATA" "${board}:white:esata"
	ucidef_set_led_wlan "wps" "WPS" "${board}:white:wps" "phy0tpt"
	ucidef_set_led_wlan "rfkill" "rfkill" "${board}:white:rfkill" "phy1tpt"
	;;
ea8500)
	ucidef_set_led_wlan "wifi" "WIFI" "ea8500:green:wifi" "phy0radio"
	ucidef_set_led_default "wps" "WPS" "ea8500:green:wps" "0"
	;;
nbg6817)
	ucidef_set_led_wlan "wlan2g" "WLAN2g" "$board:amber:wifi" "phy1radio"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "$board:amber:wifi5" "phy0radio"
	ucidef_set_led_netdev "wan" "WAN" "$board:white:internet" "eth1"
	;;
vr2600v)
	ucidef_set_led_usbport "usb" "USB" "${board}:white:usb" "usb1-port1" "usb2-port1" "usb3-port1" "usb4-port1"
	ucidef_set_led_switch "lan" "lan" "${board}:white:lan" "switch0" "0x1e"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "${board}:white:wlan2g" "phy0radio"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "${board}:white:wlan5g" "phy1radio"
	ucidef_set_led_switch "wan" "wan" "${board}:white:wan" "switch0" "0x20"
	;;
*)
	;;
esac

board_config_flush

exit 0
