From ee286f4b57536ec4a7c1b52d0a3476f8e52594d5 Mon Sep 17 00:00:00 2001
From: Jes Sorensen <Jes.Sorensen@redhat.com>
Date: Fri, 30 Sep 2016 16:39:39 -0400
Subject: [PATCH] rtl8xxxu: Fix rtl8723bu driver reload issue

The generic disable_rf() function clears bits 22 and 23 in
REG_RX_WAIT_CCA, however we did not re-enable them again in
rtl8723b_enable_rf()

This resolves the problem for me with 8723bu devices not working again
after reloading the driver.

Signed-off-by: Jes Sorensen <Jes.Sorensen@redhat.com>
---
 drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_8723b.c | 4 ++++
 1 file changed, 4 insertions(+)

--- a/drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_8723b.c
+++ b/drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_8723b.c
@@ -1498,6 +1498,10 @@ static void rtl8723b_enable_rf(struct rt
 	u32 val32;
 	u8 val8;
 
+	val32 = rtl8xxxu_read32(priv, REG_RX_WAIT_CCA);
+	val32 |= (BIT(22) | BIT(23));
+	rtl8xxxu_write32(priv, REG_RX_WAIT_CCA, val32);
+
 	/*
 	 * No indication anywhere as to what 0x0790 does. The 2 antenna
 	 * vendor code preserves bits 6-7 here.
