--- a/arch/mips/lantiq/xway/reset.c	2016-01-20 08:45:18.382597595 +0100
+++ b/arch/mips/lantiq/xway/reset.c	2016-01-20 08:45:31.927107016 +0100
@@ -370,6 +370,7 @@ static int __init mips_reboot_setup(void
 		panic("Failed to remap core memory");
 
 	if (of_machine_is_compatible("lantiq,ar9") ||
+	    of_machine_is_compatible("lantiq,danube") ||
 	    of_machine_is_compatible("lantiq,vr9"))
 		ltq_usb_init();
 
