From 5bdac7f7f6e6d9938da0d6bd0d58a136cf29515b Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Fri, 12 Aug 2016 11:02:14 -0700
Subject: [PATCH] BCM2710: Drop incorrect HDMI HPD line from the DT.

It's actually off on the GPIO expander, which I don't think we have
access to.

Signed-off-by: Eric Anholt <eric@anholt.net>
---
 arch/arm/boot/dts/bcm2710-rpi-3-b.dts | 4 ----
 1 file changed, 4 deletions(-)

--- a/arch/arm/boot/dts/bcm2710-rpi-3-b.dts
+++ b/arch/arm/boot/dts/bcm2710-rpi-3-b.dts
@@ -166,10 +166,6 @@
 	};
 };
 
-&hdmi {
-	hpd-gpios = <&gpio 46 GPIO_ACTIVE_LOW>;
-};
-
 &audio {
 	pinctrl-names = "default";
 	pinctrl-0 = <&audio_pins>;
