From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Subject: [PATCH] mtd: bcm47xxpart: fix parsing first block after aligned TRX
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

After parsing TRX we should skip to the first block placed behind it.
Our code was working only with TRX with length not aligned to the
blocksize. In other cases (length aligned) it was missing the block
places right after TRX.

This fixes calculation and simplifies the comment.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
---
 drivers/mtd/bcm47xxpart.c | 10 ++++------
 1 file changed, 4 insertions(+), 6 deletions(-)

--- a/drivers/mtd/bcm47xxpart.c
+++ b/drivers/mtd/bcm47xxpart.c
@@ -229,12 +229,10 @@ static int bcm47xxpart_parse(struct mtd_
 
 			last_trx_part = curr_part - 1;
 
-			/*
-			 * We have whole TRX scanned, skip to the next part. Use
-			 * roundown (not roundup), as the loop will increase
-			 * offset in next step.
-			 */
-			offset = rounddown(offset + trx->length, blocksize);
+			/* Jump to the end of TRX */
+			offset = roundup(offset + trx->length, blocksize);
+			/* Next loop iteration will increase the offset */
+			offset -= blocksize;
 			continue;
 		}
 
