From eb25cb9956cc9384b7fa0d75dec908c9fac8c444 Mon Sep 17 00:00:00 2001
From: Stephan Linz <linz@li-pro.net>
Date: Fri, 10 Jun 2016 07:59:56 +0200
Subject: [PATCH] leds: convert IDE trigger to common disk trigger
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This patch converts the IDE specific LED trigger to a generic disk
activity LED trigger. The libata core is now a trigger source just
like before the IDE disk driver. It's merely a replacement of the
string ide by disk.

The patch is taken from http://dev.gentoo.org/~josejx/ata.patch and is
widely used by any ibook/powerbook owners with great satisfaction.
Likewise, it is very often used successfully on different ARM platforms.

Unlike the original patch, the existing 'ide-disk' trigger is still
available for backward compatibility. That reduce the amount of patches
in affected device trees out of the mainline kernel. For further
development, the new name 'disk-activity' should be used.

Cc: Joseph Jezak <josejx@gentoo.org>
Cc: Jörg Sommer <joerg@alea.gnuu.de>
Cc: Richard Purdie <rpurdie@rpsys.net>
Signed-off-by: Stephan Linz <linz@li-pro.net>
Signed-off-by: Jacek Anaszewski <j.anaszewski@samsung.com>
---
 drivers/ata/libata-core.c               |  4 ++++
 drivers/ide/ide-disk.c                  |  2 +-
 drivers/leds/trigger/Kconfig            |  8 +++----
 drivers/leds/trigger/Makefile           |  2 +-
 drivers/leds/trigger/ledtrig-disk.c     | 41 +++++++++++++++++++++++++++++++++
 drivers/leds/trigger/ledtrig-ide-disk.c | 36 -----------------------------
 include/linux/leds.h                    |  6 ++---
 8 files changed, 55 insertions(+), 46 deletions(-)
 create mode 100644 drivers/leds/trigger/ledtrig-disk.c
 delete mode 100644 drivers/leds/trigger/ledtrig-ide-disk.c

--- a/drivers/ata/libata-core.c
+++ b/drivers/ata/libata-core.c
@@ -67,6 +67,7 @@
 #include <asm/byteorder.h>
 #include <linux/cdrom.h>
 #include <linux/ratelimit.h>
+#include <linux/leds.h>
 #include <linux/pm_runtime.h>
 #include <linux/platform_device.h>
 
@@ -4914,6 +4915,9 @@ void ata_qc_complete(struct ata_queued_c
 {
 	struct ata_port *ap = qc->ap;
 
+	/* Trigger the LED (if available) */
+	ledtrig_disk_activity();
+
 	/* XXX: New EH and old EH use different mechanisms to
 	 * synchronize EH with regular execution path.
 	 *
--- a/drivers/ide/ide-disk.c
+++ b/drivers/ide/ide-disk.c
@@ -186,7 +186,7 @@ static ide_startstop_t ide_do_rw_disk(id
 	BUG_ON(drive->dev_flags & IDE_DFLAG_BLOCKED);
 	BUG_ON(rq->cmd_type != REQ_TYPE_FS);
 
-	ledtrig_ide_activity();
+	ledtrig_disk_activity();
 
 	pr_debug("%s: %sing: block=%llu, sectors=%u\n",
 		 drive->name, rq_data_dir(rq) == READ ? "read" : "writ",
--- a/drivers/leds/trigger/Kconfig
+++ b/drivers/leds/trigger/Kconfig
@@ -33,12 +33,12 @@ config LEDS_TRIGGER_ONESHOT
 
 	  If unsure, say Y.
 
-config LEDS_TRIGGER_IDE_DISK
-	bool "LED IDE Disk Trigger"
-	depends on IDE_GD_ATA
+config LEDS_TRIGGER_DISK
+	bool "LED Disk Trigger"
+	depends on IDE_GD_ATA || ATA
 	depends on LEDS_TRIGGERS
 	help
-	  This allows LEDs to be controlled by IDE disk activity.
+	  This allows LEDs to be controlled by disk activity.
 	  If unsure, say Y.
 
 config LEDS_TRIGGER_HEARTBEAT
--- a/drivers/leds/trigger/Makefile
+++ b/drivers/leds/trigger/Makefile
@@ -1,6 +1,6 @@
 obj-$(CONFIG_LEDS_TRIGGER_TIMER)	+= ledtrig-timer.o
 obj-$(CONFIG_LEDS_TRIGGER_ONESHOT)	+= ledtrig-oneshot.o
-obj-$(CONFIG_LEDS_TRIGGER_IDE_DISK)	+= ledtrig-ide-disk.o
+obj-$(CONFIG_LEDS_TRIGGER_DISK)		+= ledtrig-disk.o
 obj-$(CONFIG_LEDS_TRIGGER_HEARTBEAT)	+= ledtrig-heartbeat.o
 obj-$(CONFIG_LEDS_TRIGGER_BACKLIGHT)	+= ledtrig-backlight.o
 obj-$(CONFIG_LEDS_TRIGGER_GPIO)		+= ledtrig-gpio.o
--- /dev/null
+++ b/drivers/leds/trigger/ledtrig-disk.c
@@ -0,0 +1,41 @@
+/*
+ * LED Disk Activity Trigger
+ *
+ * Copyright 2006 Openedhand Ltd.
+ *
+ * Author: Richard Purdie <rpurdie@openedhand.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ *
+ */
+
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <linux/leds.h>
+
+#define BLINK_DELAY 30
+
+DEFINE_LED_TRIGGER(ledtrig_disk);
+DEFINE_LED_TRIGGER(ledtrig_ide);
+
+void ledtrig_disk_activity(void)
+{
+	unsigned long blink_delay = BLINK_DELAY;
+
+	led_trigger_blink_oneshot(ledtrig_disk,
+				  &blink_delay, &blink_delay, 0);
+	led_trigger_blink_oneshot(ledtrig_ide,
+				  &blink_delay, &blink_delay, 0);
+}
+EXPORT_SYMBOL(ledtrig_disk_activity);
+
+static int __init ledtrig_disk_init(void)
+{
+	led_trigger_register_simple("disk-activity", &ledtrig_disk);
+	led_trigger_register_simple("ide-disk", &ledtrig_ide);
+
+	return 0;
+}
+device_initcall(ledtrig_disk_init);
--- a/drivers/leds/trigger/ledtrig-ide-disk.c
+++ /dev/null
@@ -1,47 +0,0 @@
-/*
- * LED IDE-Disk Activity Trigger
- *
- * Copyright 2006 Openedhand Ltd.
- *
- * Author: Richard Purdie <rpurdie@openedhand.com>
- *
- * This program is free software; you can redistribute it and/or modify
- * it under the terms of the GNU General Public License version 2 as
- * published by the Free Software Foundation.
- *
- */
-
-#include <linux/module.h>
-#include <linux/kernel.h>
-#include <linux/init.h>
-#include <linux/leds.h>
-
-#define BLINK_DELAY 30
-
-DEFINE_LED_TRIGGER(ledtrig_ide);
-static unsigned long ide_blink_delay = BLINK_DELAY;
-
-void ledtrig_ide_activity(void)
-{
-	led_trigger_blink_oneshot(ledtrig_ide,
-				  &ide_blink_delay, &ide_blink_delay, 0);
-}
-EXPORT_SYMBOL(ledtrig_ide_activity);
-
-static int __init ledtrig_ide_init(void)
-{
-	led_trigger_register_simple("ide-disk", &ledtrig_ide);
-	return 0;
-}
-
-static void __exit ledtrig_ide_exit(void)
-{
-	led_trigger_unregister_simple(ledtrig_ide);
-}
-
-module_init(ledtrig_ide_init);
-module_exit(ledtrig_ide_exit);
-
-MODULE_AUTHOR("Richard Purdie <rpurdie@openedhand.com>");
-MODULE_DESCRIPTION("LED IDE Disk Activity Trigger");
-MODULE_LICENSE("GPL");
--- a/include/linux/leds.h
+++ b/include/linux/leds.h
@@ -302,10 +302,10 @@ static inline void *led_get_trigger_data
 #endif /* CONFIG_LEDS_TRIGGERS */
 
 /* Trigger specific functions */
-#ifdef CONFIG_LEDS_TRIGGER_IDE_DISK
-extern void ledtrig_ide_activity(void);
+#ifdef CONFIG_LEDS_TRIGGER_DISK
+extern void ledtrig_disk_activity(void);
 #else
-static inline void ledtrig_ide_activity(void) {}
+static inline void ledtrig_disk_activity(void) {}
 #endif
 
 #if defined(CONFIG_LEDS_TRIGGER_CAMERA) || defined(CONFIG_LEDS_TRIGGER_CAMERA_MODULE)
