From: Felix Fietkau <nbd@nbd.name>
Date: Mon, 13 Apr 2015 15:54:04 +0200
Subject: [PATCH] bgmac: fix MAC soft-reset bit for corerev > 4

Only core revisions older than 4 use BGMAC_CMDCFG_SR_REV0

Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/drivers/net/ethernet/broadcom/bgmac.h
+++ b/drivers/net/ethernet/broadcom/bgmac.h
@@ -198,9 +198,9 @@
 #define  BGMAC_CMDCFG_TAI			0x00000200
 #define  BGMAC_CMDCFG_HD			0x00000400	/* Set if in half duplex mode */
 #define  BGMAC_CMDCFG_HD_SHIFT			10
-#define  BGMAC_CMDCFG_SR_REV0			0x00000800	/* Set to reset mode, for other revs */
-#define  BGMAC_CMDCFG_SR_REV4			0x00002000	/* Set to reset mode, only for core rev 4 */
-#define  BGMAC_CMDCFG_SR(rev)  ((rev == 4) ? BGMAC_CMDCFG_SR_REV4 : BGMAC_CMDCFG_SR_REV0)
+#define  BGMAC_CMDCFG_SR_REV0			0x00000800	/* Set to reset mode, for core rev 0-3 */
+#define  BGMAC_CMDCFG_SR_REV4			0x00002000	/* Set to reset mode, for core rev >= 4 */
+#define  BGMAC_CMDCFG_SR(rev)  ((rev >= 4) ? BGMAC_CMDCFG_SR_REV4 : BGMAC_CMDCFG_SR_REV0)
 #define  BGMAC_CMDCFG_ML			0x00008000	/* Set to activate mac loopback mode */
 #define  BGMAC_CMDCFG_AE			0x00400000
 #define  BGMAC_CMDCFG_CFE			0x00800000
