From ec662a26071a7aa2d7617ac366ce91beebaf2ad1 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Fri, 19 Aug 2016 11:19:02 +0100
Subject: [PATCH] BCM270X_DT: Don't enable UART0 in CM3 dtb

---
 arch/arm/boot/dts/bcm2710-rpi-cm3.dts | 12 ------------
 1 file changed, 12 deletions(-)

--- a/arch/arm/boot/dts/bcm2710-rpi-cm3.dts
+++ b/arch/arm/boot/dts/bcm2710-rpi-cm3.dts
@@ -40,12 +40,6 @@
 		brcm,function = <4>; /* alt0 */
 	};
 
-	uart0_pins: uart0_pins {
-		brcm,pins;
-		brcm,function;
-		brcm,pull = <0 2>;
-	};
-
 	audio_pins: audio_pins {
 		brcm,pins;
 		brcm,function;
@@ -75,12 +69,6 @@
 	status = "okay";
 };
 
-&uart0 {
-	pinctrl-names = "default";
-	pinctrl-0 = <&uart0_pins>;
-	status = "okay";
-};
-
 &spi0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
