From 90ded6778736d5a0843d24eb8e5a47db72c05af9 Mon Sep 17 00:00:00 2001
From: Mingkai Hu <mingkai.hu@nxp.com>
Date: Mon, 18 Apr 2016 22:44:21 +0800
Subject: [PATCH 21/93] sf: set the Uniform Sector to CR3NV instead of CR3V

Signed-off-by: Mingkai Hu <mingkai.hu@nxp.com>
---
 drivers/mtd/spi/spi_flash.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/mtd/spi/spi_flash.c b/drivers/mtd/spi/spi_flash.c
index 865e929..97e53c7 100644
--- a/drivers/mtd/spi/spi_flash.c
+++ b/drivers/mtd/spi/spi_flash.c
@@ -942,7 +942,7 @@ int spi_flash_decode_fdt(const void *blob, struct spi_flash *flash)
 static int spansion_s25fss_disable_4KB_erase(struct spi_slave *spi)
 {
 	u8 cmd[4];
-	u32 offset = 0x800004; /* CR3V register offset */
+	u32 offset = 0x000004; /* CR3NV register offset */
 	u8 cr3v;
 	int ret;
 
-- 
1.7.9.5

