From: Florian Fainelli <f.fainelli@gmail.com>
Subject: [PATCH v3 7/9] mtd: rawnand: brcmnand: Allow platform data instantation
Date: Fri, 07 Jan 2022 10:46:12 -0800
Content-Type: text/plain; charset="utf-8"

Make use of the recently refactored code in brcmnand_init_cs() and
derive the chip-select from the platform data that is supplied. Update
the various code paths to avoid relying on possibly non-existent
resources, too.

Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 drivers/mtd/nand/raw/brcmnand/brcmnand.c | 45 ++++++++++++++++++------
 1 file changed, 35 insertions(+), 10 deletions(-)

--- a/drivers/mtd/nand/raw/brcmnand/brcmnand.c
+++ b/drivers/mtd/nand/raw/brcmnand/brcmnand.c
@@ -9,6 +9,7 @@
 #include <linux/delay.h>
 #include <linux/device.h>
 #include <linux/platform_device.h>
+#include <linux/platform_data/brcmnand.h>
 #include <linux/err.h>
 #include <linux/completion.h>
 #include <linux/interrupt.h>
@@ -2811,7 +2812,8 @@ static const struct nand_controller_ops
 	.attach_chip = brcmnand_attach_chip,
 };
 
-static int brcmnand_init_cs(struct brcmnand_host *host)
+static int brcmnand_init_cs(struct brcmnand_host *host,
+			    const char * const *part_probe_types)
 {
 	struct brcmnand_controller *ctrl = host->ctrl;
 	struct device *dev = ctrl->dev;
@@ -2864,7 +2866,7 @@ static int brcmnand_init_cs(struct brcmn
 	if (ret)
 		return ret;
 
-	ret = mtd_device_register(mtd, NULL, 0);
+	ret = mtd_device_parse_register(mtd, part_probe_types, NULL, NULL, 0);
 	if (ret)
 		nand_cleanup(chip);
 
@@ -3033,17 +3035,15 @@ static int brcmnand_edu_setup(struct pla
 
 int brcmnand_probe(struct platform_device *pdev, struct brcmnand_soc *soc)
 {
+	struct brcmnand_platform_data *pd = dev_get_platdata(&pdev->dev);
 	struct device *dev = &pdev->dev;
 	struct device_node *dn = dev->of_node, *child;
 	struct brcmnand_controller *ctrl;
+	struct brcmnand_host *host;
 	struct resource *res;
 	int ret;
 
-	/* We only support device-tree instantiation */
-	if (!dn)
-		return -ENODEV;
-
-	if (!of_match_node(brcmnand_of_match, dn))
+	if (dn && !of_match_node(brcmnand_of_match, dn))
 		return -ENODEV;
 
 	ctrl = devm_kzalloc(dev, sizeof(*ctrl), GFP_KERNEL);
@@ -3070,7 +3070,7 @@ int brcmnand_probe(struct platform_devic
 	/* NAND register range */
 	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
 	ctrl->nand_base = devm_ioremap_resource(dev, res);
-	if (IS_ERR(ctrl->nand_base))
+	if (IS_ERR(ctrl->nand_base) && !brcmnand_soc_has_ops(soc))
 		return PTR_ERR(ctrl->nand_base);
 
 	/* Enable clock before using NAND registers */
@@ -3218,7 +3218,6 @@ int brcmnand_probe(struct platform_devic
 
 	for_each_available_child_of_node(dn, child) {
 		if (of_device_is_compatible(child, "brcm,nandcs")) {
-			struct brcmnand_host *host;
 
 			host = devm_kzalloc(dev, sizeof(*host), GFP_KERNEL);
 			if (!host) {
@@ -3238,7 +3237,7 @@ int brcmnand_probe(struct platform_devic
 
 			nand_set_flash_node(&host->chip, child);
 
-			ret = brcmnand_init_cs(host);
+			ret = brcmnand_init_cs(host, NULL);
 			if (ret) {
 				devm_kfree(dev, host);
 				continue; /* Try all chip-selects */
@@ -3248,6 +3247,32 @@ int brcmnand_probe(struct platform_devic
 		}
 	}
 
+	if (!list_empty(&ctrl->host_list))
+		return 0;
+
+	if (!pd) {
+		ret = -ENODEV;
+		goto err;
+	}
+
+	/* If we got there we must have been probing via platform data */
+	host = devm_kzalloc(dev, sizeof(*host), GFP_KERNEL);
+	if (!host) {
+		ret = -ENOMEM;
+		goto err;
+	}
+	host->pdev = pdev;
+	host->ctrl = ctrl;
+	host->cs = pd->chip_select;
+	host->chip.ecc.size = pd->ecc_stepsize;
+	host->chip.ecc.strength = pd->ecc_strength;
+
+	ret = brcmnand_init_cs(host, pd->part_probe_types);
+	if (ret)
+		goto err;
+
+	list_add_tail(&host->node, &ctrl->host_list);
+
 	/* No chip-selects could initialize properly */
 	if (list_empty(&ctrl->host_list)) {
 		ret = -ENODEV;
