From 7390609b0121a1b982c5ecdfcd72dc328e5784ee Mon Sep 17 00:00:00 2001
From: Michael Walle <michael@walle.cc>
Date: Mon, 6 Feb 2023 13:43:42 +0000
Subject: [PATCH] net: add helper eth_addr_add()

Add a helper to add an offset to a ethernet address. This comes in handy
if you have a base ethernet address for multiple interfaces.

Signed-off-by: Michael Walle <michael@walle.cc>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Acked-by: Jakub Kicinski <kuba@kernel.org>
Signed-off-by: Srinivas Kandagatla <srinivas.kandagatla@linaro.org>
Link: https://lore.kernel.org/r/20230206134356.839737-9-srinivas.kandagatla@linaro.org
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 include/linux/etherdevice.h | 14 ++++++++++++++
 1 file changed, 14 insertions(+)

--- a/include/linux/etherdevice.h
+++ b/include/linux/etherdevice.h
@@ -508,6 +508,20 @@ static inline void eth_addr_inc(u8 *addr
 }
 
 /**
+ * eth_addr_add() - Add (or subtract) an offset to/from the given MAC address.
+ *
+ * @offset: Offset to add.
+ * @addr: Pointer to a six-byte array containing Ethernet address to increment.
+ */
+static inline void eth_addr_add(u8 *addr, long offset)
+{
+	u64 u = ether_addr_to_u64(addr);
+
+	u += offset;
+	u64_to_ether_addr(u, addr);
+}
+
+/**
  * is_etherdev_addr - Tell if given Ethernet address belongs to the device.
  * @dev: Pointer to a device structure
  * @addr: Pointer to a six-byte array containing the Ethernet address
