From feeef118fda562cf9081edef8ad464d89db070f4 Mon Sep 17 00:00:00 2001
From: Robert Marko <robimarko@gmail.com>
Date: Tue, 27 Sep 2022 22:12:18 +0200
Subject: [PATCH] arm64: dts: qcom: ipq6018: move ARMv8 timer out of SoC node

The ARM timer is usually considered not part of SoC node, just like
other ARM designed blocks (PMU, PSCI).  This fixes dtbs_check warning:

arch/arm64/boot/dts/qcom/ipq6018-cp01-c1.dtb: soc: timer: {'compatible': ['arm,armv8-timer'], 'interrupts': [[1, 2, 3848], [1, 3, 3848], [1, 4, 3848], [1, 1, 3848]]} should not be valid under {'type': 'object'}
	From schema: dtschema/schemas/simple-bus.yaml

Signed-off-by: Robert Marko <robimarko@gmail.com>
Reviewed-by: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Reviewed-by: Neil Armstrong <neil.armstrong@linaro.org>
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
Link: https://lore.kernel.org/r/20220927201218.1264506-2-robimarko@gmail.com
---
 arch/arm64/boot/dts/qcom/ipq6018.dtsi | 16 ++++++++--------
 1 file changed, 8 insertions(+), 8 deletions(-)

--- a/arch/arm64/boot/dts/qcom/ipq6018.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq6018.dtsi
@@ -510,14 +510,6 @@
 			clock-names = "xo";
 		};
 
-		timer {
-			compatible = "arm,armv8-timer";
-			interrupts = <GIC_PPI 2 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
-				     <GIC_PPI 3 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
-				     <GIC_PPI 4 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
-				     <GIC_PPI 1 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>;
-		};
-
 		timer@b120000 {
 			#address-cells = <1>;
 			#size-cells = <1>;
@@ -769,6 +761,14 @@
 		};
 	};
 
+	timer {
+		compatible = "arm,armv8-timer";
+		interrupts = <GIC_PPI 2 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 3 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 4 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 1 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>;
+	};
+
 	wcss: wcss-smp2p {
 		compatible = "qcom,smp2p";
 		qcom,smem = <435>, <428>;
