From a8bdb91f7d3fb93b0e4304602fba5e15d93fc4ce Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Wed, 31 Oct 2018 14:59:40 +0000
Subject: [PATCH] MAINTAINERS: Add entry for BCM2835 Unicam driver

Adds entry for the new BCM2835 Unicam (CSI-2 receiver) driver

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 MAINTAINERS | 7 +++++++
 1 file changed, 7 insertions(+)

--- a/MAINTAINERS
+++ b/MAINTAINERS
@@ -4030,6 +4030,13 @@ N:	bcm113*
 N:	bcm216*
 N:	kona
 
+BROADCOM BCM2835 CAMERA DRIVER
+M:	Dave Stevenson <dave.stevenson@raspberrypi.org>
+L:	linux-media@vger.kernel.org
+S:	Maintained
+F:	drivers/media/platform/bcm2835/
+F:	Documentation/devicetree/bindings/media/bcm2835-unicam.txt
+
 BROADCOM BCM47XX MIPS ARCHITECTURE
 M:	Hauke Mehrtens <hauke@hauke-m.de>
 M:	Rafał Miłecki <zajec5@gmail.com>
