From e6c32770ef83f3e8cc057f3920b1c06aa9d1c9c2 Mon Sep 17 00:00:00 2001
From: Chukun Pan <amadeus@jmu.edu.cn>
Date: Sun, 3 Dec 2023 23:39:14 +0800
Subject: [PATCH] arm64: dts: qcom: ipq6018: Add remaining QUP UART node

Add node to support all the QUP UART node controller inside of IPQ6018.
Some routers use these bus to connect Bluetooth chips.

Signed-off-by: Chukun Pan <amadeus@jmu.edu.cn>
Link: https://lore.kernel.org/r/20231203153914.532654-1-amadeus@jmu.edu.cn
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
---
 arch/arm64/boot/dts/qcom/ipq6018.dtsi | 50 +++++++++++++++++++++++++++
 1 file changed, 50 insertions(+)

--- a/arch/arm64/boot/dts/qcom/ipq6018.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq6018.dtsi
@@ -458,6 +458,26 @@
 			qcom,ee = <0>;
 		};
 
+		blsp1_uart1: serial@78af000 {
+			compatible = "qcom,msm-uartdm-v1.4", "qcom,msm-uartdm";
+			reg = <0x0 0x78af000 0x0 0x200>;
+			interrupts = <GIC_SPI 107 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&gcc GCC_BLSP1_UART1_APPS_CLK>,
+				 <&gcc GCC_BLSP1_AHB_CLK>;
+			clock-names = "core", "iface";
+			status = "disabled";
+		};
+
+		blsp1_uart2: serial@78b0000 {
+			compatible = "qcom,msm-uartdm-v1.4", "qcom,msm-uartdm";
+			reg = <0x0 0x78b0000 0x0 0x200>;
+			interrupts = <GIC_SPI 108 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&gcc GCC_BLSP1_UART2_APPS_CLK>,
+				 <&gcc GCC_BLSP1_AHB_CLK>;
+			clock-names = "core", "iface";
+			status = "disabled";
+		};
+
 		blsp1_uart3: serial@78b1000 {
 			compatible = "qcom,msm-uartdm-v1.4", "qcom,msm-uartdm";
 			reg = <0x0 0x078b1000 0x0 0x200>;
@@ -466,6 +486,36 @@
 				 <&gcc GCC_BLSP1_AHB_CLK>;
 			clock-names = "core", "iface";
 			status = "disabled";
+		};
+
+		blsp1_uart4: serial@78b2000 {
+			compatible = "qcom,msm-uartdm-v1.4", "qcom,msm-uartdm";
+			reg = <0x0 0x078b2000 0x0 0x200>;
+			interrupts = <GIC_SPI 307 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&gcc GCC_BLSP1_UART4_APPS_CLK>,
+				 <&gcc GCC_BLSP1_AHB_CLK>;
+			clock-names = "core", "iface";
+			status = "disabled";
+		};
+
+		blsp1_uart5: serial@78b3000 {
+			compatible = "qcom,msm-uartdm-v1.4", "qcom,msm-uartdm";
+			reg = <0x0 0x78b3000 0x0 0x200>;
+			interrupts = <GIC_SPI 308 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&gcc GCC_BLSP1_UART5_APPS_CLK>,
+				 <&gcc GCC_BLSP1_AHB_CLK>;
+			clock-names = "core", "iface";
+			status = "disabled";
+		};
+
+		blsp1_uart6: serial@78b4000 {
+			compatible = "qcom,msm-uartdm-v1.4", "qcom,msm-uartdm";
+			reg = <0x0 0x078b4000 0x0 0x200>;
+			interrupts = <GIC_SPI 309 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&gcc GCC_BLSP1_UART6_APPS_CLK>,
+				 <&gcc GCC_BLSP1_AHB_CLK>;
+			clock-names = "core", "iface";
+			status = "disabled";
 		};
 
 		blsp1_spi1: spi@78b5000 {
