From 7d78bab533eb9aa0e5240e25a204e8f416723ed6 Mon Sep 17 00:00:00 2001
From: Daniel Lezcano <daniel.lezcano@linaro.org>
Date: Wed, 1 Mar 2023 21:14:30 +0100
Subject: [PATCH 07/42] thermal/core: Use the thermal zone 'devdata' accessor
 in thermal located drivers
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The thermal zone device structure is exposed to the different drivers
and obviously they access the internals while that should be
restricted to the core thermal code.

In order to self-encapsulate the thermal core code, we need to prevent
the drivers accessing directly the thermal zone structure and provide
accessor functions to deal with.

Use the devdata accessor introduced in the previous patch.

No functional changes intended.

[skipped drivers not relevant for mediatek target]

Signed-off-by: Daniel Lezcano <daniel.lezcano@linaro.org>
Reviewed-by: Niklas Söderlund <niklas.soderlund+renesas@ragnatech.se> #R-Car
Acked-by: Mark Brown <broonie@kernel.org>
Reviewed-by: AngeloGioacchino Del Regno <angelogioacchino.delregno@collabora.com> #MediaTek auxadc and lvts
Reviewed-by: Balsam CHIHI <bchihi@baylibre.com> #Mediatek lvts
Reviewed-by: Adam Ward <DLG-Adam.Ward.opensource@dm.renesas.com> #da9062
Reviewed-by: Baolin Wang <baolin.wang@linux.alibaba.com>  #spread
Acked-by: Jernej Skrabec <jernej.skrabec@gmail.com> #sun8i_thermal
Acked-by: Rafael J. Wysocki <rafael.j.wysocki@intel.com>
Acked-by: Florian Fainelli <f.fainelli@gmail.com> #Broadcom
Reviewed-by: Dhruva Gole <d-gole@ti.com> # K3 bandgap
Acked-by: Linus Walleij <linus.walleij@linaro.org>
Acked-by: Heiko Stuebner <heiko@sntech.de> #rockchip
Reviewed-by: Kunihiko Hayashi <hayashi.kunihiko@socionext.com> #uniphier
Signed-off-by: Rafael J. Wysocki <rafael.j.wysocki@intel.com>
---
 drivers/thermal/mediatek/auxadc_thermal.c           |  2 +-
 drivers/thermal/mediatek/lvts_thermal.c             |  4 ++--
 43 files changed, 71 insertions(+), 73 deletions(-)

--- a/drivers/thermal/mediatek/auxadc_thermal.c
+++ b/drivers/thermal/mediatek/auxadc_thermal.c
@@ -763,7 +763,7 @@ static int mtk_thermal_bank_temperature(
 
 static int mtk_read_temp(struct thermal_zone_device *tz, int *temperature)
 {
-	struct mtk_thermal *mt = tz->devdata;
+	struct mtk_thermal *mt = thermal_zone_device_priv(tz);
 	int i;
 	int tempmax = INT_MIN;
 
--- a/drivers/thermal/mediatek/lvts_thermal.c
+++ b/drivers/thermal/mediatek/lvts_thermal.c
@@ -252,7 +252,7 @@ static u32 lvts_temp_to_raw(int temperat
 
 static int lvts_get_temp(struct thermal_zone_device *tz, int *temp)
 {
-	struct lvts_sensor *lvts_sensor = tz->devdata;
+	struct lvts_sensor *lvts_sensor = thermal_zone_device_priv(tz);
 	void __iomem *msr = lvts_sensor->msr;
 	u32 value;
 
@@ -290,7 +290,7 @@ static int lvts_get_temp(struct thermal_
 
 static int lvts_set_trips(struct thermal_zone_device *tz, int low, int high)
 {
-	struct lvts_sensor *lvts_sensor = tz->devdata;
+	struct lvts_sensor *lvts_sensor = thermal_zone_device_priv(tz);
 	void __iomem *base = lvts_sensor->base;
 	u32 raw_low = lvts_temp_to_raw(low);
 	u32 raw_high = lvts_temp_to_raw(high);
