From: Felix Fietkau <nbd@nbd.name>
Date: Fri, 24 Mar 2023 14:56:58 +0100
Subject: [PATCH] net: ethernet: mtk_eth_soc: fix tx throughput regression with
 direct 1G links

Using the QDMA tx scheduler to throttle tx to line speed works fine for
switch ports, but apparently caused a regression on non-switch ports.

Based on a number of tests, it seems that this throttling can be safely
dropped without re-introducing the issues on switch ports that the
tx scheduling changes resolved.

Link: https://lore.kernel.org/netdev/trinity-92c3826f-c2c8-40af-8339-bc6d0d3ffea4-1678213958520@3c-app-gmx-bs16/
Fixes: f63959c7eec3 ("net: ethernet: mtk_eth_soc: implement multi-queue support for per-port queues")
Reported-by: Frank Wunderlich <frank-w@public-files.de>
Reported-by: Daniel Golle <daniel@makrotopia.org>
Tested-by: Daniel Golle <daniel@makrotopia.org>
Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -719,8 +719,6 @@ static void mtk_mac_link_up(struct phyli
 		break;
 	}
 
-	mtk_set_queue_speed(mac->hw, mac->id, speed);
-
 	/* Configure duplex */
 	if (duplex == DUPLEX_FULL)
 		mcr |= MAC_MCR_FORCE_DPX;
