// SPDX-License-Identifier: GPL-2.0-only OR MIT

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "GL.iNet GL-S1300";
	compatible = "glinet,gl-s1300";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	memory {
		device_type = "memory";
		reg = <0x80000000 0x10000000>;
	};

	soc {
		rng@22000 {
			status = "okay";
		};

		mdio@90000 {
			status = "okay";
		};

		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		tcsr@194b000 {
			/* select hostmode */
			compatible = "qcom,tcsr";
			reg = <0x194b000 0x100>;
			qcom,usb-hsphy-mode-select = <TCSR_USB_HSPHY_HOST_MODE>;
			status = "okay";
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};

		usb2@60f8800 {
			status = "okay";
		};

		usb3@8af8800 {
			status = "okay";
		};

		crypto@8e3a000 {
			status = "okay";
		};

		watchdog@b017000 {
			status = "okay";
		};
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			gpios = <&tlmm 53 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		reset {
			label = "reset";
			gpios = <&tlmm 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&tlmm 57 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};

		mesh {
			label = "green:mesh";
			gpios = <&tlmm 59 GPIO_ACTIVE_HIGH>;
		};

		wlan {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&tlmm 60 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0tpt";
		};
	};
};

&vqmmc {
	status = "okay";
};

&sdhci {
	status = "okay";
	pinctrl-0 = <&sd_pins>;
	pinctrl-names = "default";
	cd-gpios = <&tlmm 22 GPIO_ACTIVE_LOW>;
	vqmmc-supply = <&vqmmc>;
};

&blsp_dma {
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&blsp1_spi1 {
	pinctrl-0 = <&spi_0_pins>;
	pinctrl-names = "default";
	status = "okay";
	cs-gpios = <&tlmm 12 GPIO_ACTIVE_HIGH>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <24000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			SBL1@0 {
				label = "SBL1";
				reg = <0x0 0x40000>;
				read-only;
			};

			MIBIB@40000 {
				label = "MIBIB";
				reg = <0x40000 0x20000>;
				read-only;
			};

			QSEE@60000 {
				label = "QSEE";
				reg = <0x60000 0x60000>;
				read-only;
			};

			CDT@c0000 {
				label = "CDT";
				reg = <0xc0000 0x10000>;
				read-only;
			};

			DDRPARAMS@d0000 {
				label = "DDRPARAMS";
				reg = <0xd0000 0x10000>;
				read-only;
			};

			APPSBLENV@e0000 {
				label = "APPSBLENV";
				reg = <0xe0000 0x10000>;
				read-only;
			};

			APPSBL@f0000 {
				label = "APPSBL";
				reg = <0xf0000 0x80000>;
				read-only;
			};

			ART@170000 {
				label = "ART";
				reg = <0x170000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					precal_art_1000: precal@1000 {
						reg = <0x1000 0x2f20>;
					};

					precal_art_5000: precal@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};

			firmware@180000 {
				compatible = "denx,fit";
				label = "firmware";
				reg = <0x180000 0xe80000>;
			};
		};
	};
};

&blsp1_spi2 {
	pinctrl-0 = <&spi_1_pins>;
	pinctrl-names = "default";
	status = "okay";

	spidev1: spi@0 {
		compatible = "silabs,si3210";
		reg = <0>;
		spi-max-frequency = <24000000>;
	};
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&blsp1_uart2 {
	pinctrl-0 = <&serial_1_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&tlmm {
	serial_pins: serial_pinmux {
		mux {
			pins = "gpio16", "gpio17";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	serial_1_pins: serial1_pinmux {
		mux {
			pins = "gpio8", "gpio9",
				"gpio10", "gpio11";
			function = "blsp_uart1";
			bias-disable;
		};
	};

	spi_0_pins: spi_0_pinmux {
		pinmux {
			function = "blsp_spi0";
			pins = "gpio13", "gpio14", "gpio15";
		};
		pinmux_cs {
			function = "gpio";
			pins = "gpio12";
		};
		pinconf {
			pins = "gpio13", "gpio14", "gpio15";
			drive-strength = <12>;
			bias-disable;
		};
		pinconf_cs {
			pins = "gpio12";
			drive-strength = <2>;
			bias-disable;
			output-high;
		};
	};

	spi_1_pins: spi_1_pinmux {
		mux {
			pins = "gpio44", "gpio46", "gpio47";
			function = "blsp_spi1";
			bias-disable;
		};
		host_int {
			pins = "gpio42";
			function = "gpio";
			input;
		};
		cs {
			pins = "gpio45";
			function = "gpio";
			bias-pull-up;
		};
		wake {
			pins = "gpio40";
			function = "gpio";
			output-high;
		};
		reset {
			pins = "gpio49";
			function = "gpio";
			output-high;
		};
	};

	sd_pins: sd_pins {
		pinmux {
			function = "sdio";
			pins = "gpio23", "gpio24", "gpio25", "gpio26",
				"gpio28", "gpio29", "gpio30", "gpio31";
			drive-strength = <10>;
		};

		pinmux_sd_clk {
			function = "sdio";
			pins = "gpio27";
			drive-strength = <16>;
		};

		pinmux_sd7 {
			function = "sdio";
			pins = "gpio32";
			drive-strength = <10>;
			bias-disable;
		};
	};
};

&usb2_hs_phy {
	status = "okay";
};

&usb3_hs_phy {
	status = "okay";
};

&usb3_ss_phy {
	status = "okay";
};

&wifi0 {
	status = "okay";
	nvmem-cell-names = "pre-calibration";
	nvmem-cells = <&precal_art_1000>;
	qcom,ath10k-calibration-variant = "GL-S1300";
};

&wifi1 {
	status = "okay";
	nvmem-cell-names = "pre-calibration";
	nvmem-cells = <&precal_art_5000>;
	qcom,ath10k-calibration-variant = "GL-S1300";
};
