/* Copyright (c) 2015, The Linux Foundation. All rights reserved.
 *
 * Permission to use, copy, modify, and/or distribute this software for any
 * purpose with or without fee is hereby granted, provided that the above
 * copyright notice and this permission notice appear in all copies.
 *
 * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
 * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
 * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR
 * ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
 * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
 * ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF
 * OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
 *
 */

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "GL.iNet GL-B1300";
	compatible = "glinet,gl-b1300";

	aliases {
		led-boot = &power;
		led-failsafe = &power;
		led-running = &power;
		led-upgrade = &power;
		label-mac-device = &swport4;
	};

	memory {
		device_type = "memory";
		reg = <0x80000000 0x10000000>;
	};

	soc {
		rng@22000 {
			status = "okay";
		};

		mdio@90000 {
			status = "okay";
		};

		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		tcsr@194b000 {
			/* select hostmode */
			compatible = "qcom,tcsr";
			reg = <0x194b000 0x100>;
			qcom,usb-hsphy-mode-select = <TCSR_USB_HSPHY_HOST_MODE>;
			status = "okay";
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};

		usb2@60f8800 {
			status = "okay";
		};

		usb3@8af8800 {
			status = "okay";
		};

		crypto@8e3a000 {
			status = "okay";
		};

		watchdog@b017000 {
			status = "okay";
		};
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			gpios = <&tlmm 5 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		reset {
			label = "reset";
			gpios = <&tlmm 63 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		power: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&tlmm 4 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};

		mesh {
			label = "green:mesh";
			gpios = <&tlmm 3 GPIO_ACTIVE_HIGH>;
		};

		wlan {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&tlmm 2 GPIO_ACTIVE_HIGH>;
		};
	};
};

&blsp_dma {
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&blsp1_spi1 {
	pinctrl-0 = <&spi_0_pins>;
	pinctrl-names = "default";
	status = "okay";
	cs-gpios = <&tlmm 54 GPIO_ACTIVE_HIGH>;

	mx25l25635f@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <24000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			SBL1@0 {
				label = "SBL1";
				reg = <0x0 0x40000>;
				read-only;
			};

			MIBIB@40000 {
				label = "MIBIB";
				reg = <0x40000 0x20000>;
				read-only;
			};

			QSEE@60000 {
				label = "QSEE";
				reg = <0x60000 0x60000>;
				read-only;
			};

			CDT@c0000 {
				label = "CDT";
				reg = <0xc0000 0x10000>;
				read-only;
			};

			DDRPARAMS@d0000 {
				label = "DDRPARAMS";
				reg = <0xd0000 0x10000>;
				read-only;
			};

			APPSBLENV@e0000 {
				label = "APPSBLENV";
				reg = <0xe0000 0x10000>;
				read-only;
			};

			APPSBL@f0000 {
				label = "APPSBL";
				reg = <0xf0000 0x80000>;
				read-only;
			};

			ART@170000 {
				label = "ART";
				reg = <0x170000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_gmac0: macaddr@0 {
						compatible = "mac-base";
						reg = <0x0 0x6>;
						#nvmem-cell-cells = <1>;
					};

					macaddr_gmac1: macaddr@6 {
						reg = <0x6 0x6>;
					};

					precal_art_1000: precal@1000 {
						reg = <0x1000 0x2f20>;
					};

					precal_art_5000: precal@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};

			firmware@180000 {
				compatible = "denx,fit";
				label = "firmware";
				reg = <0x180000 0x1e80000>;
			};
		};
	};
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&tlmm {
	serial_pins: serial_pinmux {
		mux {
			pins = "gpio60", "gpio61";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	spi_0_pins: spi_0_pinmux {
		pinmux {
			function = "blsp_spi0";
			pins = "gpio55", "gpio56", "gpio57";
		};
		pinmux_cs {
			function = "gpio";
			pins = "gpio54";
		};
		pinconf {
			pins = "gpio55", "gpio56", "gpio57";
			drive-strength = <12>;
			bias-disable;
		};
		pinconf_cs {
			pins = "gpio54";
			drive-strength = <2>;
			bias-disable;
			output-high;
		};
	};
};

&usb2_hs_phy {
	status = "okay";
};

&usb3_hs_phy {
	status = "okay";
};

&usb3_ss_phy {
	status = "okay";
};

&gmac {
	status = "okay";
};

&switch {
	status = "okay";
};

&swport3 {
	status = "okay";

	label = "lan2";
	nvmem-cell-names = "mac-address";
	nvmem-cells = <&macaddr_gmac0 2>;
};

&swport4 {
	status = "okay";

	label = "lan1";
	nvmem-cell-names = "mac-address";
	nvmem-cells = <&macaddr_gmac0 0>;
};

&swport5 {
	status = "okay";

	nvmem-cell-names = "mac-address";
	nvmem-cells = <&macaddr_gmac1>;
};

&wifi0 {
	status = "okay";
	nvmem-cell-names = "pre-calibration";
	nvmem-cells = <&precal_art_1000>;
	qcom,ath10k-calibration-variant = "GL-B1300";
};

&wifi1 {
	status = "okay";
	nvmem-cell-names = "pre-calibration";
	nvmem-cells = <&precal_art_5000>;
	qcom,ath10k-calibration-variant = "GL-B1300";
};
