From b8afc254b40167fd37b4d4263e750dab1f9ef157 Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Wed, 9 Sep 2020 18:38:31 +0200
Subject: [PATCH] ARM: dts: qcom: ipq4019: add USB devicetree nodes

Since we now have driver for the USB PHY, and USB controller is already supported by the DWC3 driver lets add the necessary nodes to DTSI.

Signed-off-by: John Crispin <john@phrozen.org>
Signed-off-by: Robert Marko <robert.marko@sartura.hr>
Cc: Luka Perkov <luka.perkov@sartura.hr>
Reviewed-by: Vinod Koul <vkoul@kernel.org>
Link: https://lore.kernel.org/r/20200909163831.1894142-1-robert.marko@sartura.hr
Signed-off-by: Bjorn Andersson <bjorn.andersson@linaro.org>
---
 arch/arm/boot/dts/qcom-ipq4019.dtsi | 74 +++++++++++++++++++++++++++++
 1 file changed, 74 insertions(+)

--- a/arch/arm/boot/dts/qcom-ipq4019.dtsi
+++ b/arch/arm/boot/dts/qcom-ipq4019.dtsi
@@ -605,5 +605,79 @@
 				reg = <4>;
 			};
 		};
+
+		usb3_ss_phy: ssphy@9a000 {
+			compatible = "qcom,usb-ss-ipq4019-phy";
+			#phy-cells = <0>;
+			reg = <0x9a000 0x800>;
+			reg-names = "phy_base";
+			resets = <&gcc USB3_UNIPHY_PHY_ARES>;
+			reset-names = "por_rst";
+			status = "disabled";
+		};
+
+		usb3_hs_phy: hsphy@a6000 {
+			compatible = "qcom,usb-hs-ipq4019-phy";
+			#phy-cells = <0>;
+			reg = <0xa6000 0x40>;
+			reg-names = "phy_base";
+			resets = <&gcc USB3_HSPHY_POR_ARES>, <&gcc USB3_HSPHY_S_ARES>;
+			reset-names = "por_rst", "srif_rst";
+			status = "disabled";
+		};
+
+		usb3: usb3@8af8800 {
+			compatible = "qcom,dwc3";
+			reg = <0x8af8800 0x100>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			clocks = <&gcc GCC_USB3_MASTER_CLK>,
+				 <&gcc GCC_USB3_SLEEP_CLK>,
+				 <&gcc GCC_USB3_MOCK_UTMI_CLK>;
+			clock-names = "master", "sleep", "mock_utmi";
+			ranges;
+			status = "disabled";
+
+			dwc3@8a00000 {
+				compatible = "snps,dwc3";
+				reg = <0x8a00000 0xf8000>;
+				interrupts = <GIC_SPI 132 IRQ_TYPE_LEVEL_HIGH>;
+				phys = <&usb3_hs_phy>, <&usb3_ss_phy>;
+				phy-names = "usb2-phy", "usb3-phy";
+				dr_mode = "host";
+			};
+		};
+
+		usb2_hs_phy: hsphy@a8000 {
+			compatible = "qcom,usb-hs-ipq4019-phy";
+			#phy-cells = <0>;
+			reg = <0xa8000 0x40>;
+			reg-names = "phy_base";
+			resets = <&gcc USB2_HSPHY_POR_ARES>, <&gcc USB2_HSPHY_S_ARES>;
+			reset-names = "por_rst", "srif_rst";
+			status = "disabled";
+		};
+
+		usb2: usb2@60f8800 {
+			compatible = "qcom,dwc3";
+			reg = <0x60f8800 0x100>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			clocks = <&gcc GCC_USB2_MASTER_CLK>,
+				 <&gcc GCC_USB2_SLEEP_CLK>,
+				 <&gcc GCC_USB2_MOCK_UTMI_CLK>;
+			clock-names = "master", "sleep", "mock_utmi";
+			ranges;
+			status = "disabled";
+
+			dwc3@6000000 {
+				compatible = "snps,dwc3";
+				reg = <0x6000000 0xf8000>;
+				interrupts = <GIC_SPI 136 IRQ_TYPE_LEVEL_HIGH>;
+				phys = <&usb2_hs_phy>;
+				phy-names = "usb2-phy";
+				dr_mode = "host";
+			};
+		};
 	};
 };
