// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7620a.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	aliases {
		label-mac-device = &ethernet;
		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power_green: power_green {
			label = "green:power";
			gpios = <&gpio0 9 GPIO_ACTIVE_HIGH>;
		};

		wan_orange {
			label = "orange:wan";
			gpios = <&gpio0 12 GPIO_ACTIVE_HIGH>;
		};

		wan_green {
			label = "green:wan";
			gpios = <&gpio2 0 GPIO_ACTIVE_LOW>;
		};

		power_orange {
			label = "orange:power";
			gpios = <&gpio0 13 GPIO_ACTIVE_HIGH>;
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			factory5g: partition@50000 {
				label = "factory5g";
				reg = <0x50000 0x10000>;
				read-only;
			};

			partition@60000 {
				label = "Wolf_Config";
				reg = <0x60000 0x10000>;
				read-only;
			};

			partition@70000 {
				label = "MyDlink";
				reg = <0x70000 0x80000>;
				read-only;
			};

			partition@f0000 {
				label = "Jffs2";
				reg = <0xf0000 0x80000>;
				read-only;
			};

			partition@170000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x170000 0x690000>;
			};
		};
	};
};

&state_default {
	gpio {
		groups = "i2c", "uartf", "ephy";
		function = "gpio";
	};
};

&ethernet {
	nvmem-cells = <&macaddr_factory_28>;
	nvmem-cell-names = "mac-address";

	mediatek,portmap = "llllw";
};

&gpio2 {
	status = "okay";
};

&wmac {
	pinctrl-names = "default";
	pinctrl-0 = <&pa_pins>;

	ralink,mtd-eeprom = <&factory 0x0>;
	nvmem-cells = <&macaddr_factory_28>;
	nvmem-cell-names = "mac-address";
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		ieee80211-freq-limit = <5000000 6000000>;
		nvmem-cells = <&macaddr_factory_28>;
		nvmem-cell-names = "mac-address";
		mac-address-increment = <2>;
	};
};

&factory {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_factory_28: macaddr@28 {
		reg = <0x28 0x6>;
	};
};
