From 75a5646c26895c4cfadc8d54aa53ac5455947895 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Thu, 19 Aug 2021 08:57:01 +0200
Subject: [PATCH] ARM: dts: BCM5301X: Fix MDIO mux binding
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This fixes following error for all BCM5301X dts files:
mdio-bus-mux@18003000: compatible: ['mdio-mux-mmioreg'] is too short

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm5301x.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/bcm5301x.dtsi
+++ b/arch/arm/boot/dts/bcm5301x.dtsi
@@ -370,7 +370,7 @@
 	};
 
 	mdio-mux@18003000 {
-		compatible = "mdio-mux-mmioreg";
+		compatible = "mdio-mux-mmioreg", "mdio-mux";
 		mdio-parent-bus = <&mdio>;
 		#address-cells = <1>;
 		#size-cells = <0>;
