From ab6a07d577dbd45d00a1738a6b5a28a6666be754 Mon Sep 17 00:00:00 2001
From: Hou Zhiqiang <Zhiqiang.Hou@nxp.com>
Date: Tue, 25 Jun 2019 09:09:07 +0000
Subject: [PATCH] PCI: mobiveil: Refactor Mobiveil PCIe Host Bridge IP driver

Refactor the Mobiveil PCIe Host Bridge IP driver to make
it easier to add support for both RC and EP mode driver.
This patch moved the Mobiveil driver to an new directory
'drivers/pci/controller/mobiveil' and refactor it according
to the RC and EP abstraction.

Signed-off-by: Hou Zhiqiang <Zhiqiang.Hou@nxp.com>
Reviewed-by: Minghuan Lian <Minghuan.Lian@nxp.com>
Reviewed-by: Subrahmanya Lingappa <l.subrahmanya@mobiveil.co.in>
---
 MAINTAINERS                                        |   2 +-
 drivers/pci/controller/Kconfig                     |  11 +-
 drivers/pci/controller/Makefile                    |   2 +-
 drivers/pci/controller/mobiveil/Kconfig            |  24 +
 drivers/pci/controller/mobiveil/Makefile           |   4 +
 .../pci/controller/mobiveil/pcie-mobiveil-host.c   | 611 +++++++++++++
 .../pci/controller/mobiveil/pcie-mobiveil-plat.c   |  59 ++
 drivers/pci/controller/mobiveil/pcie-mobiveil.c    | 227 +++++
 drivers/pci/controller/mobiveil/pcie-mobiveil.h    | 189 ++++
 drivers/pci/controller/pcie-mobiveil.c             | 964 ---------------------
 10 files changed, 1117 insertions(+), 976 deletions(-)
 create mode 100644 drivers/pci/controller/mobiveil/Kconfig
 create mode 100644 drivers/pci/controller/mobiveil/Makefile
 create mode 100644 drivers/pci/controller/mobiveil/pcie-mobiveil-host.c
 create mode 100644 drivers/pci/controller/mobiveil/pcie-mobiveil-plat.c
 create mode 100644 drivers/pci/controller/mobiveil/pcie-mobiveil.c
 create mode 100644 drivers/pci/controller/mobiveil/pcie-mobiveil.h
 delete mode 100644 drivers/pci/controller/pcie-mobiveil.c

--- a/MAINTAINERS
+++ b/MAINTAINERS
@@ -12504,7 +12504,7 @@ M:	Hou Zhiqiang <Zhiqiang.Hou@nxp.com>
 L:	linux-pci@vger.kernel.org
 S:	Supported
 F:	Documentation/devicetree/bindings/pci/mobiveil-pcie.txt
-F:	drivers/pci/controller/pcie-mobiveil.c
+F:	drivers/pci/controller/mobiveil/pcie-mobiveil*
 
 PCI DRIVER FOR MVEBU (Marvell Armada 370 and Armada XP SOC support)
 M:	Thomas Petazzoni <thomas.petazzoni@bootlin.com>
--- a/drivers/pci/controller/Kconfig
+++ b/drivers/pci/controller/Kconfig
@@ -241,16 +241,6 @@ config PCIE_MEDIATEK
 	  Say Y here if you want to enable PCIe controller support on
 	  MediaTek SoCs.
 
-config PCIE_MOBIVEIL
-	bool "Mobiveil AXI PCIe controller"
-	depends on ARCH_ZYNQMP || COMPILE_TEST
-	depends on OF
-	depends on PCI_MSI_IRQ_DOMAIN
-	help
-	  Say Y here if you want to enable support for the Mobiveil AXI PCIe
-	  Soft IP. It has up to 8 outbound and inbound windows
-	  for address translation and it is a PCIe Gen4 IP.
-
 config PCIE_TANGO_SMP8759
 	bool "Tango SMP8759 PCIe controller (DANGEROUS)"
 	depends on ARCH_TANGO && PCI_MSI && OF
@@ -289,4 +279,5 @@ config PCI_HYPERV_INTERFACE
 	  have a common interface with the Hyper-V PCI frontend driver.
 
 source "drivers/pci/controller/dwc/Kconfig"
+source "drivers/pci/controller/mobiveil/Kconfig"
 endmenu
--- a/drivers/pci/controller/Makefile
+++ b/drivers/pci/controller/Makefile
@@ -27,11 +27,11 @@ obj-$(CONFIG_PCIE_ROCKCHIP) += pcie-rock
 obj-$(CONFIG_PCIE_ROCKCHIP_EP) += pcie-rockchip-ep.o
 obj-$(CONFIG_PCIE_ROCKCHIP_HOST) += pcie-rockchip-host.o
 obj-$(CONFIG_PCIE_MEDIATEK) += pcie-mediatek.o
-obj-$(CONFIG_PCIE_MOBIVEIL) += pcie-mobiveil.o
 obj-$(CONFIG_PCIE_TANGO_SMP8759) += pcie-tango.o
 obj-$(CONFIG_VMD) += vmd.o
 # pcie-hisi.o quirks are needed even without CONFIG_PCIE_DW
 obj-y				+= dwc/
+obj-y				+= mobiveil/
 
 
 # The following drivers are for devices that use the generic ACPI
--- /dev/null
+++ b/drivers/pci/controller/mobiveil/Kconfig
@@ -0,0 +1,24 @@
+# SPDX-License-Identifier: GPL-2.0
+
+menu "Mobiveil PCIe Core Support"
+	depends on PCI
+
+config PCIE_MOBIVEIL
+	bool
+
+config PCIE_MOBIVEIL_HOST
+        bool
+	depends on PCI_MSI_IRQ_DOMAIN
+        select PCIE_MOBIVEIL
+
+config PCIE_MOBIVEIL_PLAT
+	bool "Mobiveil AXI PCIe controller"
+	depends on ARCH_ZYNQMP || COMPILE_TEST
+	depends on OF
+	select PCIE_MOBIVEIL_HOST
+	help
+	  Say Y here if you want to enable support for the Mobiveil AXI PCIe
+	  Soft IP. It has up to 8 outbound and inbound windows
+	  for address translation and it is a PCIe Gen4 IP.
+
+endmenu
--- /dev/null
+++ b/drivers/pci/controller/mobiveil/Makefile
@@ -0,0 +1,4 @@
+# SPDX-License-Identifier: GPL-2.0
+obj-$(CONFIG_PCIE_MOBIVEIL) += pcie-mobiveil.o
+obj-$(CONFIG_PCIE_MOBIVEIL_HOST) += pcie-mobiveil-host.o
+obj-$(CONFIG_PCIE_MOBIVEIL_PLAT) += pcie-mobiveil-plat.o
--- /dev/null
+++ b/drivers/pci/controller/mobiveil/pcie-mobiveil-host.c
@@ -0,0 +1,611 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * PCIe host controller driver for Mobiveil PCIe Host controller
+ *
+ * Copyright (c) 2018 Mobiveil Inc.
+ * Copyright 2019 NXP
+ *
+ * Author: Subrahmanya Lingappa <l.subrahmanya@mobiveil.co.in>
+ * Refactor: Zhiqiang Hou <Zhiqiang.Hou@nxp.com>
+ */
+
+#include <linux/init.h>
+#include <linux/interrupt.h>
+#include <linux/irq.h>
+#include <linux/irqchip/chained_irq.h>
+#include <linux/irqdomain.h>
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/msi.h>
+#include <linux/of_address.h>
+#include <linux/of_irq.h>
+#include <linux/of_platform.h>
+#include <linux/of_pci.h>
+#include <linux/pci.h>
+#include <linux/platform_device.h>
+#include <linux/slab.h>
+
+#include "pcie-mobiveil.h"
+
+static bool mobiveil_pcie_valid_device(struct pci_bus *bus, unsigned int devfn)
+{
+	struct mobiveil_pcie *pcie = bus->sysdata;
+
+	/* Only one device down on each root port */
+	if ((bus->number == pcie->rp.root_bus_nr) && (devfn > 0))
+		return false;
+
+	/*
+	 * Do not read more than one device on the bus directly
+	 * attached to RC
+	 */
+	if ((bus->primary == pcie->rp.root_bus_nr) && (PCI_SLOT(devfn) > 0))
+		return false;
+
+	return true;
+}
+
+/*
+ * mobiveil_pcie_map_bus - routine to get the configuration base of either
+ * root port or endpoint
+ */
+static void __iomem *mobiveil_pcie_map_bus(struct pci_bus *bus,
+					   unsigned int devfn, int where)
+{
+	struct mobiveil_pcie *pcie = bus->sysdata;
+	u32 value;
+
+	if (!mobiveil_pcie_valid_device(bus, devfn))
+		return NULL;
+
+	/* RC config access */
+	if (bus->number == pcie->rp.root_bus_nr)
+		return pcie->csr_axi_slave_base + where;
+
+	/*
+	 * EP config access (in Config/APIO space)
+	 * Program PEX Address base (31..16 bits) with appropriate value
+	 * (BDF) in PAB_AXI_AMAP_PEX_WIN_L0 Register.
+	 * Relies on pci_lock serialization
+	 */
+	value = bus->number << PAB_BUS_SHIFT |
+		PCI_SLOT(devfn) << PAB_DEVICE_SHIFT |
+		PCI_FUNC(devfn) << PAB_FUNCTION_SHIFT;
+
+	csr_writel(pcie, value, PAB_AXI_AMAP_PEX_WIN_L(WIN_NUM_0));
+
+	return pcie->rp.config_axi_slave_base + where;
+}
+
+static struct pci_ops mobiveil_pcie_ops = {
+	.map_bus = mobiveil_pcie_map_bus,
+	.read = pci_generic_config_read,
+	.write = pci_generic_config_write,
+};
+
+static void mobiveil_pcie_isr(struct irq_desc *desc)
+{
+	struct irq_chip *chip = irq_desc_get_chip(desc);
+	struct mobiveil_pcie *pcie = irq_desc_get_handler_data(desc);
+	struct device *dev = &pcie->pdev->dev;
+	struct mobiveil_msi *msi = &pcie->rp.msi;
+	u32 msi_data, msi_addr_lo, msi_addr_hi;
+	u32 intr_status, msi_status;
+	unsigned long shifted_status;
+	u32 bit, virq, val, mask;
+
+	/*
+	 * The core provides a single interrupt for both INTx/MSI messages.
+	 * So we'll read both INTx and MSI status
+	 */
+
+	chained_irq_enter(chip, desc);
+
+	/* read INTx status */
+	val = csr_readl(pcie, PAB_INTP_AMBA_MISC_STAT);
+	mask = csr_readl(pcie, PAB_INTP_AMBA_MISC_ENB);
+	intr_status = val & mask;
+
+	/* Handle INTx */
+	if (intr_status & PAB_INTP_INTX_MASK) {
+		shifted_status = csr_readl(pcie, PAB_INTP_AMBA_MISC_STAT);
+		shifted_status &= PAB_INTP_INTX_MASK;
+		shifted_status >>= PAB_INTX_START;
+		do {
+			for_each_set_bit(bit, &shifted_status, PCI_NUM_INTX) {
+				virq = irq_find_mapping(pcie->rp.intx_domain,
+							bit + 1);
+				if (virq)
+					generic_handle_irq(virq);
+				else
+					dev_err_ratelimited(dev, "unexpected IRQ, INT%d\n",
+							    bit);
+
+				/* clear interrupt handled */
+				csr_writel(pcie, 1 << (PAB_INTX_START + bit),
+					   PAB_INTP_AMBA_MISC_STAT);
+			}
+
+			shifted_status = csr_readl(pcie,
+						   PAB_INTP_AMBA_MISC_STAT);
+			shifted_status &= PAB_INTP_INTX_MASK;
+			shifted_status >>= PAB_INTX_START;
+		} while (shifted_status != 0);
+	}
+
+	/* read extra MSI status register */
+	msi_status = readl_relaxed(pcie->apb_csr_base + MSI_STATUS_OFFSET);
+
+	/* handle MSI interrupts */
+	while (msi_status & 1) {
+		msi_data = readl_relaxed(pcie->apb_csr_base + MSI_DATA_OFFSET);
+
+		/*
+		 * MSI_STATUS_OFFSET register gets updated to zero
+		 * once we pop not only the MSI data but also address
+		 * from MSI hardware FIFO. So keeping these following
+		 * two dummy reads.
+		 */
+		msi_addr_lo = readl_relaxed(pcie->apb_csr_base +
+					    MSI_ADDR_L_OFFSET);
+		msi_addr_hi = readl_relaxed(pcie->apb_csr_base +
+					    MSI_ADDR_H_OFFSET);
+		dev_dbg(dev, "MSI registers, data: %08x, addr: %08x:%08x\n",
+			msi_data, msi_addr_hi, msi_addr_lo);
+
+		virq = irq_find_mapping(msi->dev_domain, msi_data);
+		if (virq)
+			generic_handle_irq(virq);
+
+		msi_status = readl_relaxed(pcie->apb_csr_base +
+					   MSI_STATUS_OFFSET);
+	}
+
+	/* Clear the interrupt status */
+	csr_writel(pcie, intr_status, PAB_INTP_AMBA_MISC_STAT);
+	chained_irq_exit(chip, desc);
+}
+
+static int mobiveil_pcie_parse_dt(struct mobiveil_pcie *pcie)
+{
+	struct device *dev = &pcie->pdev->dev;
+	struct platform_device *pdev = pcie->pdev;
+	struct device_node *node = dev->of_node;
+	struct resource *res;
+
+	/* map config resource */
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM,
+					   "config_axi_slave");
+	pcie->rp.config_axi_slave_base = devm_pci_remap_cfg_resource(dev, res);
+	if (IS_ERR(pcie->rp.config_axi_slave_base))
+		return PTR_ERR(pcie->rp.config_axi_slave_base);
+	pcie->rp.ob_io_res = res;
+
+	/* map csr resource */
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM,
+					   "csr_axi_slave");
+	pcie->csr_axi_slave_base = devm_pci_remap_cfg_resource(dev, res);
+	if (IS_ERR(pcie->csr_axi_slave_base))
+		return PTR_ERR(pcie->csr_axi_slave_base);
+	pcie->pcie_reg_base = res->start;
+
+	/* read the number of windows requested */
+	if (of_property_read_u32(node, "apio-wins", &pcie->apio_wins))
+		pcie->apio_wins = MAX_PIO_WINDOWS;
+
+	if (of_property_read_u32(node, "ppio-wins", &pcie->ppio_wins))
+		pcie->ppio_wins = MAX_PIO_WINDOWS;
+
+	return 0;
+}
+
+static void mobiveil_pcie_enable_msi(struct mobiveil_pcie *pcie)
+{
+	phys_addr_t msg_addr = pcie->pcie_reg_base;
+	struct mobiveil_msi *msi = &pcie->rp.msi;
+
+	msi->num_of_vectors = PCI_NUM_MSI;
+	msi->msi_pages_phys = (phys_addr_t)msg_addr;
+
+	writel_relaxed(lower_32_bits(msg_addr),
+		       pcie->apb_csr_base + MSI_BASE_LO_OFFSET);
+	writel_relaxed(upper_32_bits(msg_addr),
+		       pcie->apb_csr_base + MSI_BASE_HI_OFFSET);
+	writel_relaxed(4096, pcie->apb_csr_base + MSI_SIZE_OFFSET);
+	writel_relaxed(1, pcie->apb_csr_base + MSI_ENABLE_OFFSET);
+}
+
+static int mobiveil_host_init(struct mobiveil_pcie *pcie)
+{
+	u32 value, pab_ctrl, type;
+	struct resource_entry *win;
+
+	/* setup bus numbers */
+	value = csr_readl(pcie, PCI_PRIMARY_BUS);
+	value &= 0xff000000;
+	value |= 0x00ff0100;
+	csr_writel(pcie, value, PCI_PRIMARY_BUS);
+
+	/*
+	 * program Bus Master Enable Bit in Command Register in PAB Config
+	 * Space
+	 */
+	value = csr_readl(pcie, PCI_COMMAND);
+	value |= PCI_COMMAND_IO | PCI_COMMAND_MEMORY | PCI_COMMAND_MASTER;
+	csr_writel(pcie, value, PCI_COMMAND);
+
+	/*
+	 * program PIO Enable Bit to 1 (and PEX PIO Enable to 1) in PAB_CTRL
+	 * register
+	 */
+	pab_ctrl = csr_readl(pcie, PAB_CTRL);
+	pab_ctrl |= (1 << AMBA_PIO_ENABLE_SHIFT) | (1 << PEX_PIO_ENABLE_SHIFT);
+	csr_writel(pcie, pab_ctrl, PAB_CTRL);
+
+	/*
+	 * program PIO Enable Bit to 1 and Config Window Enable Bit to 1 in
+	 * PAB_AXI_PIO_CTRL Register
+	 */
+	value = csr_readl(pcie, PAB_AXI_PIO_CTRL);
+	value |= APIO_EN_MASK;
+	csr_writel(pcie, value, PAB_AXI_PIO_CTRL);
+
+	/* Enable PCIe PIO master */
+	value = csr_readl(pcie, PAB_PEX_PIO_CTRL);
+	value |= 1 << PIO_ENABLE_SHIFT;
+	csr_writel(pcie, value, PAB_PEX_PIO_CTRL);
+
+	/*
+	 * we'll program one outbound window for config reads and
+	 * another default inbound window for all the upstream traffic
+	 * rest of the outbound windows will be configured according to
+	 * the "ranges" field defined in device tree
+	 */
+
+	/* config outbound translation window */
+	program_ob_windows(pcie, WIN_NUM_0, pcie->rp.ob_io_res->start, 0,
+			   CFG_WINDOW_TYPE, resource_size(pcie->rp.ob_io_res));
+
+	/* memory inbound translation window */
+	program_ib_windows(pcie, WIN_NUM_0, 0, 0, MEM_WINDOW_TYPE, IB_WIN_SIZE);
+
+	/* Get the I/O and memory ranges from DT */
+	resource_list_for_each_entry(win, &pcie->resources) {
+		if (resource_type(win->res) == IORESOURCE_MEM) {
+			type = MEM_WINDOW_TYPE;
+		} else if (resource_type(win->res) == IORESOURCE_IO) {
+			type = IO_WINDOW_TYPE;
+		} else if (resource_type(win->res) == IORESOURCE_BUS) {
+			pcie->rp.root_bus_nr = win->res->start;
+			continue;
+		} else {
+			continue;
+		}
+
+		/* configure outbound translation window */
+		program_ob_windows(pcie, pcie->ob_wins_configured,
+				   win->res->start,
+				   win->res->start - win->offset,
+				   type, resource_size(win->res));
+	}
+
+	/* fixup for PCIe class register */
+	value = csr_readl(pcie, PAB_INTP_AXI_PIO_CLASS);
+	value &= 0xff;
+	value |= (PCI_CLASS_BRIDGE_PCI << 16);
+	csr_writel(pcie, value, PAB_INTP_AXI_PIO_CLASS);
+
+	return 0;
+}
+
+static void mobiveil_mask_intx_irq(struct irq_data *data)
+{
+	struct irq_desc *desc = irq_to_desc(data->irq);
+	struct mobiveil_pcie *pcie;
+	unsigned long flags;
+	u32 mask, shifted_val;
+
+	pcie = irq_desc_get_chip_data(desc);
+	mask = 1 << ((data->hwirq + PAB_INTX_START) - 1);
+	raw_spin_lock_irqsave(&pcie->rp.intx_mask_lock, flags);
+	shifted_val = csr_readl(pcie, PAB_INTP_AMBA_MISC_ENB);
+	shifted_val &= ~mask;
+	csr_writel(pcie, shifted_val, PAB_INTP_AMBA_MISC_ENB);
+	raw_spin_unlock_irqrestore(&pcie->rp.intx_mask_lock, flags);
+}
+
+static void mobiveil_unmask_intx_irq(struct irq_data *data)
+{
+	struct irq_desc *desc = irq_to_desc(data->irq);
+	struct mobiveil_pcie *pcie;
+	unsigned long flags;
+	u32 shifted_val, mask;
+
+	pcie = irq_desc_get_chip_data(desc);
+	mask = 1 << ((data->hwirq + PAB_INTX_START) - 1);
+	raw_spin_lock_irqsave(&pcie->rp.intx_mask_lock, flags);
+	shifted_val = csr_readl(pcie, PAB_INTP_AMBA_MISC_ENB);
+	shifted_val |= mask;
+	csr_writel(pcie, shifted_val, PAB_INTP_AMBA_MISC_ENB);
+	raw_spin_unlock_irqrestore(&pcie->rp.intx_mask_lock, flags);
+}
+
+static struct irq_chip intx_irq_chip = {
+	.name = "mobiveil_pcie:intx",
+	.irq_enable = mobiveil_unmask_intx_irq,
+	.irq_disable = mobiveil_mask_intx_irq,
+	.irq_mask = mobiveil_mask_intx_irq,
+	.irq_unmask = mobiveil_unmask_intx_irq,
+};
+
+/* routine to setup the INTx related data */
+static int mobiveil_pcie_intx_map(struct irq_domain *domain, unsigned int irq,
+				  irq_hw_number_t hwirq)
+{
+	irq_set_chip_and_handler(irq, &intx_irq_chip, handle_level_irq);
+	irq_set_chip_data(irq, domain->host_data);
+
+	return 0;
+}
+
+/* INTx domain operations structure */
+static const struct irq_domain_ops intx_domain_ops = {
+	.map = mobiveil_pcie_intx_map,
+};
+
+static struct irq_chip mobiveil_msi_irq_chip = {
+	.name = "Mobiveil PCIe MSI",
+	.irq_mask = pci_msi_mask_irq,
+	.irq_unmask = pci_msi_unmask_irq,
+};
+
+static struct msi_domain_info mobiveil_msi_domain_info = {
+	.flags	= (MSI_FLAG_USE_DEF_DOM_OPS | MSI_FLAG_USE_DEF_CHIP_OPS |
+		   MSI_FLAG_PCI_MSIX),
+	.chip	= &mobiveil_msi_irq_chip,
+};
+
+static void mobiveil_compose_msi_msg(struct irq_data *data, struct msi_msg *msg)
+{
+	struct mobiveil_pcie *pcie = irq_data_get_irq_chip_data(data);
+	phys_addr_t addr = pcie->pcie_reg_base + (data->hwirq * sizeof(int));
+
+	msg->address_lo = lower_32_bits(addr);
+	msg->address_hi = upper_32_bits(addr);
+	msg->data = data->hwirq;
+
+	dev_dbg(&pcie->pdev->dev, "msi#%d address_hi %#x address_lo %#x\n",
+		(int)data->hwirq, msg->address_hi, msg->address_lo);
+}
+
+static int mobiveil_msi_set_affinity(struct irq_data *irq_data,
+				     const struct cpumask *mask, bool force)
+{
+	return -EINVAL;
+}
+
+static struct irq_chip mobiveil_msi_bottom_irq_chip = {
+	.name			= "Mobiveil MSI",
+	.irq_compose_msi_msg	= mobiveil_compose_msi_msg,
+	.irq_set_affinity	= mobiveil_msi_set_affinity,
+};
+
+static int mobiveil_irq_msi_domain_alloc(struct irq_domain *domain,
+					 unsigned int virq,
+					 unsigned int nr_irqs, void *args)
+{
+	struct mobiveil_pcie *pcie = domain->host_data;
+	struct mobiveil_msi *msi = &pcie->rp.msi;
+	unsigned long bit;
+
+	WARN_ON(nr_irqs != 1);
+	mutex_lock(&msi->lock);
+
+	bit = find_first_zero_bit(msi->msi_irq_in_use, msi->num_of_vectors);
+	if (bit >= msi->num_of_vectors) {
+		mutex_unlock(&msi->lock);
+		return -ENOSPC;
+	}
+
+	set_bit(bit, msi->msi_irq_in_use);
+
+	mutex_unlock(&msi->lock);
+
+	irq_domain_set_info(domain, virq, bit, &mobiveil_msi_bottom_irq_chip,
+			    domain->host_data, handle_level_irq, NULL, NULL);
+	return 0;
+}
+
+static void mobiveil_irq_msi_domain_free(struct irq_domain *domain,
+					 unsigned int virq,
+					 unsigned int nr_irqs)
+{
+	struct irq_data *d = irq_domain_get_irq_data(domain, virq);
+	struct mobiveil_pcie *pcie = irq_data_get_irq_chip_data(d);
+	struct mobiveil_msi *msi = &pcie->rp.msi;
+
+	mutex_lock(&msi->lock);
+
+	if (!test_bit(d->hwirq, msi->msi_irq_in_use))
+		dev_err(&pcie->pdev->dev, "trying to free unused MSI#%lu\n",
+			d->hwirq);
+	else
+		__clear_bit(d->hwirq, msi->msi_irq_in_use);
+
+	mutex_unlock(&msi->lock);
+}
+static const struct irq_domain_ops msi_domain_ops = {
+	.alloc	= mobiveil_irq_msi_domain_alloc,
+	.free	= mobiveil_irq_msi_domain_free,
+};
+
+static int mobiveil_allocate_msi_domains(struct mobiveil_pcie *pcie)
+{
+	struct device *dev = &pcie->pdev->dev;
+	struct fwnode_handle *fwnode = of_node_to_fwnode(dev->of_node);
+	struct mobiveil_msi *msi = &pcie->rp.msi;
+
+	mutex_init(&msi->lock);
+	msi->dev_domain = irq_domain_add_linear(NULL, msi->num_of_vectors,
+						&msi_domain_ops, pcie);
+	if (!msi->dev_domain) {
+		dev_err(dev, "failed to create IRQ domain\n");
+		return -ENOMEM;
+	}
+
+	msi->msi_domain = pci_msi_create_irq_domain(fwnode,
+						    &mobiveil_msi_domain_info,
+						    msi->dev_domain);
+	if (!msi->msi_domain) {
+		dev_err(dev, "failed to create MSI domain\n");
+		irq_domain_remove(msi->dev_domain);
+		return -ENOMEM;
+	}
+
+	return 0;
+}
+
+static int mobiveil_pcie_init_irq_domain(struct mobiveil_pcie *pcie)
+{
+	struct device *dev = &pcie->pdev->dev;
+	struct device_node *node = dev->of_node;
+	int ret;
+
+	/* setup INTx */
+	pcie->rp.intx_domain = irq_domain_add_linear(node, PCI_NUM_INTX,
+						     &intx_domain_ops, pcie);
+
+	if (!pcie->rp.intx_domain) {
+		dev_err(dev, "Failed to get a INTx IRQ domain\n");
+		return -ENOMEM;
+	}
+
+	raw_spin_lock_init(&pcie->rp.intx_mask_lock);
+
+	/* setup MSI */
+	ret = mobiveil_allocate_msi_domains(pcie);
+	if (ret)
+		return ret;
+
+	return 0;
+}
+
+static int mobiveil_pcie_interrupt_init(struct mobiveil_pcie *pcie)
+{
+	struct device *dev = &pcie->pdev->dev;
+	struct resource *res;
+	int ret;
+
+	if (pcie->rp.ops->interrupt_init)
+		return pcie->rp.ops->interrupt_init(pcie);
+
+	/* map MSI config resource */
+	res = platform_get_resource_byname(pcie->pdev, IORESOURCE_MEM,
+					   "apb_csr");
+	pcie->apb_csr_base = devm_pci_remap_cfg_resource(dev, res);
+	if (IS_ERR(pcie->apb_csr_base))
+		return PTR_ERR(pcie->apb_csr_base);
+
+	/* setup MSI hardware registers */
+	mobiveil_pcie_enable_msi(pcie);
+
+	pcie->rp.irq = platform_get_irq(pcie->pdev, 0);
+	if (pcie->rp.irq <= 0) {
+		dev_err(dev, "failed to map IRQ: %d\n", pcie->rp.irq);
+		return -ENODEV;
+	}
+
+	/* initialize the IRQ domains */
+	ret = mobiveil_pcie_init_irq_domain(pcie);
+	if (ret) {
+		dev_err(dev, "Failed creating IRQ Domain\n");
+		return ret;
+	}
+
+	irq_set_chained_handler_and_data(pcie->rp.irq,
+					 mobiveil_pcie_isr, pcie);
+
+	/* Enable interrupts */
+	csr_writel(pcie, (PAB_INTP_INTX_MASK | PAB_INTP_MSI_MASK),
+		   PAB_INTP_AMBA_MISC_ENB);
+
+	return 0;
+}
+
+int mobiveil_pcie_host_probe(struct mobiveil_pcie *pcie)
+{
+	struct pci_bus *bus;
+	struct pci_bus *child;
+	struct pci_host_bridge *bridge = pcie->bridge;
+	struct device *dev = &pcie->pdev->dev;
+	resource_size_t iobase;
+	int ret;
+
+	INIT_LIST_HEAD(&pcie->resources);
+
+	ret = mobiveil_pcie_parse_dt(pcie);
+	if (ret) {
+		dev_err(dev, "Parsing DT failed, ret: %x\n", ret);
+		return ret;
+	}
+
+	/* parse the host bridge base addresses from the device tree file */
+	ret = devm_of_pci_get_host_bridge_resources(dev, 0, 0xff,
+						    &pcie->resources, &iobase);
+	if (ret) {
+		dev_err(dev, "Getting bridge resources failed\n");
+		return ret;
+	}
+
+	/*
+	 * configure all inbound and outbound windows and prepare the RC for
+	 * config access
+	 */
+	ret = mobiveil_host_init(pcie);
+	if (ret) {
+		dev_err(dev, "Failed to initialize host\n");
+		goto error;
+	}
+
+	ret = mobiveil_pcie_interrupt_init(pcie);
+	if (ret) {
+		dev_err(dev, "Interrupt init failed\n");
+		goto error;
+	}
+
+	ret = devm_request_pci_bus_resources(dev, &pcie->resources);
+	if (ret)
+		goto error;
+
+	/* Initialize bridge */
+	list_splice_init(&pcie->resources, &bridge->windows);
+	bridge->dev.parent = dev;
+	bridge->sysdata = pcie;
+	bridge->busnr = pcie->rp.root_bus_nr;
+	bridge->ops = &mobiveil_pcie_ops;
+	bridge->map_irq = of_irq_parse_and_map_pci;
+	bridge->swizzle_irq = pci_common_swizzle;
+
+	ret = mobiveil_bringup_link(pcie);
+	if (ret) {
+		dev_info(dev, "link bring-up failed\n");
+		goto error;
+	}
+
+	/* setup the kernel resources for the newly added PCIe root bus */
+	ret = pci_scan_root_bus_bridge(bridge);
+	if (ret)
+		goto error;
+
+	bus = bridge->bus;
+
+	pci_assign_unassigned_bus_resources(bus);
+	list_for_each_entry(child, &bus->children, node)
+		pcie_bus_configure_settings(child);
+	pci_bus_add_devices(bus);
+
+	return 0;
+error:
+	pci_free_resource_list(&pcie->resources);
+	return ret;
+}
--- /dev/null
+++ b/drivers/pci/controller/mobiveil/pcie-mobiveil-plat.c
@@ -0,0 +1,59 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * PCIe host controller driver for Mobiveil PCIe Host controller
+ *
+ * Copyright (c) 2018 Mobiveil Inc.
+ * Copyright 2019 NXP
+ *
+ * Author: Subrahmanya Lingappa <l.subrahmanya@mobiveil.co.in>
+ * Refactor: Zhiqiang Hou <Zhiqiang.Hou@nxp.com>
+ */
+
+#include <linux/init.h>
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/of_pci.h>
+#include <linux/pci.h>
+#include <linux/platform_device.h>
+#include <linux/slab.h>
+
+#include "pcie-mobiveil.h"
+
+static int mobiveil_pcie_probe(struct platform_device *pdev)
+{
+	struct mobiveil_pcie *pcie;
+	struct pci_host_bridge *bridge;
+	struct device *dev = &pdev->dev;
+
+	bridge = devm_pci_alloc_host_bridge(dev, sizeof(*pcie));
+	if (!bridge)
+		return -ENOMEM;
+
+	pcie = pci_host_bridge_priv(bridge);
+
+	pcie->pdev = pdev;
+
+	return mobiveil_pcie_host_probe(pcie);
+}
+
+static const struct of_device_id mobiveil_pcie_of_match[] = {
+	{.compatible = "mbvl,gpex40-pcie",},
+	{},
+};
+
+MODULE_DEVICE_TABLE(of, mobiveil_pcie_of_match);
+
+static struct platform_driver mobiveil_pcie_driver = {
+	.probe = mobiveil_pcie_probe,
+	.driver = {
+		.name = "mobiveil-pcie",
+		.of_match_table = mobiveil_pcie_of_match,
+		.suppress_bind_attrs = true,
+	},
+};
+
+builtin_platform_driver(mobiveil_pcie_driver);
+
+MODULE_LICENSE("GPL v2");
+MODULE_DESCRIPTION("Mobiveil PCIe host controller driver");
+MODULE_AUTHOR("Subrahmanya Lingappa <l.subrahmanya@mobiveil.co.in>");
--- /dev/null
+++ b/drivers/pci/controller/mobiveil/pcie-mobiveil.c
@@ -0,0 +1,227 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * PCIe host controller driver for Mobiveil PCIe Host controller
+ *
+ * Copyright (c) 2018 Mobiveil Inc.
+ * Copyright 2019 NXP
+ *
+ * Author: Subrahmanya Lingappa <l.subrahmanya@mobiveil.co.in>
+ * Refactor: Zhiqiang Hou <Zhiqiang.Hou@nxp.com>
+ */
+
+#include <linux/delay.h>
+#include <linux/init.h>
+#include <linux/kernel.h>
+#include <linux/pci.h>
+#include <linux/platform_device.h>
+
+#include "pcie-mobiveil.h"
+
+/*
+ * mobiveil_pcie_sel_page - routine to access paged register
+ *
+ * Registers whose address greater than PAGED_ADDR_BNDRY (0xc00) are paged,
+ * for this scheme to work extracted higher 6 bits of the offset will be
+ * written to pg_sel field of PAB_CTRL register and rest of the lower 10
+ * bits enabled with PAGED_ADDR_BNDRY are used as offset of the register.
+ */
+static void mobiveil_pcie_sel_page(struct mobiveil_pcie *pcie, u8 pg_idx)
+{
+	u32 val;
+
+	val = readl(pcie->csr_axi_slave_base + PAB_CTRL);
+	val &= ~(PAGE_SEL_MASK << PAGE_SEL_SHIFT);
+	val |= (pg_idx & PAGE_SEL_MASK) << PAGE_SEL_SHIFT;
+
+	writel(val, pcie->csr_axi_slave_base + PAB_CTRL);
+}
+
+static void *mobiveil_pcie_comp_addr(struct mobiveil_pcie *pcie, u32 off)
+{
+	if (off < PAGED_ADDR_BNDRY) {
+		/* For directly accessed registers, clear the pg_sel field */
+		mobiveil_pcie_sel_page(pcie, 0);
+		return pcie->csr_axi_slave_base + off;
+	}
+
+	mobiveil_pcie_sel_page(pcie, OFFSET_TO_PAGE_IDX(off));
+	return pcie->csr_axi_slave_base + OFFSET_TO_PAGE_ADDR(off);
+}
+
+static int mobiveil_pcie_read(void __iomem *addr, int size, u32 *val)
+{
+	if ((uintptr_t)addr & (size - 1)) {
+		*val = 0;
+		return PCIBIOS_BAD_REGISTER_NUMBER;
+	}
+
+	switch (size) {
+	case 4:
+		*val = readl(addr);
+		break;
+	case 2:
+		*val = readw(addr);
+		break;
+	case 1:
+		*val = readb(addr);
+		break;
+	default:
+		*val = 0;
+		return PCIBIOS_BAD_REGISTER_NUMBER;
+	}
+
+	return PCIBIOS_SUCCESSFUL;
+}
+
+static int mobiveil_pcie_write(void __iomem *addr, int size, u32 val)
+{
+	if ((uintptr_t)addr & (size - 1))
+		return PCIBIOS_BAD_REGISTER_NUMBER;
+
+	switch (size) {
+	case 4:
+		writel(val, addr);
+		break;
+	case 2:
+		writew(val, addr);
+		break;
+	case 1:
+		writeb(val, addr);
+		break;
+	default:
+		return PCIBIOS_BAD_REGISTER_NUMBER;
+	}
+
+	return PCIBIOS_SUCCESSFUL;
+}
+
+u32 csr_read(struct mobiveil_pcie *pcie, u32 off, size_t size)
+{
+	void *addr;
+	u32 val;
+	int ret;
+
+	addr = mobiveil_pcie_comp_addr(pcie, off);
+
+	ret = mobiveil_pcie_read(addr, size, &val);
+	if (ret)
+		dev_err(&pcie->pdev->dev, "read CSR address failed\n");
+
+	return val;
+}
+
+void csr_write(struct mobiveil_pcie *pcie, u32 val, u32 off, size_t size)
+{
+	void *addr;
+	int ret;
+
+	addr = mobiveil_pcie_comp_addr(pcie, off);
+
+	ret = mobiveil_pcie_write(addr, size, val);
+	if (ret)
+		dev_err(&pcie->pdev->dev, "write CSR address failed\n");
+}
+
+bool mobiveil_pcie_link_up(struct mobiveil_pcie *pcie)
+{
+	if (pcie->ops->link_up)
+		return pcie->ops->link_up(pcie);
+
+	return (csr_readl(pcie, LTSSM_STATUS) &
+		LTSSM_STATUS_L0_MASK) == LTSSM_STATUS_L0;
+}
+
+void program_ib_windows(struct mobiveil_pcie *pcie, int win_num, u64 cpu_addr,
+			u64 pci_addr, u32 type, u64 size)
+{
+	u32 value;
+	u64 size64 = ~(size - 1);
+
+	if (win_num >= pcie->ppio_wins) {
+		dev_err(&pcie->pdev->dev,
+			"ERROR: max inbound windows reached !\n");
+		return;
+	}
+
+	value = csr_readl(pcie, PAB_PEX_AMAP_CTRL(win_num));
+	value &= ~(AMAP_CTRL_TYPE_MASK << AMAP_CTRL_TYPE_SHIFT | WIN_SIZE_MASK);
+	value |= type << AMAP_CTRL_TYPE_SHIFT | 1 << AMAP_CTRL_EN_SHIFT |
+		 (lower_32_bits(size64) & WIN_SIZE_MASK);
+	csr_writel(pcie, value, PAB_PEX_AMAP_CTRL(win_num));
+
+	csr_writel(pcie, upper_32_bits(size64),
+		   PAB_EXT_PEX_AMAP_SIZEN(win_num));
+
+	csr_writel(pcie, lower_32_bits(cpu_addr),
+		   PAB_PEX_AMAP_AXI_WIN(win_num));
+	csr_writel(pcie, upper_32_bits(cpu_addr),
+		   PAB_EXT_PEX_AMAP_AXI_WIN(win_num));
+
+	csr_writel(pcie, lower_32_bits(pci_addr),
+		   PAB_PEX_AMAP_PEX_WIN_L(win_num));
+	csr_writel(pcie, upper_32_bits(pci_addr),
+		   PAB_PEX_AMAP_PEX_WIN_H(win_num));
+
+	pcie->ib_wins_configured++;
+}
+
+/*
+ * routine to program the outbound windows
+ */
+void program_ob_windows(struct mobiveil_pcie *pcie, int win_num, u64 cpu_addr,
+			u64 pci_addr, u32 type, u64 size)
+{
+	u32 value;
+	u64 size64 = ~(size - 1);
+
+	if (win_num >= pcie->apio_wins) {
+		dev_err(&pcie->pdev->dev,
+			"ERROR: max outbound windows reached !\n");
+		return;
+	}
+
+	/*
+	 * program Enable Bit to 1, Type Bit to (00) base 2, AXI Window Size Bit
+	 * to 4 KB in PAB_AXI_AMAP_CTRL register
+	 */
+	value = csr_readl(pcie, PAB_AXI_AMAP_CTRL(win_num));
+	value &= ~(WIN_TYPE_MASK << WIN_TYPE_SHIFT | WIN_SIZE_MASK);
+	value |= 1 << WIN_ENABLE_SHIFT | type << WIN_TYPE_SHIFT |
+		 (lower_32_bits(size64) & WIN_SIZE_MASK);
+	csr_writel(pcie, value, PAB_AXI_AMAP_CTRL(win_num));
+
+	csr_writel(pcie, upper_32_bits(size64), PAB_EXT_AXI_AMAP_SIZE(win_num));
+
+	/*
+	 * program AXI window base with appropriate value in
+	 * PAB_AXI_AMAP_AXI_WIN0 register
+	 */
+	csr_writel(pcie, lower_32_bits(cpu_addr) & (~AXI_WINDOW_ALIGN_MASK),
+		   PAB_AXI_AMAP_AXI_WIN(win_num));
+	csr_writel(pcie, upper_32_bits(cpu_addr),
+		   PAB_EXT_AXI_AMAP_AXI_WIN(win_num));
+
+	csr_writel(pcie, lower_32_bits(pci_addr),
+		   PAB_AXI_AMAP_PEX_WIN_L(win_num));
+	csr_writel(pcie, upper_32_bits(pci_addr),
+		   PAB_AXI_AMAP_PEX_WIN_H(win_num));
+
+	pcie->ob_wins_configured++;
+}
+
+int mobiveil_bringup_link(struct mobiveil_pcie *pcie)
+{
+	int retries;
+
+	/* check if the link is up or not */
+	for (retries = 0; retries < LINK_WAIT_MAX_RETRIES; retries++) {
+		if (mobiveil_pcie_link_up(pcie))
+			return 0;
+
+		usleep_range(LINK_WAIT_MIN, LINK_WAIT_MAX);
+	}
+
+	dev_err(&pcie->pdev->dev, "link never came up\n");
+
+	return -ETIMEDOUT;
+}
--- /dev/null
+++ b/drivers/pci/controller/mobiveil/pcie-mobiveil.h
@@ -0,0 +1,189 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * PCIe host controller driver for Mobiveil PCIe Host controller
+ *
+ * Copyright (c) 2018 Mobiveil Inc.
+ * Copyright 2019 NXP
+ *
+ * Author: Subrahmanya Lingappa <l.subrahmanya@mobiveil.co.in>
+ * Refactor: Zhiqiang Hou <Zhiqiang.Hou@nxp.com>
+ */
+
+#ifndef _PCIE_MOBIVEIL_H
+#define _PCIE_MOBIVEIL_H
+
+#include <linux/pci.h>
+#include <linux/irq.h>
+#include <linux/msi.h>
+#include "../../pci.h"
+
+/* register offsets and bit positions */
+
+/*
+ * translation tables are grouped into windows, each window registers are
+ * grouped into blocks of 4 or 16 registers each
+ */
+#define PAB_REG_BLOCK_SIZE		16
+#define PAB_EXT_REG_BLOCK_SIZE		4
+
+#define PAB_REG_ADDR(offset, win)	\
+	(offset + (win * PAB_REG_BLOCK_SIZE))
+#define PAB_EXT_REG_ADDR(offset, win)	\
+	(offset + (win * PAB_EXT_REG_BLOCK_SIZE))
+
+#define LTSSM_STATUS			0x0404
+#define  LTSSM_STATUS_L0_MASK		0x3f
+#define  LTSSM_STATUS_L0		0x2d
+
+#define PAB_CTRL			0x0808
+#define  AMBA_PIO_ENABLE_SHIFT		0
+#define  PEX_PIO_ENABLE_SHIFT		1
+#define  PAGE_SEL_SHIFT			13
+#define  PAGE_SEL_MASK			0x3f
+#define  PAGE_LO_MASK			0x3ff
+#define  PAGE_SEL_OFFSET_SHIFT		10
+
+#define PAB_AXI_PIO_CTRL		0x0840
+#define  APIO_EN_MASK			0xf
+
+#define PAB_PEX_PIO_CTRL		0x08c0
+#define  PIO_ENABLE_SHIFT		0
+
+#define PAB_INTP_AMBA_MISC_ENB		0x0b0c
+#define PAB_INTP_AMBA_MISC_STAT		0x0b1c
+#define  PAB_INTP_INTX_MASK		0x01e0
+#define  PAB_INTP_MSI_MASK		0x8
+
+#define PAB_AXI_AMAP_CTRL(win)		PAB_REG_ADDR(0x0ba0, win)
+#define  WIN_ENABLE_SHIFT		0
+#define  WIN_TYPE_SHIFT			1
+#define  WIN_TYPE_MASK			0x3
+#define  WIN_SIZE_MASK			0xfffffc00
+
+#define PAB_EXT_AXI_AMAP_SIZE(win)	PAB_EXT_REG_ADDR(0xbaf0, win)
+
+#define PAB_EXT_AXI_AMAP_AXI_WIN(win)	PAB_EXT_REG_ADDR(0x80a0, win)
+#define PAB_AXI_AMAP_AXI_WIN(win)	PAB_REG_ADDR(0x0ba4, win)
+#define  AXI_WINDOW_ALIGN_MASK		3
+
+#define PAB_AXI_AMAP_PEX_WIN_L(win)	PAB_REG_ADDR(0x0ba8, win)
+#define  PAB_BUS_SHIFT			24
+#define  PAB_DEVICE_SHIFT		19
+#define  PAB_FUNCTION_SHIFT		16
+
+#define PAB_AXI_AMAP_PEX_WIN_H(win)	PAB_REG_ADDR(0x0bac, win)
+#define PAB_INTP_AXI_PIO_CLASS		0x474
+
+#define PAB_PEX_AMAP_CTRL(win)		PAB_REG_ADDR(0x4ba0, win)
+#define  AMAP_CTRL_EN_SHIFT		0
+#define  AMAP_CTRL_TYPE_SHIFT		1
+#define  AMAP_CTRL_TYPE_MASK		3
+
+#define PAB_EXT_PEX_AMAP_SIZEN(win)	PAB_EXT_REG_ADDR(0xbef0, win)
+#define PAB_EXT_PEX_AMAP_AXI_WIN(win)	PAB_EXT_REG_ADDR(0xb4a0, win)
+#define PAB_PEX_AMAP_AXI_WIN(win)	PAB_REG_ADDR(0x4ba4, win)
+#define PAB_PEX_AMAP_PEX_WIN_L(win)	PAB_REG_ADDR(0x4ba8, win)
+#define PAB_PEX_AMAP_PEX_WIN_H(win)	PAB_REG_ADDR(0x4bac, win)
+
+/* starting offset of INTX bits in status register */
+#define PAB_INTX_START			5
+
+/* supported number of MSI interrupts */
+#define PCI_NUM_MSI			16
+
+/* MSI registers */
+#define MSI_BASE_LO_OFFSET		0x04
+#define MSI_BASE_HI_OFFSET		0x08
+#define MSI_SIZE_OFFSET			0x0c
+#define MSI_ENABLE_OFFSET		0x14
+#define MSI_STATUS_OFFSET		0x18
+#define MSI_DATA_OFFSET			0x20
+#define MSI_ADDR_L_OFFSET		0x24
+#define MSI_ADDR_H_OFFSET		0x28
+
+/* outbound and inbound window definitions */
+#define WIN_NUM_0			0
+#define WIN_NUM_1			1
+#define CFG_WINDOW_TYPE			0
+#define IO_WINDOW_TYPE			1
+#define MEM_WINDOW_TYPE			2
+#define IB_WIN_SIZE			((u64)256 * 1024 * 1024 * 1024)
+#define MAX_PIO_WINDOWS			8
+
+/* Parameters for the waiting for link up routine */
+#define LINK_WAIT_MAX_RETRIES		10
+#define LINK_WAIT_MIN			90000
+#define LINK_WAIT_MAX			100000
+
+#define PAGED_ADDR_BNDRY		0xc00
+#define OFFSET_TO_PAGE_ADDR(off)	\
+	((off & PAGE_LO_MASK) | PAGED_ADDR_BNDRY)
+#define OFFSET_TO_PAGE_IDX(off)		\
+	((off >> PAGE_SEL_OFFSET_SHIFT) & PAGE_SEL_MASK)
+
+struct mobiveil_pcie;
+
+struct mobiveil_msi {			/* MSI information */
+	struct mutex lock;		/* protect bitmap variable */
+	struct irq_domain *msi_domain;
+	struct irq_domain *dev_domain;
+	phys_addr_t msi_pages_phys;
+	int num_of_vectors;
+	DECLARE_BITMAP(msi_irq_in_use, PCI_NUM_MSI);
+};
+
+struct mobiveil_rp_ops {
+	int (*interrupt_init)(struct mobiveil_pcie *pcie);
+};
+
+struct root_port {
+	u8 root_bus_nr;
+	void __iomem *config_axi_slave_base;	/* endpoint config base */
+	struct resource *ob_io_res;
+	struct mobiveil_rp_ops *ops;
+	int irq;
+	raw_spinlock_t intx_mask_lock;
+	struct irq_domain *intx_domain;
+	struct mobiveil_msi msi;
+};
+
+struct mobiveil_pab_ops {
+	int (*link_up)(struct mobiveil_pcie *pcie);
+};
+
+struct mobiveil_pcie {
+	struct platform_device *pdev;
+	struct list_head resources;
+	void __iomem *csr_axi_slave_base;	/* PAB registers base */
+	phys_addr_t pcie_reg_base;	/* Physical PCIe Controller Base */
+	void __iomem *apb_csr_base;	/* MSI register base */
+	u32 apio_wins;
+	u32 ppio_wins;
+	u32 ob_wins_configured;		/* configured outbound windows */
+	u32 ib_wins_configured;		/* configured inbound windows */
+	const struct mobiveil_pab_ops *ops;
+	struct root_port rp;
+	struct pci_host_bridge *bridge;
+};
+
+int mobiveil_pcie_host_probe(struct mobiveil_pcie *pcie);
+bool mobiveil_pcie_link_up(struct mobiveil_pcie *pcie);
+int mobiveil_bringup_link(struct mobiveil_pcie *pcie);
+void program_ob_windows(struct mobiveil_pcie *pcie, int win_num, u64 cpu_addr,
+			u64 pci_addr, u32 type, u64 size);
+void program_ib_windows(struct mobiveil_pcie *pcie, int win_num, u64 cpu_addr,
+			u64 pci_addr, u32 type, u64 size);
+u32 csr_read(struct mobiveil_pcie *pcie, u32 off, size_t size);
+void csr_write(struct mobiveil_pcie *pcie, u32 val, u32 off, size_t size);
+
+static inline u32 csr_readl(struct mobiveil_pcie *pcie, u32 off)
+{
+	return csr_read(pcie, off, 0x4);
+}
+
+static inline void csr_writel(struct mobiveil_pcie *pcie, u32 val, u32 off)
+{
+	csr_write(pcie, val, off, 0x4);
+}
+
+#endif /* _PCIE_MOBIVEIL_H */
--- a/drivers/pci/controller/pcie-mobiveil.c
+++ /dev/null
@@ -1,964 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0
-/*
- * PCIe host controller driver for Mobiveil PCIe Host controller
- *
- * Copyright (c) 2018 Mobiveil Inc.
- * Author: Subrahmanya Lingappa <l.subrahmanya@mobiveil.co.in>
- */
-
-#include <linux/delay.h>
-#include <linux/init.h>
-#include <linux/interrupt.h>
-#include <linux/irq.h>
-#include <linux/irqchip/chained_irq.h>
-#include <linux/irqdomain.h>
-#include <linux/kernel.h>
-#include <linux/module.h>
-#include <linux/msi.h>
-#include <linux/of_address.h>
-#include <linux/of_irq.h>
-#include <linux/of_platform.h>
-#include <linux/of_pci.h>
-#include <linux/pci.h>
-#include <linux/platform_device.h>
-#include <linux/slab.h>
-
-#include "../pci.h"
-
-/* register offsets and bit positions */
-
-/*
- * translation tables are grouped into windows, each window registers are
- * grouped into blocks of 4 or 16 registers each
- */
-#define PAB_REG_BLOCK_SIZE		16
-#define PAB_EXT_REG_BLOCK_SIZE		4
-
-#define PAB_REG_ADDR(offset, win)	\
-	(offset + (win * PAB_REG_BLOCK_SIZE))
-#define PAB_EXT_REG_ADDR(offset, win)	\
-	(offset + (win * PAB_EXT_REG_BLOCK_SIZE))
-
-#define LTSSM_STATUS			0x0404
-#define  LTSSM_STATUS_L0_MASK		0x3f
-#define  LTSSM_STATUS_L0		0x2d
-
-#define PAB_CTRL			0x0808
-#define  AMBA_PIO_ENABLE_SHIFT		0
-#define  PEX_PIO_ENABLE_SHIFT		1
-#define  PAGE_SEL_SHIFT			13
-#define  PAGE_SEL_MASK			0x3f
-#define  PAGE_LO_MASK			0x3ff
-#define  PAGE_SEL_OFFSET_SHIFT		10
-
-#define PAB_AXI_PIO_CTRL		0x0840
-#define  APIO_EN_MASK			0xf
-
-#define PAB_PEX_PIO_CTRL		0x08c0
-#define  PIO_ENABLE_SHIFT		0
-
-#define PAB_INTP_AMBA_MISC_ENB		0x0b0c
-#define PAB_INTP_AMBA_MISC_STAT		0x0b1c
-#define  PAB_INTP_INTX_MASK		0x01e0
-#define  PAB_INTP_MSI_MASK		0x8
-
-#define PAB_AXI_AMAP_CTRL(win)		PAB_REG_ADDR(0x0ba0, win)
-#define  WIN_ENABLE_SHIFT		0
-#define  WIN_TYPE_SHIFT			1
-#define  WIN_TYPE_MASK			0x3
-#define  WIN_SIZE_MASK			0xfffffc00
-
-#define PAB_EXT_AXI_AMAP_SIZE(win)	PAB_EXT_REG_ADDR(0xbaf0, win)
-
-#define PAB_EXT_AXI_AMAP_AXI_WIN(win)	PAB_EXT_REG_ADDR(0x80a0, win)
-#define PAB_AXI_AMAP_AXI_WIN(win)	PAB_REG_ADDR(0x0ba4, win)
-#define  AXI_WINDOW_ALIGN_MASK		3
-
-#define PAB_AXI_AMAP_PEX_WIN_L(win)	PAB_REG_ADDR(0x0ba8, win)
-#define  PAB_BUS_SHIFT			24
-#define  PAB_DEVICE_SHIFT		19
-#define  PAB_FUNCTION_SHIFT		16
-
-#define PAB_AXI_AMAP_PEX_WIN_H(win)	PAB_REG_ADDR(0x0bac, win)
-#define PAB_INTP_AXI_PIO_CLASS		0x474
-
-#define PAB_PEX_AMAP_CTRL(win)		PAB_REG_ADDR(0x4ba0, win)
-#define  AMAP_CTRL_EN_SHIFT		0
-#define  AMAP_CTRL_TYPE_SHIFT		1
-#define  AMAP_CTRL_TYPE_MASK		3
-
-#define PAB_EXT_PEX_AMAP_SIZEN(win)	PAB_EXT_REG_ADDR(0xbef0, win)
-#define PAB_EXT_PEX_AMAP_AXI_WIN(win)	PAB_EXT_REG_ADDR(0xb4a0, win)
-#define PAB_PEX_AMAP_AXI_WIN(win)	PAB_REG_ADDR(0x4ba4, win)
-#define PAB_PEX_AMAP_PEX_WIN_L(win)	PAB_REG_ADDR(0x4ba8, win)
-#define PAB_PEX_AMAP_PEX_WIN_H(win)	PAB_REG_ADDR(0x4bac, win)
-
-/* starting offset of INTX bits in status register */
-#define PAB_INTX_START			5
-
-/* supported number of MSI interrupts */
-#define PCI_NUM_MSI			16
-
-/* MSI registers */
-#define MSI_BASE_LO_OFFSET		0x04
-#define MSI_BASE_HI_OFFSET		0x08
-#define MSI_SIZE_OFFSET			0x0c
-#define MSI_ENABLE_OFFSET		0x14
-#define MSI_STATUS_OFFSET		0x18
-#define MSI_DATA_OFFSET			0x20
-#define MSI_ADDR_L_OFFSET		0x24
-#define MSI_ADDR_H_OFFSET		0x28
-
-/* outbound and inbound window definitions */
-#define WIN_NUM_0			0
-#define WIN_NUM_1			1
-#define CFG_WINDOW_TYPE			0
-#define IO_WINDOW_TYPE			1
-#define MEM_WINDOW_TYPE			2
-#define IB_WIN_SIZE			((u64)256 * 1024 * 1024 * 1024)
-#define MAX_PIO_WINDOWS			8
-
-/* Parameters for the waiting for link up routine */
-#define LINK_WAIT_MAX_RETRIES		10
-#define LINK_WAIT_MIN			90000
-#define LINK_WAIT_MAX			100000
-
-#define PAGED_ADDR_BNDRY		0xc00
-#define OFFSET_TO_PAGE_ADDR(off)	\
-	((off & PAGE_LO_MASK) | PAGED_ADDR_BNDRY)
-#define OFFSET_TO_PAGE_IDX(off)		\
-	((off >> PAGE_SEL_OFFSET_SHIFT) & PAGE_SEL_MASK)
-
-struct mobiveil_msi {			/* MSI information */
-	struct mutex lock;		/* protect bitmap variable */
-	struct irq_domain *msi_domain;
-	struct irq_domain *dev_domain;
-	phys_addr_t msi_pages_phys;
-	int num_of_vectors;
-	DECLARE_BITMAP(msi_irq_in_use, PCI_NUM_MSI);
-};
-
-struct mobiveil_pcie {
-	struct platform_device *pdev;
-	struct list_head resources;
-	void __iomem *config_axi_slave_base;	/* endpoint config base */
-	void __iomem *csr_axi_slave_base;	/* root port config base */
-	void __iomem *apb_csr_base;	/* MSI register base */
-	phys_addr_t pcie_reg_base;	/* Physical PCIe Controller Base */
-	struct irq_domain *intx_domain;
-	raw_spinlock_t intx_mask_lock;
-	int irq;
-	int apio_wins;
-	int ppio_wins;
-	int ob_wins_configured;		/* configured outbound windows */
-	int ib_wins_configured;		/* configured inbound windows */
-	struct resource *ob_io_res;
-	char root_bus_nr;
-	struct mobiveil_msi msi;
-};
-
-/*
- * mobiveil_pcie_sel_page - routine to access paged register
- *
- * Registers whose address greater than PAGED_ADDR_BNDRY (0xc00) are paged,
- * for this scheme to work extracted higher 6 bits of the offset will be
- * written to pg_sel field of PAB_CTRL register and rest of the lower 10
- * bits enabled with PAGED_ADDR_BNDRY are used as offset of the register.
- */
-static void mobiveil_pcie_sel_page(struct mobiveil_pcie *pcie, u8 pg_idx)
-{
-	u32 val;
-
-	val = readl(pcie->csr_axi_slave_base + PAB_CTRL);
-	val &= ~(PAGE_SEL_MASK << PAGE_SEL_SHIFT);
-	val |= (pg_idx & PAGE_SEL_MASK) << PAGE_SEL_SHIFT;
-
-	writel(val, pcie->csr_axi_slave_base + PAB_CTRL);
-}
-
-static void *mobiveil_pcie_comp_addr(struct mobiveil_pcie *pcie, u32 off)
-{
-	if (off < PAGED_ADDR_BNDRY) {
-		/* For directly accessed registers, clear the pg_sel field */
-		mobiveil_pcie_sel_page(pcie, 0);
-		return pcie->csr_axi_slave_base + off;
-	}
-
-	mobiveil_pcie_sel_page(pcie, OFFSET_TO_PAGE_IDX(off));
-	return pcie->csr_axi_slave_base + OFFSET_TO_PAGE_ADDR(off);
-}
-
-static int mobiveil_pcie_read(void __iomem *addr, int size, u32 *val)
-{
-	if ((uintptr_t)addr & (size - 1)) {
-		*val = 0;
-		return PCIBIOS_BAD_REGISTER_NUMBER;
-	}
-
-	switch (size) {
-	case 4:
-		*val = readl(addr);
-		break;
-	case 2:
-		*val = readw(addr);
-		break;
-	case 1:
-		*val = readb(addr);
-		break;
-	default:
-		*val = 0;
-		return PCIBIOS_BAD_REGISTER_NUMBER;
-	}
-
-	return PCIBIOS_SUCCESSFUL;
-}
-
-static int mobiveil_pcie_write(void __iomem *addr, int size, u32 val)
-{
-	if ((uintptr_t)addr & (size - 1))
-		return PCIBIOS_BAD_REGISTER_NUMBER;
-
-	switch (size) {
-	case 4:
-		writel(val, addr);
-		break;
-	case 2:
-		writew(val, addr);
-		break;
-	case 1:
-		writeb(val, addr);
-		break;
-	default:
-		return PCIBIOS_BAD_REGISTER_NUMBER;
-	}
-
-	return PCIBIOS_SUCCESSFUL;
-}
-
-static u32 csr_read(struct mobiveil_pcie *pcie, u32 off, size_t size)
-{
-	void *addr;
-	u32 val;
-	int ret;
-
-	addr = mobiveil_pcie_comp_addr(pcie, off);
-
-	ret = mobiveil_pcie_read(addr, size, &val);
-	if (ret)
-		dev_err(&pcie->pdev->dev, "read CSR address failed\n");
-
-	return val;
-}
-
-static void csr_write(struct mobiveil_pcie *pcie, u32 val, u32 off, size_t size)
-{
-	void *addr;
-	int ret;
-
-	addr = mobiveil_pcie_comp_addr(pcie, off);
-
-	ret = mobiveil_pcie_write(addr, size, val);
-	if (ret)
-		dev_err(&pcie->pdev->dev, "write CSR address failed\n");
-}
-
-static u32 csr_readl(struct mobiveil_pcie *pcie, u32 off)
-{
-	return csr_read(pcie, off, 0x4);
-}
-
-static void csr_writel(struct mobiveil_pcie *pcie, u32 val, u32 off)
-{
-	csr_write(pcie, val, off, 0x4);
-}
-
-static bool mobiveil_pcie_link_up(struct mobiveil_pcie *pcie)
-{
-	return (csr_readl(pcie, LTSSM_STATUS) &
-		LTSSM_STATUS_L0_MASK) == LTSSM_STATUS_L0;
-}
-
-static bool mobiveil_pcie_valid_device(struct pci_bus *bus, unsigned int devfn)
-{
-	struct mobiveil_pcie *pcie = bus->sysdata;
-
-	/* Only one device down on each root port */
-	if ((bus->number == pcie->root_bus_nr) && (devfn > 0))
-		return false;
-
-	/*
-	 * Do not read more than one device on the bus directly
-	 * attached to RC
-	 */
-	if ((bus->primary == pcie->root_bus_nr) && (PCI_SLOT(devfn) > 0))
-		return false;
-
-	return true;
-}
-
-/*
- * mobiveil_pcie_map_bus - routine to get the configuration base of either
- * root port or endpoint
- */
-static void __iomem *mobiveil_pcie_map_bus(struct pci_bus *bus,
-					   unsigned int devfn, int where)
-{
-	struct mobiveil_pcie *pcie = bus->sysdata;
-	u32 value;
-
-	if (!mobiveil_pcie_valid_device(bus, devfn))
-		return NULL;
-
-	/* RC config access */
-	if (bus->number == pcie->root_bus_nr)
-		return pcie->csr_axi_slave_base + where;
-
-	/*
-	 * EP config access (in Config/APIO space)
-	 * Program PEX Address base (31..16 bits) with appropriate value
-	 * (BDF) in PAB_AXI_AMAP_PEX_WIN_L0 Register.
-	 * Relies on pci_lock serialization
-	 */
-	value = bus->number << PAB_BUS_SHIFT |
-		PCI_SLOT(devfn) << PAB_DEVICE_SHIFT |
-		PCI_FUNC(devfn) << PAB_FUNCTION_SHIFT;
-
-	csr_writel(pcie, value, PAB_AXI_AMAP_PEX_WIN_L(WIN_NUM_0));
-
-	return pcie->config_axi_slave_base + where;
-}
-
-static struct pci_ops mobiveil_pcie_ops = {
-	.map_bus = mobiveil_pcie_map_bus,
-	.read = pci_generic_config_read,
-	.write = pci_generic_config_write,
-};
-
-static void mobiveil_pcie_isr(struct irq_desc *desc)
-{
-	struct irq_chip *chip = irq_desc_get_chip(desc);
-	struct mobiveil_pcie *pcie = irq_desc_get_handler_data(desc);
-	struct device *dev = &pcie->pdev->dev;
-	struct mobiveil_msi *msi = &pcie->msi;
-	u32 msi_data, msi_addr_lo, msi_addr_hi;
-	u32 intr_status, msi_status;
-	unsigned long shifted_status;
-	u32 bit, virq, val, mask;
-
-	/*
-	 * The core provides a single interrupt for both INTx/MSI messages.
-	 * So we'll read both INTx and MSI status
-	 */
-
-	chained_irq_enter(chip, desc);
-
-	/* read INTx status */
-	val = csr_readl(pcie, PAB_INTP_AMBA_MISC_STAT);
-	mask = csr_readl(pcie, PAB_INTP_AMBA_MISC_ENB);
-	intr_status = val & mask;
-
-	/* Handle INTx */
-	if (intr_status & PAB_INTP_INTX_MASK) {
-		shifted_status = csr_readl(pcie, PAB_INTP_AMBA_MISC_STAT);
-		shifted_status &= PAB_INTP_INTX_MASK;
-		shifted_status >>= PAB_INTX_START;
-		do {
-			for_each_set_bit(bit, &shifted_status, PCI_NUM_INTX) {
-				virq = irq_find_mapping(pcie->intx_domain,
-							bit + 1);
-				if (virq)
-					generic_handle_irq(virq);
-				else
-					dev_err_ratelimited(dev, "unexpected IRQ, INT%d\n",
-							    bit);
-
-				/* clear interrupt handled */
-				csr_writel(pcie, 1 << (PAB_INTX_START + bit),
-					   PAB_INTP_AMBA_MISC_STAT);
-			}
-
-			shifted_status = csr_readl(pcie,
-						   PAB_INTP_AMBA_MISC_STAT);
-			shifted_status &= PAB_INTP_INTX_MASK;
-			shifted_status >>= PAB_INTX_START;
-		} while (shifted_status != 0);
-	}
-
-	/* read extra MSI status register */
-	msi_status = readl_relaxed(pcie->apb_csr_base + MSI_STATUS_OFFSET);
-
-	/* handle MSI interrupts */
-	while (msi_status & 1) {
-		msi_data = readl_relaxed(pcie->apb_csr_base + MSI_DATA_OFFSET);
-
-		/*
-		 * MSI_STATUS_OFFSET register gets updated to zero
-		 * once we pop not only the MSI data but also address
-		 * from MSI hardware FIFO. So keeping these following
-		 * two dummy reads.
-		 */
-		msi_addr_lo = readl_relaxed(pcie->apb_csr_base +
-					    MSI_ADDR_L_OFFSET);
-		msi_addr_hi = readl_relaxed(pcie->apb_csr_base +
-					    MSI_ADDR_H_OFFSET);
-		dev_dbg(dev, "MSI registers, data: %08x, addr: %08x:%08x\n",
-			msi_data, msi_addr_hi, msi_addr_lo);
-
-		virq = irq_find_mapping(msi->dev_domain, msi_data);
-		if (virq)
-			generic_handle_irq(virq);
-
-		msi_status = readl_relaxed(pcie->apb_csr_base +
-					   MSI_STATUS_OFFSET);
-	}
-
-	/* Clear the interrupt status */
-	csr_writel(pcie, intr_status, PAB_INTP_AMBA_MISC_STAT);
-	chained_irq_exit(chip, desc);
-}
-
-static int mobiveil_pcie_parse_dt(struct mobiveil_pcie *pcie)
-{
-	struct device *dev = &pcie->pdev->dev;
-	struct platform_device *pdev = pcie->pdev;
-	struct device_node *node = dev->of_node;
-	struct resource *res;
-
-	/* map config resource */
-	res = platform_get_resource_byname(pdev, IORESOURCE_MEM,
-					   "config_axi_slave");
-	pcie->config_axi_slave_base = devm_pci_remap_cfg_resource(dev, res);
-	if (IS_ERR(pcie->config_axi_slave_base))
-		return PTR_ERR(pcie->config_axi_slave_base);
-	pcie->ob_io_res = res;
-
-	/* map csr resource */
-	res = platform_get_resource_byname(pdev, IORESOURCE_MEM,
-					   "csr_axi_slave");
-	pcie->csr_axi_slave_base = devm_pci_remap_cfg_resource(dev, res);
-	if (IS_ERR(pcie->csr_axi_slave_base))
-		return PTR_ERR(pcie->csr_axi_slave_base);
-	pcie->pcie_reg_base = res->start;
-
-	/* map MSI config resource */
-	res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "apb_csr");
-	pcie->apb_csr_base = devm_pci_remap_cfg_resource(dev, res);
-	if (IS_ERR(pcie->apb_csr_base))
-		return PTR_ERR(pcie->apb_csr_base);
-
-	/* read the number of windows requested */
-	if (of_property_read_u32(node, "apio-wins", &pcie->apio_wins))
-		pcie->apio_wins = MAX_PIO_WINDOWS;
-
-	if (of_property_read_u32(node, "ppio-wins", &pcie->ppio_wins))
-		pcie->ppio_wins = MAX_PIO_WINDOWS;
-
-	pcie->irq = platform_get_irq(pdev, 0);
-	if (pcie->irq <= 0) {
-		dev_err(dev, "failed to map IRQ: %d\n", pcie->irq);
-		return -ENODEV;
-	}
-
-	return 0;
-}
-
-static void program_ib_windows(struct mobiveil_pcie *pcie, int win_num,
-			       u64 cpu_addr, u64 pci_addr, u32 type, u64 size)
-{
-	u32 value;
-	u64 size64 = ~(size - 1);
-
-	if (win_num >= pcie->ppio_wins) {
-		dev_err(&pcie->pdev->dev,
-			"ERROR: max inbound windows reached !\n");
-		return;
-	}
-
-	value = csr_readl(pcie, PAB_PEX_AMAP_CTRL(win_num));
-	value &= ~(AMAP_CTRL_TYPE_MASK << AMAP_CTRL_TYPE_SHIFT | WIN_SIZE_MASK);
-	value |= type << AMAP_CTRL_TYPE_SHIFT | 1 << AMAP_CTRL_EN_SHIFT |
-		 (lower_32_bits(size64) & WIN_SIZE_MASK);
-	csr_writel(pcie, value, PAB_PEX_AMAP_CTRL(win_num));
-
-	csr_writel(pcie, upper_32_bits(size64),
-		   PAB_EXT_PEX_AMAP_SIZEN(win_num));
-
-	csr_writel(pcie, lower_32_bits(cpu_addr),
-		   PAB_PEX_AMAP_AXI_WIN(win_num));
-	csr_writel(pcie, upper_32_bits(cpu_addr),
-		   PAB_EXT_PEX_AMAP_AXI_WIN(win_num));
-
-	csr_writel(pcie, lower_32_bits(pci_addr),
-		   PAB_PEX_AMAP_PEX_WIN_L(win_num));
-	csr_writel(pcie, upper_32_bits(pci_addr),
-		   PAB_PEX_AMAP_PEX_WIN_H(win_num));
-
-	pcie->ib_wins_configured++;
-}
-
-/*
- * routine to program the outbound windows
- */
-static void program_ob_windows(struct mobiveil_pcie *pcie, int win_num,
-			       u64 cpu_addr, u64 pci_addr, u32 type, u64 size)
-{
-	u32 value;
-	u64 size64 = ~(size - 1);
-
-	if (win_num >= pcie->apio_wins) {
-		dev_err(&pcie->pdev->dev,
-			"ERROR: max outbound windows reached !\n");
-		return;
-	}
-
-	/*
-	 * program Enable Bit to 1, Type Bit to (00) base 2, AXI Window Size Bit
-	 * to 4 KB in PAB_AXI_AMAP_CTRL register
-	 */
-	value = csr_readl(pcie, PAB_AXI_AMAP_CTRL(win_num));
-	value &= ~(WIN_TYPE_MASK << WIN_TYPE_SHIFT | WIN_SIZE_MASK);
-	value |= 1 << WIN_ENABLE_SHIFT | type << WIN_TYPE_SHIFT |
-		 (lower_32_bits(size64) & WIN_SIZE_MASK);
-	csr_writel(pcie, value, PAB_AXI_AMAP_CTRL(win_num));
-
-	csr_writel(pcie, upper_32_bits(size64), PAB_EXT_AXI_AMAP_SIZE(win_num));
-
-	/*
-	 * program AXI window base with appropriate value in
-	 * PAB_AXI_AMAP_AXI_WIN0 register
-	 */
-	csr_writel(pcie, lower_32_bits(cpu_addr) & (~AXI_WINDOW_ALIGN_MASK),
-		   PAB_AXI_AMAP_AXI_WIN(win_num));
-	csr_writel(pcie, upper_32_bits(cpu_addr),
-		   PAB_EXT_AXI_AMAP_AXI_WIN(win_num));
-
-	csr_writel(pcie, lower_32_bits(pci_addr),
-		   PAB_AXI_AMAP_PEX_WIN_L(win_num));
-	csr_writel(pcie, upper_32_bits(pci_addr),
-		   PAB_AXI_AMAP_PEX_WIN_H(win_num));
-
-	pcie->ob_wins_configured++;
-}
-
-static int mobiveil_bringup_link(struct mobiveil_pcie *pcie)
-{
-	int retries;
-
-	/* check if the link is up or not */
-	for (retries = 0; retries < LINK_WAIT_MAX_RETRIES; retries++) {
-		if (mobiveil_pcie_link_up(pcie))
-			return 0;
-
-		usleep_range(LINK_WAIT_MIN, LINK_WAIT_MAX);
-	}
-
-	dev_err(&pcie->pdev->dev, "link never came up\n");
-
-	return -ETIMEDOUT;
-}
-
-static void mobiveil_pcie_enable_msi(struct mobiveil_pcie *pcie)
-{
-	phys_addr_t msg_addr = pcie->pcie_reg_base;
-	struct mobiveil_msi *msi = &pcie->msi;
-
-	pcie->msi.num_of_vectors = PCI_NUM_MSI;
-	msi->msi_pages_phys = (phys_addr_t)msg_addr;
-
-	writel_relaxed(lower_32_bits(msg_addr),
-		       pcie->apb_csr_base + MSI_BASE_LO_OFFSET);
-	writel_relaxed(upper_32_bits(msg_addr),
-		       pcie->apb_csr_base + MSI_BASE_HI_OFFSET);
-	writel_relaxed(4096, pcie->apb_csr_base + MSI_SIZE_OFFSET);
-	writel_relaxed(1, pcie->apb_csr_base + MSI_ENABLE_OFFSET);
-}
-
-static int mobiveil_host_init(struct mobiveil_pcie *pcie)
-{
-	u32 value, pab_ctrl, type;
-	struct resource_entry *win;
-
-	/* setup bus numbers */
-	value = csr_readl(pcie, PCI_PRIMARY_BUS);
-	value &= 0xff000000;
-	value |= 0x00ff0100;
-	csr_writel(pcie, value, PCI_PRIMARY_BUS);
-
-	/*
-	 * program Bus Master Enable Bit in Command Register in PAB Config
-	 * Space
-	 */
-	value = csr_readl(pcie, PCI_COMMAND);
-	value |= PCI_COMMAND_IO | PCI_COMMAND_MEMORY | PCI_COMMAND_MASTER;
-	csr_writel(pcie, value, PCI_COMMAND);
-
-	/*
-	 * program PIO Enable Bit to 1 (and PEX PIO Enable to 1) in PAB_CTRL
-	 * register
-	 */
-	pab_ctrl = csr_readl(pcie, PAB_CTRL);
-	pab_ctrl |= (1 << AMBA_PIO_ENABLE_SHIFT) | (1 << PEX_PIO_ENABLE_SHIFT);
-	csr_writel(pcie, pab_ctrl, PAB_CTRL);
-
-	csr_writel(pcie, (PAB_INTP_INTX_MASK | PAB_INTP_MSI_MASK),
-		   PAB_INTP_AMBA_MISC_ENB);
-
-	/*
-	 * program PIO Enable Bit to 1 and Config Window Enable Bit to 1 in
-	 * PAB_AXI_PIO_CTRL Register
-	 */
-	value = csr_readl(pcie, PAB_AXI_PIO_CTRL);
-	value |= APIO_EN_MASK;
-	csr_writel(pcie, value, PAB_AXI_PIO_CTRL);
-
-	/* Enable PCIe PIO master */
-	value = csr_readl(pcie, PAB_PEX_PIO_CTRL);
-	value |= 1 << PIO_ENABLE_SHIFT;
-	csr_writel(pcie, value, PAB_PEX_PIO_CTRL);
-
-	/*
-	 * we'll program one outbound window for config reads and
-	 * another default inbound window for all the upstream traffic
-	 * rest of the outbound windows will be configured according to
-	 * the "ranges" field defined in device tree
-	 */
-
-	/* config outbound translation window */
-	program_ob_windows(pcie, WIN_NUM_0, pcie->ob_io_res->start, 0,
-			   CFG_WINDOW_TYPE, resource_size(pcie->ob_io_res));
-
-	/* memory inbound translation window */
-	program_ib_windows(pcie, WIN_NUM_0, 0, 0, MEM_WINDOW_TYPE, IB_WIN_SIZE);
-
-	/* Get the I/O and memory ranges from DT */
-	resource_list_for_each_entry(win, &pcie->resources) {
-		if (resource_type(win->res) == IORESOURCE_MEM)
-			type = MEM_WINDOW_TYPE;
-		else if (resource_type(win->res) == IORESOURCE_IO)
-			type = IO_WINDOW_TYPE;
-		else
-			continue;
-
-		/* configure outbound translation window */
-		program_ob_windows(pcie, pcie->ob_wins_configured,
-				   win->res->start,
-				   win->res->start - win->offset,
-				   type, resource_size(win->res));
-	}
-
-	/* fixup for PCIe class register */
-	value = csr_readl(pcie, PAB_INTP_AXI_PIO_CLASS);
-	value &= 0xff;
-	value |= (PCI_CLASS_BRIDGE_PCI << 16);
-	csr_writel(pcie, value, PAB_INTP_AXI_PIO_CLASS);
-
-	/* setup MSI hardware registers */
-	mobiveil_pcie_enable_msi(pcie);
-
-	return 0;
-}
-
-static void mobiveil_mask_intx_irq(struct irq_data *data)
-{
-	struct irq_desc *desc = irq_to_desc(data->irq);
-	struct mobiveil_pcie *pcie;
-	unsigned long flags;
-	u32 mask, shifted_val;
-
-	pcie = irq_desc_get_chip_data(desc);
-	mask = 1 << ((data->hwirq + PAB_INTX_START) - 1);
-	raw_spin_lock_irqsave(&pcie->intx_mask_lock, flags);
-	shifted_val = csr_readl(pcie, PAB_INTP_AMBA_MISC_ENB);
-	shifted_val &= ~mask;
-	csr_writel(pcie, shifted_val, PAB_INTP_AMBA_MISC_ENB);
-	raw_spin_unlock_irqrestore(&pcie->intx_mask_lock, flags);
-}
-
-static void mobiveil_unmask_intx_irq(struct irq_data *data)
-{
-	struct irq_desc *desc = irq_to_desc(data->irq);
-	struct mobiveil_pcie *pcie;
-	unsigned long flags;
-	u32 shifted_val, mask;
-
-	pcie = irq_desc_get_chip_data(desc);
-	mask = 1 << ((data->hwirq + PAB_INTX_START) - 1);
-	raw_spin_lock_irqsave(&pcie->intx_mask_lock, flags);
-	shifted_val = csr_readl(pcie, PAB_INTP_AMBA_MISC_ENB);
-	shifted_val |= mask;
-	csr_writel(pcie, shifted_val, PAB_INTP_AMBA_MISC_ENB);
-	raw_spin_unlock_irqrestore(&pcie->intx_mask_lock, flags);
-}
-
-static struct irq_chip intx_irq_chip = {
-	.name = "mobiveil_pcie:intx",
-	.irq_enable = mobiveil_unmask_intx_irq,
-	.irq_disable = mobiveil_mask_intx_irq,
-	.irq_mask = mobiveil_mask_intx_irq,
-	.irq_unmask = mobiveil_unmask_intx_irq,
-};
-
-/* routine to setup the INTx related data */
-static int mobiveil_pcie_intx_map(struct irq_domain *domain, unsigned int irq,
-				  irq_hw_number_t hwirq)
-{
-	irq_set_chip_and_handler(irq, &intx_irq_chip, handle_level_irq);
-	irq_set_chip_data(irq, domain->host_data);
-
-	return 0;
-}
-
-/* INTx domain operations structure */
-static const struct irq_domain_ops intx_domain_ops = {
-	.map = mobiveil_pcie_intx_map,
-};
-
-static struct irq_chip mobiveil_msi_irq_chip = {
-	.name = "Mobiveil PCIe MSI",
-	.irq_mask = pci_msi_mask_irq,
-	.irq_unmask = pci_msi_unmask_irq,
-};
-
-static struct msi_domain_info mobiveil_msi_domain_info = {
-	.flags	= (MSI_FLAG_USE_DEF_DOM_OPS | MSI_FLAG_USE_DEF_CHIP_OPS |
-		   MSI_FLAG_PCI_MSIX),
-	.chip	= &mobiveil_msi_irq_chip,
-};
-
-static void mobiveil_compose_msi_msg(struct irq_data *data, struct msi_msg *msg)
-{
-	struct mobiveil_pcie *pcie = irq_data_get_irq_chip_data(data);
-	phys_addr_t addr = pcie->pcie_reg_base + (data->hwirq * sizeof(int));
-
-	msg->address_lo = lower_32_bits(addr);
-	msg->address_hi = upper_32_bits(addr);
-	msg->data = data->hwirq;
-
-	dev_dbg(&pcie->pdev->dev, "msi#%d address_hi %#x address_lo %#x\n",
-		(int)data->hwirq, msg->address_hi, msg->address_lo);
-}
-
-static int mobiveil_msi_set_affinity(struct irq_data *irq_data,
-				     const struct cpumask *mask, bool force)
-{
-	return -EINVAL;
-}
-
-static struct irq_chip mobiveil_msi_bottom_irq_chip = {
-	.name			= "Mobiveil MSI",
-	.irq_compose_msi_msg	= mobiveil_compose_msi_msg,
-	.irq_set_affinity	= mobiveil_msi_set_affinity,
-};
-
-static int mobiveil_irq_msi_domain_alloc(struct irq_domain *domain,
-					 unsigned int virq,
-					 unsigned int nr_irqs, void *args)
-{
-	struct mobiveil_pcie *pcie = domain->host_data;
-	struct mobiveil_msi *msi = &pcie->msi;
-	unsigned long bit;
-
-	WARN_ON(nr_irqs != 1);
-	mutex_lock(&msi->lock);
-
-	bit = find_first_zero_bit(msi->msi_irq_in_use, msi->num_of_vectors);
-	if (bit >= msi->num_of_vectors) {
-		mutex_unlock(&msi->lock);
-		return -ENOSPC;
-	}
-
-	set_bit(bit, msi->msi_irq_in_use);
-
-	mutex_unlock(&msi->lock);
-
-	irq_domain_set_info(domain, virq, bit, &mobiveil_msi_bottom_irq_chip,
-			    domain->host_data, handle_level_irq, NULL, NULL);
-	return 0;
-}
-
-static void mobiveil_irq_msi_domain_free(struct irq_domain *domain,
-					 unsigned int virq,
-					 unsigned int nr_irqs)
-{
-	struct irq_data *d = irq_domain_get_irq_data(domain, virq);
-	struct mobiveil_pcie *pcie = irq_data_get_irq_chip_data(d);
-	struct mobiveil_msi *msi = &pcie->msi;
-
-	mutex_lock(&msi->lock);
-
-	if (!test_bit(d->hwirq, msi->msi_irq_in_use))
-		dev_err(&pcie->pdev->dev, "trying to free unused MSI#%lu\n",
-			d->hwirq);
-	else
-		__clear_bit(d->hwirq, msi->msi_irq_in_use);
-
-	mutex_unlock(&msi->lock);
-}
-static const struct irq_domain_ops msi_domain_ops = {
-	.alloc	= mobiveil_irq_msi_domain_alloc,
-	.free	= mobiveil_irq_msi_domain_free,
-};
-
-static int mobiveil_allocate_msi_domains(struct mobiveil_pcie *pcie)
-{
-	struct device *dev = &pcie->pdev->dev;
-	struct fwnode_handle *fwnode = of_node_to_fwnode(dev->of_node);
-	struct mobiveil_msi *msi = &pcie->msi;
-
-	mutex_init(&pcie->msi.lock);
-	msi->dev_domain = irq_domain_add_linear(NULL, msi->num_of_vectors,
-						&msi_domain_ops, pcie);
-	if (!msi->dev_domain) {
-		dev_err(dev, "failed to create IRQ domain\n");
-		return -ENOMEM;
-	}
-
-	msi->msi_domain = pci_msi_create_irq_domain(fwnode,
-						    &mobiveil_msi_domain_info,
-						    msi->dev_domain);
-	if (!msi->msi_domain) {
-		dev_err(dev, "failed to create MSI domain\n");
-		irq_domain_remove(msi->dev_domain);
-		return -ENOMEM;
-	}
-
-	return 0;
-}
-
-static int mobiveil_pcie_init_irq_domain(struct mobiveil_pcie *pcie)
-{
-	struct device *dev = &pcie->pdev->dev;
-	struct device_node *node = dev->of_node;
-	int ret;
-
-	/* setup INTx */
-	pcie->intx_domain = irq_domain_add_linear(node, PCI_NUM_INTX,
-						  &intx_domain_ops, pcie);
-
-	if (!pcie->intx_domain) {
-		dev_err(dev, "Failed to get a INTx IRQ domain\n");
-		return -ENOMEM;
-	}
-
-	raw_spin_lock_init(&pcie->intx_mask_lock);
-
-	/* setup MSI */
-	ret = mobiveil_allocate_msi_domains(pcie);
-	if (ret)
-		return ret;
-
-	return 0;
-}
-
-static int mobiveil_pcie_probe(struct platform_device *pdev)
-{
-	struct mobiveil_pcie *pcie;
-	struct pci_bus *bus;
-	struct pci_bus *child;
-	struct pci_host_bridge *bridge;
-	struct device *dev = &pdev->dev;
-	resource_size_t iobase;
-	int ret;
-
-	/* allocate the PCIe port */
-	bridge = devm_pci_alloc_host_bridge(dev, sizeof(*pcie));
-	if (!bridge)
-		return -ENOMEM;
-
-	pcie = pci_host_bridge_priv(bridge);
-
-	pcie->pdev = pdev;
-
-	ret = mobiveil_pcie_parse_dt(pcie);
-	if (ret) {
-		dev_err(dev, "Parsing DT failed, ret: %x\n", ret);
-		return ret;
-	}
-
-	INIT_LIST_HEAD(&pcie->resources);
-
-	/* parse the host bridge base addresses from the device tree file */
-	ret = devm_of_pci_get_host_bridge_resources(dev, 0, 0xff,
-						    &pcie->resources, &iobase);
-	if (ret) {
-		dev_err(dev, "Getting bridge resources failed\n");
-		return ret;
-	}
-
-	/*
-	 * configure all inbound and outbound windows and prepare the RC for
-	 * config access
-	 */
-	ret = mobiveil_host_init(pcie);
-	if (ret) {
-		dev_err(dev, "Failed to initialize host\n");
-		goto error;
-	}
-
-	/* initialize the IRQ domains */
-	ret = mobiveil_pcie_init_irq_domain(pcie);
-	if (ret) {
-		dev_err(dev, "Failed creating IRQ Domain\n");
-		goto error;
-	}
-
-	irq_set_chained_handler_and_data(pcie->irq, mobiveil_pcie_isr, pcie);
-
-	ret = devm_request_pci_bus_resources(dev, &pcie->resources);
-	if (ret)
-		goto error;
-
-	/* Initialize bridge */
-	list_splice_init(&pcie->resources, &bridge->windows);
-	bridge->dev.parent = dev;
-	bridge->sysdata = pcie;
-	bridge->busnr = pcie->root_bus_nr;
-	bridge->ops = &mobiveil_pcie_ops;
-	bridge->map_irq = of_irq_parse_and_map_pci;
-	bridge->swizzle_irq = pci_common_swizzle;
-
-	ret = mobiveil_bringup_link(pcie);
-	if (ret) {
-		dev_info(dev, "link bring-up failed\n");
-		goto error;
-	}
-
-	/* setup the kernel resources for the newly added PCIe root bus */
-	ret = pci_scan_root_bus_bridge(bridge);
-	if (ret)
-		goto error;
-
-	bus = bridge->bus;
-
-	pci_assign_unassigned_bus_resources(bus);
-	list_for_each_entry(child, &bus->children, node)
-		pcie_bus_configure_settings(child);
-	pci_bus_add_devices(bus);
-
-	return 0;
-error:
-	pci_free_resource_list(&pcie->resources);
-	return ret;
-}
-
-static const struct of_device_id mobiveil_pcie_of_match[] = {
-	{.compatible = "mbvl,gpex40-pcie",},
-	{},
-};
-
-MODULE_DEVICE_TABLE(of, mobiveil_pcie_of_match);
-
-static struct platform_driver mobiveil_pcie_driver = {
-	.probe = mobiveil_pcie_probe,
-	.driver = {
-		.name = "mobiveil-pcie",
-		.of_match_table = mobiveil_pcie_of_match,
-		.suppress_bind_attrs = true,
-	},
-};
-
-builtin_platform_driver(mobiveil_pcie_driver);
-
-MODULE_LICENSE("GPL v2");
-MODULE_DESCRIPTION("Mobiveil PCIe host controller driver");
-MODULE_AUTHOR("Subrahmanya Lingappa <l.subrahmanya@mobiveil.co.in>");
