From bb95d7d440fefd104c593d9cb20da6d34a474e97 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Wed, 21 Apr 2021 11:00:06 +0200
Subject: [PATCH] ARM: dts: BCM5301X: Fix pinmux subnodes names
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This matches pinmux-node.yaml requirements.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm47094.dtsi | 2 +-
 arch/arm/boot/dts/bcm5301x.dtsi | 6 +++---
 2 files changed, 4 insertions(+), 4 deletions(-)

--- a/arch/arm/boot/dts/bcm47094.dtsi
+++ b/arch/arm/boot/dts/bcm47094.dtsi
@@ -11,7 +11,7 @@
 &pinctrl {
 	compatible = "brcm,bcm4709-pinmux";
 
-	pinmux_mdio: mdio {
+	pinmux_mdio: mdio-pins {
 		groups = "mdio_grp";
 		function = "mdio";
 	};
--- a/arch/arm/boot/dts/bcm5301x.dtsi
+++ b/arch/arm/boot/dts/bcm5301x.dtsi
@@ -458,18 +458,18 @@
 					function = "spi";
 				};
 
-				pinmux_i2c: i2c {
+				pinmux_i2c: i2c-pins {
 					groups = "i2c_grp";
 					function = "i2c";
 				};
 
-				pinmux_pwm: pwm {
+				pinmux_pwm: pwm-pins {
 					groups = "pwm0_grp", "pwm1_grp",
 						 "pwm2_grp", "pwm3_grp";
 					function = "pwm";
 				};
 
-				pinmux_uart1: uart1 {
+				pinmux_uart1: uart1-pins {
 					groups = "uart1_grp";
 					function = "uart1";
 				};
