#!/bin/sh

[ -e /lib/firmware/$FIRMWARE ] && exit 0

. /lib/functions/caldata.sh

board=$(board_name)

case "$FIRMWARE" in
"ath10k/pre-cal-pci-0000:01:00.0.bin")
	case $board in
	askey,rt4230w-rev6)
		caldata_extract "0:ART" 0x1000 0x2f20
		;;
	asrock,g10)
		caldata_extract "0:art" 0x1000 0x2f20
		;;
	buffalo,wxr-2533dhp |\
	nec,wg2600hp |\
	nec,wg2600hp3 |\
	tplink,vr2600v)
		caldata_extract "ART" 0x1000 0x2f20
		;;
	linksys,ea7500-v1 |\
	linksys,ea8500)
		caldata_extract "art" 0x1000 0x2f20
		ath10k_patch_mac $(macaddr_add $(mtd_get_mac_ascii devinfo hw_mac_addr) 1)
		;;
	netgear,d7800 |\
	netgear,r7500v2 |\
	netgear,r7800 |\
	netgear,xr500)
		caldata_extract "art" 0x1000 0x2f20
		;;
	tplink,ad7200 |\
	tplink,c2600)
		caldata_extract "radio" 0x1000 0x2f20
		;;
	zyxel,nbg6817)
		caldata_extract "0:art" 0x1000 0x2f20
		ath10k_patch_mac $(macaddr_add $(mtd_get_mac_ascii 0:appsblenv ethaddr) 1)
		;;
	esac
	;;
"ath10k/pre-cal-pci-0001:01:00.0.bin")
	case $board in
	askey,rt4230w-rev6)
		caldata_extract "0:ART" 0x5000 0x2f20
		;;
	asrock,g10)
		caldata_extract "0:art" 0x5000 0x2f20
		;;
	buffalo,wxr-2533dhp |\
	nec,wg2600hp |\
	nec,wg2600hp3 |\
	tplink,vr2600v)
		caldata_extract "ART" 0x5000 0x2f20
		;;
	edgecore,ecw5410)
		caldata_extract "0:art" 0x1000 0x2f20
		;;
	linksys,ea7500-v1 |\
	linksys,ea8500)
		caldata_extract "art" 0x5000 0x2f20
		ath10k_patch_mac $(macaddr_add $(mtd_get_mac_ascii devinfo hw_mac_addr) 2)
		;;
	netgear,d7800 |\
	netgear,r7500v2 |\
	netgear,r7800 |\
	netgear,xr500)
		caldata_extract "art" 0x5000 0x2f20
		;;
	tplink,ad7200 |\
	tplink,c2600)
		caldata_extract "radio" 0x5000 0x2f20
		;;
	zyxel,nbg6817)
		caldata_extract "0:art" 0x5000 0x2f20
		ath10k_patch_mac $(mtd_get_mac_ascii 0:appsblenv ethaddr)
		;;
	esac
	;;
"ath10k/pre-cal-pci-0002:01:00.0.bin")
	case $board in
	edgecore,ecw5410)
		caldata_extract "0:art" 0x5000 0x2f20
		;;
	esac
	;;
*)
	exit 1
	;;
esac
