From f95f8ebd8d55ccc27e1615b251450915a1c14315 Mon Sep 17 00:00:00 2001
From: Abhimanyu Saini <abhimanyu.saini@nxp.com>
Date: Tue, 12 Jul 2016 14:17:17 +0530
Subject: [PATCH 74/93] board: freescale: ls1012a: Intergrate and enable PPA
 on LS1012AFRDM

Signed-off-by: Abhimanyu Saini <abhimanyu.saini@nxp.com>
---
 board/freescale/ls1012afrdm/ls1012afrdm.c |    9 +++++++++
 include/configs/ls1012afrdm.h             |   12 ++++++++++++
 2 files changed, 21 insertions(+)

diff --git a/board/freescale/ls1012afrdm/ls1012afrdm.c b/board/freescale/ls1012afrdm/ls1012afrdm.c
index 4b7902a..04f8f9a 100644
--- a/board/freescale/ls1012afrdm/ls1012afrdm.c
+++ b/board/freescale/ls1012afrdm/ls1012afrdm.c
@@ -143,6 +143,9 @@ int board_early_init_f(void)
 int board_init(void)
 {
 	struct ccsr_cci400 *cci = (struct ccsr_cci400 *)CONFIG_SYS_CCI400_ADDR;
+#ifdef CONFIG_FSL_LS_PPA
+	u64 ppa_entry;
+#endif
 	/*
 	 * Set CCI-400 control override register to enable barrier
 	 * transaction
@@ -157,6 +160,12 @@ int board_init(void)
 	enable_layerscape_ns_access();
 #endif
 
+#ifdef CONFIG_FSL_LS_PPA
+	ppa_init_pre(&ppa_entry);
+
+	if (ppa_entry)
+		ppa_init_entry((void *)ppa_entry);
+#endif
 	return 0;
 }
 
diff --git a/include/configs/ls1012afrdm.h b/include/configs/ls1012afrdm.h
index 622c774..26e3640 100644
--- a/include/configs/ls1012afrdm.h
+++ b/include/configs/ls1012afrdm.h
@@ -9,6 +9,18 @@
 
 #include "ls1012a_common.h"
 
+#ifndef CONFIG_SECURE_BOOT
+#define CONFIG_FSL_LS_PPA
+#if defined(CONFIG_FSL_LS_PPA)
+#define CONFIG_SYS_LS_PPA_DRAM_BLOCK_MIN_SIZE	(1UL * 1024 * 1024)
+
+#define CONFIG_SYS_LS_PPA_FW_IN_XIP
+#ifdef CONFIG_SYS_LS_PPA_FW_IN_XIP
+#define CONFIG_SYS_LS_PPA_FW_ADDR	0x40500000
+#endif
+#endif
+#endif
+
 #define CONFIG_DIMM_SLOTS_PER_CTLR	1
 #define CONFIG_CHIP_SELECTS_PER_CTRL	1
 #define CONFIG_NR_DRAM_BANKS		2
-- 
1.7.9.5

