From 7d95f6b52ea5f01c9e2414d4984e5a274328c021 Mon Sep 17 00:00:00 2001
From: Samuel Holland <samuel@sholland.org>
Date: Sun, 7 Aug 2022 10:58:57 -0500
Subject: [PATCH 093/117] riscv: dts: allwinner: d1: Add LVDS0 PHY

Signed-off-by: Samuel Holland <samuel@sholland.org>
---
 arch/riscv/boot/dts/allwinner/sun20i-d1.dtsi | 2 ++
 1 file changed, 2 insertions(+)

--- a/arch/riscv/boot/dts/allwinner/sun20i-d1.dtsi
+++ b/arch/riscv/boot/dts/allwinner/sun20i-d1.dtsi
@@ -1040,6 +1040,8 @@
 			resets = <&ccu RST_BUS_TCON_LCD0>,
 				 <&ccu RST_BUS_LVDS0>;
 			reset-names = "lcd", "lvds";
+			phys = <&dphy>;
+			phy-names = "lvds0";
 			#clock-cells = <0>;
 
 			ports {
