From 1209f487d452ff7e822dec30661fd6b5163fb8cf Mon Sep 17 00:00:00 2001
From: Chun Qiu <cqca@cock.lu>
Date: Mon, 29 Jan 2024 13:30:30 +0800
Subject: [PATCH] wifi: rtl8xxxu: Add TP-Link TL-WN823N V2

TP-Link TL-WN823N V2 (2357:0135) is based on rtl8192fu and has been
tested to work with the rtl8xxxu driver.

Signed-off-by: Chun Qiu <cqca@cock.lu>
Signed-off-by: Kalle Valo <kvalo@kernel.org>
Link: https://msgid.link/20240129053030.16369-1-cqca@cock.lu
---
 drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_core.c | 5 ++++-
 1 file changed, 4 insertions(+), 1 deletion(-)

--- a/drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_core.c
+++ b/drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_core.c
@@ -7733,7 +7733,7 @@ static int rtl8xxxu_probe(struct usb_int
 			untested = 0;
 		break;
 	case 0x2357:
-		if (id->idProduct == 0x0109)
+		if (id->idProduct == 0x0109 || id->idProduct == 0x0135)
 			untested = 0;
 		break;
 	case 0x0b05:
@@ -8025,6 +8025,9 @@ static const struct usb_device_id dev_ta
 	.driver_info = (unsigned long)&rtl8192fu_fops},
 {USB_DEVICE_AND_INTERFACE_INFO(USB_VENDOR_ID_REALTEK, 0x318b, 0xff, 0xff, 0xff),
 	.driver_info = (unsigned long)&rtl8192fu_fops},
+/* TP-Link TL-WN823N V2 */
+{USB_DEVICE_AND_INTERFACE_INFO(0x2357, 0x0135, 0xff, 0xff, 0xff),
+	.driver_info = (unsigned long)&rtl8192fu_fops},
 #ifdef CPTCFG_RTL8XXXU_UNTESTED
 /* Still supported by rtlwifi */
 {USB_DEVICE_AND_INTERFACE_INFO(USB_VENDOR_ID_REALTEK, 0x8176, 0xff, 0xff, 0xff),
