From b076677ea22db8ceb66aa168c82c9c160dc1a9f1 Mon Sep 17 00:00:00 2001
From: Yassine Oudjana <y.oudjana@protonmail.com>
Date: Fri, 9 Dec 2022 17:37:40 +0300
Subject: [PATCH] media: dt-bindings: ak7375: Add supplies

commit 04a79f078329b14f260db15250e84c97022f42cd upstream

Add supply properties to describe regulators needed to power
the AK7375 VCM.

Signed-off-by: Yassine Oudjana <y.oudjana@protonmail.com>
Acked-by: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Tested-by: Umang Jain <umang.jain@ideasonboard.com>
---
 .../bindings/media/i2c/asahi-kasei,ak7375.yaml        | 11 +++++++++++
 1 file changed, 11 insertions(+)

--- a/Documentation/devicetree/bindings/media/i2c/asahi-kasei,ak7375.yaml
+++ b/Documentation/devicetree/bindings/media/i2c/asahi-kasei,ak7375.yaml
@@ -20,9 +20,17 @@ properties:
   reg:
     maxItems: 1
 
+  vdd-supply:
+    description: VDD supply
+
+  vio-supply:
+    description: I/O pull-up supply
+
 required:
   - compatible
   - reg
+  - vdd-supply
+  - vio-supply
 
 additionalProperties: false
 
@@ -35,6 +43,9 @@ examples:
         ak7375: camera-lens@c {
             compatible = "asahi-kasei,ak7375";
             reg = <0x0c>;
+
+            vdd-supply = <&vreg_l23a_2p8>;
+            vio-supply = <&vreg_lvs1a_1p8>;
         };
     };
 
