From 9d9586dc0c0deecb90675bd70862fe262f7376ab Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Wed, 14 Jun 2023 14:25:21 +0100
Subject: [PATCH] dtoverlays: Fix README text for i2c-fan

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 arch/arm/boot/dts/overlays/README | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -1800,10 +1800,10 @@ Params: addr                    Sets the
         i2c3                    Choose the I2C3 bus (configure with the i2c3
                                 overlay - BCM2711 only)
 
-        i2c4                    Choose the I2C3 bus (configure with the i2c3
+        i2c4                    Choose the I2C4 bus (configure with the i2c4
                                 overlay - BCM2711 only)
 
-        i2c5                    Choose the I2C5 bus (configure with the i2c4
+        i2c5                    Choose the I2C5 bus (configure with the i2c5
                                 overlay - BCM2711 only)
 
         i2c6                    Choose the I2C6 bus (configure with the i2c6
