From f3db55ae860a82e1224a909072783ef850e5d228 Mon Sep 17 00:00:00 2001
From: Luo Jie <quic_luoj@quicinc.com>
Date: Sun, 16 Jul 2023 16:49:20 +0800
Subject: [PATCH 2/6] net: phy: at803x: merge qca8081 slave seed function

merge the seed enablement and seed value configuration into
one function, since the random seed value is needed to be
configured when the seed is enabled.

Signed-off-by: Luo Jie <quic_luoj@quicinc.com>
Reviewed-by: Russell King (Oracle) <rmk+kernel@armlinux.org.uk>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/phy/at803x.c | 29 +++++++++--------------------
 1 file changed, 9 insertions(+), 20 deletions(-)

--- a/drivers/net/phy/at803x.c
+++ b/drivers/net/phy/at803x.c
@@ -1730,24 +1730,19 @@ static int qca808x_phy_fast_retrain_conf
 	return 0;
 }
 
-static int qca808x_phy_ms_random_seed_set(struct phy_device *phydev)
-{
-	u16 seed_value = prandom_u32_max(QCA808X_MASTER_SLAVE_SEED_RANGE);
-
-	return at803x_debug_reg_mask(phydev, QCA808X_PHY_DEBUG_LOCAL_SEED,
-			QCA808X_MASTER_SLAVE_SEED_CFG,
-			FIELD_PREP(QCA808X_MASTER_SLAVE_SEED_CFG, seed_value));
-}
-
 static int qca808x_phy_ms_seed_enable(struct phy_device *phydev, bool enable)
 {
-	u16 seed_enable = 0;
+	u16 seed_value;
 
-	if (enable)
-		seed_enable = QCA808X_MASTER_SLAVE_SEED_ENABLE;
+	if (!enable)
+		return at803x_debug_reg_mask(phydev, QCA808X_PHY_DEBUG_LOCAL_SEED,
+				QCA808X_MASTER_SLAVE_SEED_ENABLE, 0);
 
+	seed_value = prandom_u32_max(QCA808X_MASTER_SLAVE_SEED_RANGE);
 	return at803x_debug_reg_mask(phydev, QCA808X_PHY_DEBUG_LOCAL_SEED,
-			QCA808X_MASTER_SLAVE_SEED_ENABLE, seed_enable);
+			QCA808X_MASTER_SLAVE_SEED_CFG | QCA808X_MASTER_SLAVE_SEED_ENABLE,
+			FIELD_PREP(QCA808X_MASTER_SLAVE_SEED_CFG, seed_value) |
+			QCA808X_MASTER_SLAVE_SEED_ENABLE);
 }
 
 static int qca808x_config_init(struct phy_device *phydev)
@@ -1771,12 +1766,7 @@ static int qca808x_config_init(struct ph
 	if (ret)
 		return ret;
 
-	/* Configure lower ramdom seed to make phy linked as slave mode */
-	ret = qca808x_phy_ms_random_seed_set(phydev);
-	if (ret)
-		return ret;
-
-	/* Enable seed */
+	/* Enable seed and configure lower ramdom seed to make phy linked as slave mode */
 	ret = qca808x_phy_ms_seed_enable(phydev, true);
 	if (ret)
 		return ret;
@@ -1821,7 +1811,6 @@ static int qca808x_read_status(struct ph
 		if (phydev->master_slave_state == MASTER_SLAVE_STATE_ERR) {
 			qca808x_phy_ms_seed_enable(phydev, false);
 		} else {
-			qca808x_phy_ms_random_seed_set(phydev);
 			qca808x_phy_ms_seed_enable(phydev, true);
 		}
 	}
