From 4d44bb1031a68d7d5b604d3b340c059f41ca62af Mon Sep 17 00:00:00 2001
From: dissent1 <be.dissent@gmail.com>
Date: Mon, 6 May 2019 20:55:16 +0300
Subject: [PATCH] ipq40xx: fix sleep clock

It seems like sleep_clk was copied from ipq806x.
Fix ipq40xx sleep_clk to the value QSDK defines.

Also rename the sleep clock node like the GCC driver names it.

Signed-off-by: Pavel Kubelun <be.dissent@gmail.com>
---
 arch/arm/boot/dts/qcom-ipq4019.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/qcom-ipq4019.dtsi
+++ b/arch/arm/boot/dts/qcom-ipq4019.dtsi
@@ -140,9 +140,9 @@
 	};
 
 	clocks {
-		sleep_clk: sleep_clk {
+		sleep_clk: gcc_sleep_clk_src {
 			compatible = "fixed-clock";
-			clock-frequency = <32768>;
+			clock-frequency = <32000>;
 			#clock-cells = <0>;
 		};
 
